Component: ARM Compiler 5.06 update 6 (build 750) Tool: armlink [4d35ed]

==============================================================================

Section Cross References

    main.o(i.HAL_IncTick) refers to hal.o(.data) for gSysTick_Counter
    main.o(i.PeripheralInit) refers to sys.o(i.INTX_ENABLE) for INTX_ENABLE
    main.o(i.PeripheralInit) refers to hal.o(i.HAL_Init) for HAL_Init
    main.o(i.PeripheralInit) refers to sdram_hal.o(i.HAL_SDRAM_Init) for HAL_SDRAM_Init
    main.o(i.PeripheralInit) refers to cpm_hal.o(i.HAL_CPM_GETCLCK) for HAL_CPM_GETCLCK
    main.o(i.PeripheralInit) refers to debug.o(i.UART_Debug_Init) for UART_Debug_Init
    main.o(i.PeripheralInit) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    main.o(i.PeripheralInit) refers to bsp.o(i.LT_ReadParam) for LT_ReadParam
    main.o(i.PeripheralInit) refers to rtc.o(i.LT_RtcInit) for LT_RtcInit
    main.o(i.PeripheralInit) refers to main.o(i.Printf_Version) for Printf_Version
    main.o(i.PeripheralInit) refers to pwm.o(i.InitBacklight) for InitBacklight
    main.o(i.PeripheralInit) refers to pwm.o(i.InitBeep) for InitBeep
    main.o(i.PeripheralInit) refers to lcd.o(i.InitLcd) for InitLcd
    main.o(i.PeripheralInit) refers to bsp.o(i.Canvas_image_width) for Canvas_image_width
    main.o(i.PeripheralInit) refers to lt776_grac.o(i.ClearScreen) for ClearScreen
    main.o(i.PeripheralInit) refers to ft5216.o(i.CTP_Init) for CTP_Init
    main.o(i.PeripheralInit) refers to delay.o(i.DelayMS) for DelayMS
    main.o(i.PeripheralInit) refers to pwm.o(i.ConfigBacklight) for ConfigBacklight
    main.o(i.PeripheralInit) refers to cpm_drv.o(.data) for g_sdram_clk
    main.o(i.PeripheralInit) refers to cpm_drv.o(.data) for g_ips_clk
    main.o(i.Printf_Version) refers to printf8.o(i.__0printf$8) for __2printf
    main.o(i.Printf_Version) refers to main.o(.data) for .data
    main.o(i.Printf_Version) refers to cpm_drv.o(.data) for g_sys_clk
    main.o(i.Printf_Version) refers to cpm_drv.o(.data) for g_ips_clk
    main.o(i.main) refers to main.o(i.PeripheralInit) for PeripheralInit
    main.o(i.main) refers to main.o(i.x_application_define) for x_application_define
    main.o(i.main) refers to tasks.o(i.vTaskStartScheduler) for vTaskStartScheduler
    main.o(i.task_0_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_0_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_0_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_0_entry) refers to event_groups.o(i.xEventGroupSetBits) for xEventGroupSetBits
    main.o(i.task_0_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_0_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_0_entry) refers to main.o(.data) for .data
    main.o(i.task_0_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_1_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_1_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_1_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_1_entry) refers to queue.o(i.xQueueGenericSend) for xQueueGenericSend
    main.o(i.task_1_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_1_entry) refers to main.o(.constdata) for .constdata
    main.o(i.task_1_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_1_entry) refers to main.o(.data) for .data
    main.o(i.task_1_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_2_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_2_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_2_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_2_entry) refers to queue.o(i.xQueueReceive) for xQueueReceive
    main.o(i.task_2_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_2_entry) refers to main.o(.data) for .data
    main.o(i.task_2_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_3_and_4_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_3_and_4_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_3_and_4_entry) refers to queue.o(i.xQueueGenericSend) for xQueueGenericSend
    main.o(i.task_3_and_4_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_3_and_4_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_3_and_4_entry) refers to queue.o(i.xQueueSemaphoreTake) for xQueueSemaphoreTake
    main.o(i.task_3_and_4_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_3_and_4_entry) refers to main.o(.data) for .data
    main.o(i.task_3_and_4_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_5_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_5_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_5_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_5_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_5_entry) refers to event_groups.o(i.xEventGroupClearBits) for xEventGroupClearBits
    main.o(i.task_5_entry) refers to event_groups.o(i.xEventGroupWaitBits) for xEventGroupWaitBits
    main.o(i.task_5_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_5_entry) refers to main.o(.data) for .data
    main.o(i.task_5_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_6_and_7_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_6_and_7_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_6_and_7_entry) refers to queue.o(i.xQueueGenericSend) for xQueueGenericSend
    main.o(i.task_6_and_7_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_6_and_7_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_6_and_7_entry) refers to queue.o(i.xQueueSemaphoreTake) for xQueueSemaphoreTake
    main.o(i.task_6_and_7_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_6_and_7_entry) refers to main.o(.data) for .data
    main.o(i.task_6_and_7_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.task_touch_entry) refers to lt776_grac.o(i.Put16BitBMP) for Put16BitBMP
    main.o(i.task_touch_entry) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    main.o(i.task_touch_entry) refers to misc_c.o(i.Show16BitDecimal) for Show16BitDecimal
    main.o(i.task_touch_entry) refers to ft5216.o(i.FT5216_Scan) for FT5216_Scan
    main.o(i.task_touch_entry) refers to tasks.o(i.vTaskDelay) for vTaskDelay
    main.o(i.task_touch_entry) refers to acorn.o(.constdata) for BMP_Acorn
    main.o(i.task_touch_entry) refers to main.o(.data) for .data
    main.o(i.task_touch_entry) refers to data.o(.bss) for gTpInfo
    main.o(i.task_touch_entry) refers to acorn1.o(.constdata) for BMP_Acorn1
    main.o(i.vApplicationGetIdleTaskMemory) refers to main.o(.bss) for .bss
    main.o(i.x_application_define) refers to queue.o(i.xQueueGenericCreateStatic) for xQueueGenericCreateStatic
    main.o(i.x_application_define) refers to queue.o(i.xQueueCreateMutexStatic) for xQueueCreateMutexStatic
    main.o(i.x_application_define) refers to event_groups.o(i.xEventGroupCreateStatic) for xEventGroupCreateStatic
    main.o(i.x_application_define) refers to tasks.o(i.xTaskCreateStatic) for xTaskCreateStatic
    main.o(i.x_application_define) refers to main.o(.bss) for .bss
    main.o(i.x_application_define) refers to main.o(.data) for .data
    main.o(i.x_application_define) refers to main.o(i.task_0_entry) for task_0_entry
    main.o(i.x_application_define) refers to main.o(i.task_1_entry) for task_1_entry
    main.o(i.x_application_define) refers to main.o(i.task_2_entry) for task_2_entry
    main.o(i.x_application_define) refers to main.o(i.task_3_and_4_entry) for task_3_and_4_entry
    main.o(i.x_application_define) refers to main.o(i.task_5_entry) for task_5_entry
    main.o(i.x_application_define) refers to main.o(i.task_6_and_7_entry) for task_6_and_7_entry
    main.o(i.x_application_define) refers to main.o(i.task_touch_entry) for task_touch_entry
    main.o(.data) refers to main.o(.conststring) for .conststring
    bsp.o(i.Canvas_Image_Start_address) refers to bsp.o(.data) for .data
    bsp.o(i.Canvas_image_width) refers to bsp.o(.data) for .data
    bsp.o(i.DMAC_M2MTest2) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    bsp.o(i.DMAC_M2MTest2) refers to dma_hal.o(i.HAL_DMAC_StartPolling) for HAL_DMAC_StartPolling
    bsp.o(i.DMAC_M2MTest2) refers to dma_hal.o(i.HAL_DMAC_PollForTransfer) for HAL_DMAC_PollForTransfer
    bsp.o(i.DMAC_M2MTest2) refers to bsp.o(.bss) for .bss
    bsp.o(i.DMAC_M2MTest3) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    bsp.o(i.DMAC_M2MTest3) refers to dma_hal.o(i.HAL_DMAC_StartPolling) for HAL_DMAC_StartPolling
    bsp.o(i.DMAC_M2MTest3) refers to bsp.o(.bss) for .bss
    bsp.o(i.LT768_BTE_Init) refers to dma_hal.o(i.HAL_DMAC_Deinit) for HAL_DMAC_Deinit
    bsp.o(i.LT768_BTE_Init) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    bsp.o(i.LT768_BTE_Init) refers to bsp.o(.bss) for .bss
    bsp.o(i.LT768_BTE_Init) refers to bsp.o(.data) for .data
    bsp.o(i.LT768_DrawPoint) refers to bsp.o(.data) for .data
    bsp.o(i.LT768_TFT_ShowAscii) refers to bsp.o(i.LT768_TFT_Show_Internal_Char) for LT768_TFT_Show_Internal_Char
    bsp.o(i.LT768_TFT_ShowAscii) refers to bsp.o(.data) for .data
    bsp.o(i.LT768_TFT_Show_Internal_Char) refers to bsp.o(i.LT768_DrawPoint) for LT768_DrawPoint
    bsp.o(i.LT768_TFT_Show_Internal_Char) refers to font_data.o(.constdata) for asc2_3216
    bsp.o(i.LT768_TFT_Show_Internal_Char) refers to font_data.o(.constdata) for asc2_1608
    bsp.o(i.LT768_TFT_Show_Internal_Char) refers to font_data.o(.constdata) for asc2_2412
    bsp.o(i.LT768_TFT_Show_Internal_Char) refers to bsp.o(.data) for .data
    bsp.o(i.LT_ReadFlash) refers to winbond.o(i.W25NXX_Read_NoCheck) for W25NXX_Read_NoCheck
    bsp.o(i.LT_ReadFlash) refers to winbond.o(i.W25QXX_Read_QUAD) for W25QXX_Read_QUAD
    bsp.o(i.LT_ReadFlash) refers to bsp.o(.data) for .data
    bsp.o(i.LT_ReadParam) refers to memseta.o(.text) for __aeabi_memclr4
    bsp.o(i.LT_ReadParam) refers to bsp.o(.data) for .data
    can_drv.o(i.CanRecieved) refers to can_drv.o(.bss) for .bss
    can_drv.o(i.CanRecvByte) refers to can_drv.o(.bss) for .bss
    can_drv.o(i.DRV_CAN0_3_Handler) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN12_15_Handler) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN16_31_Handler) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN32_63_Handler) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN8_11_Handler) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN_DeInit) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN_FIFO_ReceiveBytesIT) refers to memcpya.o(.text) for __aeabi_memcpy4
    can_drv.o(i.DRV_CAN_FIFO_ReceiveBytesIT) refers to can_drv.o(.bss) for .bss
    can_drv.o(i.DRV_CAN_Init) refers to can_drv.o(i.DRV_CAN_FuncSwap) for DRV_CAN_FuncSwap
    can_drv.o(i.DRV_CAN_Init) refers to can_drv.o(i.DRV_CAN_SoftReset) for DRV_CAN_SoftReset
    can_drv.o(i.DRV_CAN_Init) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN_ReceiveBytesIT) refers to can_drv.o(.data) for .data
    can_drv.o(i.DRV_CAN_TransmitBytesIT) refers to can_drv.o(.data) for .data
    cpm_drv.o(i.DRV_CPM_GetEFMClHz) refers to cpm_drv.o(.data) for .data
    cpm_drv.o(i.DRV_CPM_GetIPSClHz) refers to cpm_drv.o(.data) for .data
    cpm_drv.o(i.DRV_CPM_GetSDRAMClHz) refers to cpm_drv.o(.data) for .data
    cpm_drv.o(i.DRV_CPM_GetSYSClHz) refers to cpm_drv.o(.data) for .data
    cpm_drv.o(i.DRV_CPM_PorReset) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet) for DRV_CPM_VccCoreTestModeKeySet
    cpm_drv.o(i.DRV_CPM_SystemClkVrefTrim) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet) for DRV_CPM_VccCoreTestModeKeySet
    cpm_drv.o(i.DRV_CPM_UsbPhyInit) refers to delay.o(i.DelayMS) for DelayMS
    cpm_drv.o(i.DRV_CPM_UsbPhyInit) refers to delay.o(i.delay) for delay
    cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet) for DRV_CPM_VccCoreTestModeKeySet
    dma_drv.o(i.DMA_REG_Init) refers to dma_drv.o(.data) for .data
    dma_drv.o(i.clear_dma_flag) refers to dma_drv.o(.data) for .data
    dma_drv.o(i.dma_ssi_m2p_start) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dma_drv.o(i.dma_ssi_m2p_start) refers to dma_drv.o(.data) for .data
    dma_drv.o(i.dma_ssi_p2m_lli_start) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dma_drv.o(i.dma_ssi_p2m_lli_start) refers to dma_drv.o(.bss) for .bss
    dma_drv.o(i.dma_ssi_p2m_lli_start) refers to dma_drv.o(.data) for .data
    dma_drv.o(i.dma_ssi_wait) refers to dma_drv.o(.data) for .data
    dma_drv.o(i.get_dma_flag) refers to dma_drv.o(.data) for .data
    dma2d_drv.o(i.DRV_DMA2D_BlendHard) refers to dma2d_drv.o(i.DRV_DMA2D_SetAlphaCmp) for DRV_DMA2D_SetAlphaCmp
    dma2d_drv.o(i.DRV_DMA2D_BlendHard) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dma2d_drv.o(i.DRV_DMA2D_Mem2Mem) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dma2d_drv.o(i.DRV_DMA2D_PfcHard) refers to dma2d_drv.o(i.DRV_DMA2D_SetAlphaCmp) for DRV_DMA2D_SetAlphaCmp
    dma2d_drv.o(i.DRV_DMA2D_PfcHard) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dma2d_drv.o(i.DRV_DMA2D_Reg2Mem) refers to sys.o(i.NVIC_Init) for NVIC_Init
    eflash_drv.o(i.DRV_EFLASH_SetWritePermission) refers to lib_eflash.o(i.LIB_EFLASH_SetWritePermission) for LIB_EFLASH_SetWritePermission
    eflash_drv.o(i.DRV_EFM_EreasePage) refers to lib_eflash.o(i.LIB_EFLASH_PageErase) for LIB_EFLASH_PageErase
    eflash_drv.o(i.DRV_EFM_Init) refers to lib_eflash.o(i.LIB_EFLASH_Init) for LIB_EFLASH_Init
    eflash_drv.o(i.DRV_EFM_ProgramBulk) refers to lib_eflash.o(i.LIB_EFLASH_BulkProgram) for LIB_EFLASH_BulkProgram
    eflash_drv.o(i.DRV_EFM_ProgramWord) refers to lib_eflash.o(i.LIB_EFLASH_BulkProgram) for LIB_EFLASH_BulkProgram
    eport_drv.o(i.DRV_EPORT_IRQHandler) refers to printf8.o(i.__0printf$8) for __2printf
    i2c_drv.o(i.DRV_I2C_MasterGenerateStop) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MasterGenerateStopV1) refers to delay.o(i.delay) for delay
    i2c_drv.o(i.DRV_I2C_MasterGenerateStopV1) refers to i2c_drv.o(i.DRV_I2C_GetFlag) for DRV_I2C_GetFlag
    i2c_drv.o(i.DRV_I2C_MasterGenerateStopV2) refers to delay.o(i.delay) for delay
    i2c_drv.o(i.DRV_I2C_MasterGenerateStopV2) refers to i2c_drv.o(i.DRV_I2C_GetFlag) for DRV_I2C_GetFlag
    i2c_drv.o(i.DRV_I2C_MasterHighspeedWriteRequest) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MasterReadRequest) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MasterReadRequest) refers to i2c_drv.o(i.DRV_I2C_GetFlag) for DRV_I2C_GetFlag
    i2c_drv.o(i.DRV_I2C_MasterRestartReadRequest) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MasterWriteRequest) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MasterWriteRequest) refers to i2c_drv.o(i.DRV_I2C_GetFlag) for DRV_I2C_GetFlag
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_MasterWriteRequest) for DRV_I2C_MasterWriteRequest
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_MasterHighspeedWriteRequest) for DRV_I2C_MasterHighspeedWriteRequest
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_TransmitByte) for DRV_I2C_TransmitByte
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_MasterGenerateStop) for DRV_I2C_MasterGenerateStop
    i2c_drv.o(i.DRV_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_MasterReadRequest) for DRV_I2C_MasterReadRequest
    i2c_drv.o(i.DRV_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_MasterWriteRequest) for DRV_I2C_MasterWriteRequest
    i2c_drv.o(i.DRV_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_MasterHighspeedWriteRequest) for DRV_I2C_MasterHighspeedWriteRequest
    i2c_drv.o(i.DRV_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_TransmitByte) for DRV_I2C_TransmitByte
    i2c_drv.o(i.DRV_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_MasterGenerateStop) for DRV_I2C_MasterGenerateStop
    i2c_drv.o(i.DRV_I2C_Receive) refers to i2c_drv.o(i.DRV_I2C_MasterReadRequest) for DRV_I2C_MasterReadRequest
    i2c_drv.o(i.DRV_I2C_Receive) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_Receive) refers to delay.o(i.delay) for delay
    i2c_drv.o(i.DRV_I2C_ReceiveByte) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_Transmit) refers to i2c_drv.o(i.DRV_I2C_MasterWriteRequest) for DRV_I2C_MasterWriteRequest
    i2c_drv.o(i.DRV_I2C_Transmit) refers to i2c_drv.o(i.DRV_I2C_MasterHighspeedWriteRequest) for DRV_I2C_MasterHighspeedWriteRequest
    i2c_drv.o(i.DRV_I2C_Transmit) refers to i2c_drv.o(i.DRV_I2C_TransmitByte) for DRV_I2C_TransmitByte
    i2c_drv.o(i.DRV_I2C_Transmit) refers to i2c_drv.o(i.DRV_I2C_MasterGenerateStop) for DRV_I2C_MasterGenerateStop
    i2c_drv.o(i.DRV_I2C_TransmitByte) refers to i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) for DRV_I2C_WaitonFlagTimeout
    i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) refers to delay.o(i.delay) for delay
    i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout) refers to i2c_drv.o(i.DRV_I2C_GetFlag) for DRV_I2C_GetFlag
    interrupt.o(i.Access_Error) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.Breakpoint_Exception) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.BusFault_Handler) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.CAN4_7_IRQHandler) refers to debug.o(i.DRV_CAN4_7_Handler) for DRV_CAN4_7_Handler
    interrupt.o(i.DummyHandler) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.HardFault_Handler) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.Illegal_Instrn) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.MemManage_Handler) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.Misaligned_Access) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.OperationalLogic_Error) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.PCI_IRQHandler) refers to cpm_hal.o(i.HAL_CPM_IRQHandler) for HAL_CPM_IRQHandler
    interrupt.o(i.PIT3_IRQHandler) refers to pit32_hal.o(i.HAL_PIT32_IRQHandler) for HAL_PIT32_IRQHandler
    interrupt.o(i.PIT4_IRQHandler) refers to pit32_hal.o(i.HAL_PIT32_IRQHandler) for HAL_PIT32_IRQHandler
    interrupt.o(i.SysTick_Handler3) refers to interrupt.o(.data) for .data
    interrupt.o(i.UART1_IRQHandler) refers to debug.o(i.UART1_IRQHandlerEvent) for UART1_IRQHandlerEvent
    interrupt.o(i.Unrecoverable_Error) refers to printf8.o(i.__0printf$8) for __2printf
    interrupt.o(i.UsageFault_Handler) refers to printf8.o(i.__0printf$8) for __2printf
    rtc_drv.o(i.DRV_RTC_IRQHandler) refers to printf8.o(i.__0printf$8) for __2printf
    sdio_drv.o(i.ACMD41_SD_tsk) refers to sdio_drv.o(i.CMD55_SD_tsk) for CMD55_SD_tsk
    sdio_drv.o(i.ACMD41_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.ACMD42_SD_tsk) refers to sdio_drv.o(i.CMD55_SD_tsk) for CMD55_SD_tsk
    sdio_drv.o(i.ACMD42_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.ACMD51_SD_tsk) refers to sdio_drv.o(i.CMD55_SD_tsk) for CMD55_SD_tsk
    sdio_drv.o(i.ACMD51_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.ACMD6_SD_tsk) refers to sdio_drv.o(i.CMD55_SD_tsk) for CMD55_SD_tsk
    sdio_drv.o(i.ACMD6_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD0_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD11_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD12_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD13_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD16_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD17_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD18_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD1_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD24_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD25_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD2_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD3_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD52_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD55_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD5_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD6_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD7_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD8_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.CMD9_SD_tsk) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdio_drv.o(i.SDIO_CardDetect) refers to sdio_drv.o(i.SDIO_PowerUp) for SDIO_PowerUp
    sdio_drv.o(i.SDIO_CardDetect) refers to delay.o(i.delay) for delay
    sdio_drv.o(i.SDIO_CardDetect) refers to sdio_drv.o(i.SDIO_Card_Volt) for SDIO_Card_Volt
    sdio_drv.o(i.SDIO_HCON) refers to sdio_drv.o(.data) for .data
    sdio_drv.o(i.SDIO_SetClk) refers to sdio_drv.o(i.SDIO_Start_CMD) for SDIO_Start_CMD
    sdio_drv.o(i.SDIO_SwitchClk) refers to sdio_drv.o(i.SDIO_Start_CMD) for SDIO_Start_CMD
    spi_drv.o(i.DRV_SPI_WaitonFlagTimeout) refers to spi_drv.o(i.DRV_SPI_GetFlag) for DRV_SPI_GetFlag
    ssi_drv.o(i.DRV_EFlash_Set_Read_Para) refers to ssi_drv.o(i.DRV_SSI_CS_DisInit) for DRV_SSI_CS_DisInit
    ssi_drv.o(i.DRV_EFlash_Set_Read_Para) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_EFlash_Set_Read_Para) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_EFlash_Set_Read_Para) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_DUAL_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    ssi_drv.o(i.DRV_SSI_DUAL_Init) refers to ssi_drv.o(i.DRV_SSI_StructInit) for DRV_SSI_StructInit
    ssi_drv.o(i.DRV_SSI_DUAL_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_DUAL_Read) refers to ssi_drv.o(i.DRV_SSI_DUAL_Init) for DRV_SSI_DUAL_Init
    ssi_drv.o(i.DRV_SSI_EFlash_DUAL_Read) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_DUAL_Read) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_GetFlag) for DRV_SSI_GetFlag
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2) refers to ssi_drv.o(i.DRV_SSI_GetFlag) for DRV_SSI_GetFlag
    ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status12) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status12) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) refers to ssi_drv.o(i.DRV_SSI_GetFlag) for DRV_SSI_GetFlag
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) for DRV_SSI_EFlash_QPI_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_WAIT_Status1) for DRV_SSI_EFlash_QPI_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Read) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Read) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) for DRV_SSI_EFlash_QPI_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_WAIT_Status1) for DRV_SSI_EFlash_QPI_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_WAIT_Status1) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) for DRV_SSI_EFlash_QPI_Get_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1) for DRV_SSI_EFlash_QPI_Get_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_QPI_Init) for DRV_SSI_QPI_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_QUAD_Init) for DRV_SSI_QUAD_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Read) refers to ssi_drv.o(i.DRV_SSI_QUAD_Init) for DRV_SSI_QUAD_Init
    ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Read) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Read) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Read) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Read) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Read) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) refers to ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) for DRV_SSI_EFlash_Get_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) for DRV_SSI_EFlash_Get_Status1
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1) for DRV_SSI_EFlash_WAIT_Status1
    ssi_drv.o(i.DRV_SSI_Init) refers to ssi_drv.o(i.DRV_SSI_CS_DisInit) for DRV_SSI_CS_DisInit
    ssi_drv.o(i.DRV_SSI_Init) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    ssi_drv.o(i.DRV_SSI_Init) refers to ssi_drv.o(i.DRV_SSI_CS_Init) for DRV_SSI_CS_Init
    ssi_drv.o(i.DRV_SSI_QPI_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    ssi_drv.o(i.DRV_SSI_QPI_Init) refers to ssi_drv.o(i.DRV_SSI_StructInit) for DRV_SSI_StructInit
    ssi_drv.o(i.DRV_SSI_QPI_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    ssi_drv.o(i.DRV_SSI_QUAD_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    ssi_drv.o(i.DRV_SSI_QUAD_Init) refers to ssi_drv.o(i.DRV_SSI_StructInit) for DRV_SSI_StructInit
    ssi_drv.o(i.DRV_SSI_QUAD_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    ssi_drv.o(i.DRV_SSI_STD_Init) refers to ssi_drv.o(i.DRV_SSI_StructInit) for DRV_SSI_StructInit
    ssi_drv.o(i.DRV_SSI_STD_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    ssi_drv.o(i.DRV_SSI_STD_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    ssi_drv.o(i.DRV_SSI_STD_Read_ID) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_STD_Read_ID) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_STD_Read_ID) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_STD_Reset) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_STD_Reset) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_STD_Reset) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_STD_Reset) refers to ssi_drv.o(i.DRV_SSI_clear_fifo) for DRV_SSI_clear_fifo
    ssi_drv.o(i.DRV_SSI_STD_Reset) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_STD_Reset_Enable) refers to ssi_drv.o(i.DRV_SSI_CS_LOW) for DRV_SSI_CS_LOW
    ssi_drv.o(i.DRV_SSI_STD_Reset_Enable) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_STD_Reset_Enable) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_STD_Reset_Enable) refers to ssi_drv.o(i.DRV_SSI_CS_HIGH) for DRV_SSI_CS_HIGH
    ssi_drv.o(i.DRV_SSI_WAIT_IDLE) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) refers to ssi_drv.o(i.DRV_SSI_GetFlag) for DRV_SSI_GetFlag
    ssi_drv.o(i.DRV_SSI_XIP_SET) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_SSI_clear_fifo) refers to ssi_drv.o(i.DRV_SSI_GetFlag) for DRV_SSI_GetFlag
    ssi_drv.o(i.DRV_XIP_EXIT) refers to ssi_drv.o(i.DRV_SSI_XIP_SET) for DRV_SSI_XIP_SET
    ssi_drv.o(i.DRV_XIP_EXIT) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) for DRV_SSI_EFlash_QPI_EXIT
    ssi_drv.o(i.DRV_XIP_EXIT) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1) for DRV_SSI_EFlash_Get_Status1
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2) for DRV_SSI_EFlash_Get_Status2
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_drv.o(i.DRV_XIP_Enter) refers to delay.o(i.delay) for delay
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2) for DRV_SSI_EFlash_Prog_Status2
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) for DRV_SSI_EFlash_QPI_Enter
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_EFlash_Set_Read_Para) for DRV_EFlash_Set_Read_Para
    ssi_drv.o(i.DRV_XIP_Enter) refers to ssi_drv.o(i.DRV_SSI_XIP_SET) for DRV_SSI_XIP_SET
    ssi_drv.o(i.SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.SSI_EFlash_Get_Status) for SSI_EFlash_Get_Status
    ssi_drv.o(i.SSI_QUAD_Burst_Init) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to ssi_drv.o(i.SSI_Standard_Init) for SSI_Standard_Init
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to ssi_drv.o(i.SSI_EFlash_Write_Enable) for SSI_EFlash_Write_Enable
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to dma_drv.o(i.DMA_REG_Init) for DMA_REG_Init
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to dma_drv.o(i.dma_ssi_m2p_start) for dma_ssi_m2p_start
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to ssi_drv.o(i.DRV_SSI_STD_DMA_Trig) for DRV_SSI_STD_DMA_Trig
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to dma_drv.o(i.dma_ssi_wait) for dma_ssi_wait
    ssi_drv.o(i.SSI_STD_DMA_Program) refers to ssi_drv.o(i.SSI_Wait_SPIFlash_Idle) for SSI_Wait_SPIFlash_Idle
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to ssi_drv.o(i.SSI_Standard_Init) for SSI_Standard_Init
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to dma_drv.o(i.DMA_REG_Init) for DMA_REG_Init
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to dma_drv.o(i.dma_ssi_p2m_lli_start) for dma_ssi_p2m_lli_start
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to ssi_drv.o(i.DRV_SSI_STD_DMA_Trig) for DRV_SSI_STD_DMA_Trig
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to dma_drv.o(i.get_dma_flag) for get_dma_flag
    ssi_drv.o(i.SSI_STD_DMA_Read) refers to dma_drv.o(i.clear_dma_flag) for clear_dma_flag
    ssi_drv.o(i.SSI_Wait_SPIFlash_Idle) refers to ssi_drv.o(i.SSI_Standard_Init) for SSI_Standard_Init
    ssi_drv.o(i.SSI_Wait_SPIFlash_Idle) refers to ssi_drv.o(i.SSI_EFlash_Get_Status) for SSI_EFlash_Get_Status
    uart_drv.o(i.DRV_UART_PutcDev) refers to uart_drv.o(i.DRV_UART_SendByte) for DRV_UART_SendByte
    uart_drv.o(i.DRV_UART_PutsDev) refers to uart_drv.o(i.DRV_UART_PutcDev) for DRV_UART_PutcDev
    uart_drv.o(i.DRV_UART_SendByteHex) refers to uart_drv.o(i.DRV_UART_SendOne) for DRV_UART_SendOne
    uart_drv.o(i.DRV_UART_SendBytes) refers to uart_drv.o(i.DRV_UART_SendByte) for DRV_UART_SendByte
    uart_drv.o(i.DRV_UART_SendOne) refers to uart_drv.o(i.DRV_UART_SendByte) for DRV_UART_SendByte
    uart_drv.o(i.DRV_UART_SendString) refers to uart_drv.o(i.DRV_UART_SendByte) for DRV_UART_SendByte
    uart_drv.o(i.DRV_UART_WaitonFlagTimeout) refers to uart_drv.o(i.DRV_UART_GetFlag) for DRV_UART_GetFlag
    uart_drv.o(i.UART_ISR) refers to uart_drv.o(.data) for .data
    uart_drv.o(i.UART_RecvByte) refers to uart_drv.o(.data) for .data
    uart_drv.o(i.UART_RecvByte) refers to uart_drv.o(.bss) for .bss
    cache_hal.o(i.HAL_CACHE_Close) refers to cache_drv.o(i.DRV_ICACHE_Init) for DRV_ICACHE_Init
    cache_hal.o(i.HAL_CACHE_Close) refers to cache_drv.o(i.DRV_DCACHE_Init) for DRV_DCACHE_Init
    cache_hal.o(i.HAL_CACHE_Init) refers to cache_drv.o(i.DRV_ICACHE_Init) for DRV_ICACHE_Init
    cache_hal.o(i.HAL_CACHE_Init) refers to cache_drv.o(i.DRV_DCACHE_Init) for DRV_DCACHE_Init
    cache_hal.o(i.HAL_CACHE_Syn) refers to cache_drv.o(i.DRV_ICACHE_Syn) for DRV_ICACHE_Syn
    cache_hal.o(i.HAL_CACHE_Syn) refers to cache_drv.o(i.DRV_DCACHE_Syn) for DRV_DCACHE_Syn
    can_hal.o(i.HAL_CAN_DeInit) refers to can_drv.o(i.DRV_CAN_DeInit) for DRV_CAN_DeInit
    can_hal.o(i.HAL_CAN_DeInit) refers to can_hal.o(i.NVIC_DisableIRQ) for NVIC_DisableIRQ
    can_hal.o(i.HAL_CAN_IRQHandler) refers to can_hal.o(.data) for .data
    can_hal.o(i.HAL_CAN_Init) refers to can_hal.o(i.HAL_CAN_MspInit) for HAL_CAN_MspInit
    can_hal.o(i.HAL_CAN_Init) refers to can_drv.o(i.DRV_CAN_Init) for DRV_CAN_Init
    can_hal.o(i.HAL_CAN_Init) refers to can_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    can_hal.o(i.HAL_CAN_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    can_hal.o(i.HAL_CAN_Init) refers to can_hal.o(.data) for .data
    can_hal.o(i.HAL_CAN_Receive) refers to can_drv.o(i.DRV_CAN_ReceiveBytes) for DRV_CAN_ReceiveBytes
    can_hal.o(i.HAL_CAN_Receive) refers to can_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    can_hal.o(i.HAL_CAN_Receive) refers to can_drv.o(i.DRV_CAN_FIFO_ReceiveBytes) for DRV_CAN_FIFO_ReceiveBytes
    can_hal.o(i.HAL_CAN_ReceiveIT) refers to can_drv.o(i.DRV_CAN_ReceiveBytesIT) for DRV_CAN_ReceiveBytesIT
    can_hal.o(i.HAL_CAN_ReceiveIT) refers to can_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    can_hal.o(i.HAL_CAN_ReceiveIT) refers to can_drv.o(i.DRV_CAN_FIFO_ReceiveBytesIT) for DRV_CAN_FIFO_ReceiveBytesIT
    can_hal.o(i.HAL_CAN_Transmit) refers to can_drv.o(i.DRV_CAN_TransmitBytes) for DRV_CAN_TransmitBytes
    can_hal.o(i.HAL_CAN_Transmit) refers to can_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    can_hal.o(i.HAL_CAN_TransmitIT) refers to can_drv.o(i.DRV_CAN_TransmitBytesIT) for DRV_CAN_TransmitBytesIT
    can_hal.o(i.HAL_CAN_TransmitIT) refers to can_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    clcd_hal.o(i.HAL_CLCD_CheckState) refers to delay.o(i.DelayMS) for DelayMS
    clcd_hal.o(i.HAL_CLCD_CheckState) refers to clcd_hal.o(.data) for .data
    clcd_hal.o(i.HAL_CLCD_DeInit) refers to clcd_drv.o(i.DRV_CLCD_Deinit) for DRV_CLCD_Deinit
    clcd_hal.o(i.HAL_CLCD_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetClkDiv) for DRV_CLCD_SetClkDiv
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetTiming0) for DRV_CLCD_SetTiming0
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetTiming1) for DRV_CLCD_SetTiming1
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetTiming2) for DRV_CLCD_SetTiming2
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetTiming3) for DRV_CLCD_SetTiming3
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_drv.o(i.DRV_CLCD_SetControlRegister) for DRV_CLCD_SetControlRegister
    clcd_hal.o(i.HAL_CLCD_Init) refers to clcd_hal.o(.data) for .data
    clcd_hal.o(i.HLA_CLCD_Cmd) refers to clcd_drv.o(i.DRV_CLCD_Cmd) for DRV_CLCD_Cmd
    cpm_hal.o(i.HAL_CPM_CardPowerOff) refers to delay.o(i.DelayMS) for DelayMS
    cpm_hal.o(i.HAL_CPM_CardPowerOn) refers to delay.o(i.DelayMS) for DelayMS
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(i.DRV_CPM_GetCOREClHz) for DRV_CPM_GetCOREClHz
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(i.DRV_CPM_GetSYSClHz) for DRV_CPM_GetSYSClHz
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(i.DRV_CPM_GetIPSClHz) for DRV_CPM_GetIPSClHz
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(i.DRV_CPM_GetSDRAMClHz) for DRV_CPM_GetSDRAMClHz
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_hal.o(.data) for .data
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(.data) for g_core_clk
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(.data) for g_ips_clk
    cpm_hal.o(i.HAL_CPM_GETCLCK) refers to cpm_drv.o(.data) for g_sdram_clk
    cpm_hal.o(i.HAL_CPM_GetClocksFreq) refers to cpm_drv.o(i.DRV_CPM_GetSYSClHz) for DRV_CPM_GetSYSClHz
    cpm_hal.o(i.HAL_CPM_GetClocksFreq) refers to cpm_drv.o(i.DRV_CPM_GetIPSClHz) for DRV_CPM_GetIPSClHz
    cpm_hal.o(i.HAL_CPM_GetClocksFreq) refers to cpm_drv.o(i.DRV_CPM_GetEFMClHz) for DRV_CPM_GetEFMClHz
    cpm_hal.o(i.HAL_CPM_IRQHandler) refers to printf8.o(i.__0printf$8) for __2printf
    cpm_hal.o(i.HAL_CPM_ModuleClkCmd) refers to cpm_drv.o(i.DRV_CPM_ModuleClkOn) for DRV_CPM_ModuleClkOn
    cpm_hal.o(i.HAL_CPM_ModuleClkCmd) refers to cpm_drv.o(i.DRV_CPM_ModuleClkOff) for DRV_CPM_ModuleClkOff
    cpm_hal.o(i.HAL_CPM_PorReset) refers to cpm_drv.o(i.DRV_CPM_PorReset) for DRV_CPM_PorReset
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to memcpya.o(.text) for __aeabi_memcpy
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC8MSelect) for DRV_CPM_SystemClkOSC8MSelect
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to libswithosc500mhz.o(i.HAL_CPM_SwitchOSC500MHz) for HAL_CPM_SwitchOSC500MHz
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC400MSelect) for DRV_CPM_SystemClkOSC400MSelect
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC480MSelect) for DRV_CPM_SystemClkOSC480MSelect
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSCEXTSelect) for DRV_CPM_SystemClkOSCEXTSelect
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetIpsClkDiv) for DRV_CPM_SetIpsClkDiv
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetCOREClHz) for DRV_CPM_GetCOREClHz
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetSYSClHz) for DRV_CPM_GetSYSClHz
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetIPSClHz) for DRV_CPM_GetIPSClHz
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetSdramClkDiv) for DRV_CPM_SetSdramClkDiv
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetSDRAMClHz) for DRV_CPM_GetSDRAMClHz
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_hal.o(.constdata) for .constdata
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_hal.o(.data) for .data
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(.data) for g_core_clk
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(.data) for g_ips_clk
    cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) refers to cpm_drv.o(.data) for g_sdram_clk
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC8MSelect) for DRV_CPM_SystemClkOSC8MSelect
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to libswithosc500mhz.o(i.HAL_CPM_SwitchOSC500MHz) for HAL_CPM_SwitchOSC500MHz
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC400MSelect) for DRV_CPM_SystemClkOSC400MSelect
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSC480MSelect) for DRV_CPM_SystemClkOSC480MSelect
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SystemClkOSCEXTSelect) for DRV_CPM_SystemClkOSCEXTSelect
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetIpsClkDiv) for DRV_CPM_SetIpsClkDiv
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetSystemClkDiv) for DRV_CPM_SetSystemClkDiv
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetCoreClkDiv) for DRV_CPM_SetCoreClkDiv
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetCOREClHz) for DRV_CPM_GetCOREClHz
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetSYSClHz) for DRV_CPM_GetSYSClHz
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetIPSClHz) for DRV_CPM_GetIPSClHz
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_SetSdramClkDiv) for DRV_CPM_SetSdramClkDiv
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(i.DRV_CPM_GetSDRAMClHz) for DRV_CPM_GetSDRAMClHz
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_hal.o(.data) for .data
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(.data) for g_core_clk
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(.data) for g_ips_clk
    cpm_hal.o(i.HAL_CPM_SYSCLKConfig) refers to cpm_drv.o(.data) for g_sdram_clk
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetClkoutClkDiv) for DRV_CPM_SetClkoutClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetTraceClkDiv) for DRV_CPM_SetTraceClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetSystemClkDiv) for DRV_CPM_SetSystemClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetCoreClkDiv) for DRV_CPM_SetCoreClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetArithClkDiv) for DRV_CPM_SetArithClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetAhb3ClkDiv) for DRV_CPM_SetAhb3ClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetIpsClkDiv) for DRV_CPM_SetIpsClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetTcClkDiv) for DRV_CPM_SetTcClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetMeshClkDiv) for DRV_CPM_SetMeshClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetAdcClkDiv) for DRV_CPM_SetAdcClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetMccAdrClkDiv) for DRV_CPM_SetMccAdrClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetMccClkDiv) for DRV_CPM_SetMccClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetSdram2lcdClkDiv) for DRV_CPM_SetSdram2lcdClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetSdram_smClkDiv) for DRV_CPM_SetSdram_smClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetSdramClkDiv) for DRV_CPM_SetSdramClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetClcdClkDiv) for DRV_CPM_SetClcdClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetSd_hostClkDiv) for DRV_CPM_SetSd_hostClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetDcmi_sensorClkDiv) for DRV_CPM_SetDcmi_sensorClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetDcmi_pixClkDiv) for DRV_CPM_SetDcmi_pixClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetMipi_sampleClkDiv) for DRV_CPM_SetMipi_sampleClkDiv
    cpm_hal.o(i.HAL_CPM_SetCLKDiv) refers to cpm_drv.o(i.DRV_CPM_SetDma2d_sramClkDiv) for DRV_CPM_SetDma2d_sramClkDiv
    cpm_hal.o(i.HAL_CPM_TrimCardVoltage) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet) for DRV_CPM_VccCoreTestModeKeySet
    cpm_hal.o(i.HAL_CPM_VCC5VByPass) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet) for DRV_CPM_VccCoreTestModeKeySet
    cpm_hal.o(i.HAL_CPM_WakeupInit) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dcmi_hal.o(i.HAL_DCMI_Callback) refers to printf8.o(i.__0printf$8) for __2printf
    dcmi_hal.o(i.HAL_DCMI_Getgray) refers to dcmi_drv.o(i.DRV_DCMI_Getgray) for DRV_DCMI_Getgray
    dcmi_hal.o(i.HAL_DCMI_IRQHandler) refers to dcmi_hal.o(.data) for .data
    dcmi_hal.o(i.HAL_DCMI_Init) refers to dcmi_drv.o(i.DRV_DCMI_Init) for DRV_DCMI_Init
    dcmi_hal.o(i.HAL_DCMI_Init) refers to dcmi_hal.o(.data) for .data
    dcmi_hal.o(i.HAL_DCMI_Init) refers to dcmi_hal.o(i.HAL_DCMI_Callback) for HAL_DCMI_Callback
    dma_hal.o(i.DMAC_SetConfig) refers to dma_drv.o(i.DRV_DMAC_LliRegInit) for DRV_DMAC_LliRegInit
    dma_hal.o(i.HAL_DMAC_Abort) refers to hal.o(i.HAL_GetTick) for HAL_GetTick
    dma_hal.o(i.HAL_DMAC_Abort) refers to dma_drv.o(i.DRV_DMAC_GetRawStatus) for DRV_DMAC_GetRawStatus
    dma_hal.o(i.HAL_DMAC_Abort) refers to dma_drv.o(i.DRV_DMAC_ClearRawStatus) for DRV_DMAC_ClearRawStatus
    dma_hal.o(i.HAL_DMAC_ClearRawStatus) refers to dma_drv.o(i.DRV_DMAC_ClearRawStatus) for DRV_DMAC_ClearRawStatus
    dma_hal.o(i.HAL_DMAC_ConfigLLi) refers to dma_drv.o(i.DRV_DMAC_LliRegInit) for DRV_DMAC_LliRegInit
    dma_hal.o(i.HAL_DMAC_IRQHandler) refers to dma_hal.o(.data) for .data
    dma_hal.o(i.HAL_DMAC_Init) refers to dma_drv.o(i.DRV_DMAC_CtrlRegConfig) for DRV_DMAC_CtrlRegConfig
    dma_hal.o(i.HAL_DMAC_Init) refers to dma_hal.o(i.DMAC_SetConfig) for DMAC_SetConfig
    dma_hal.o(i.HAL_DMAC_PollForTransfer) refers to dma_drv.o(i.DRV_DMAC_GetRawStatus) for DRV_DMAC_GetRawStatus
    dma_hal.o(i.HAL_DMAC_PollForTransfer) refers to hal.o(i.HAL_GetTick) for HAL_GetTick
    dma_hal.o(i.HAL_DMAC_PollForTransfer) refers to dma_drv.o(i.DRV_DMAC_ClearRawStatus) for DRV_DMAC_ClearRawStatus
    dma_hal.o(i.HAL_DMAC_PollForTransfer_IT) refers to hal.o(i.HAL_GetTick) for HAL_GetTick
    dma_hal.o(i.HAL_DMAC_PollForTransfer_IT) refers to dma_hal.o(.data) for .data
    dma_hal.o(i.HAL_DMAC_PollForTransfer_test) refers to dma_hal.o(.data) for .data
    dma_hal.o(i.HAL_DMAC_StartPolling) refers to dma_drv.o(i.DRV_DMAC_DisTfrIt) for DRV_DMAC_DisTfrIt
    dma_hal.o(i.HAL_DMAC_StartPolling_test) refers to dma_drv.o(i.DRV_DMAC_DisTfrIt) for DRV_DMAC_DisTfrIt
    dma2d_hal.o(i.HAL_DMA2D_BlendHard) refers to dma2d_drv.o(i.DRV_DMA2D_BlendHard) for DRV_DMA2D_BlendHard
    dma2d_hal.o(i.HAL_DMA2D_BlendHard) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_BlendHard) refers to dma2d_hal.o(i.HAL_DMA2D_Callback) for HAL_DMA2D_Callback
    dma2d_hal.o(i.HAL_DMA2D_Callback) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_ClutInit) refers to dma2d_drv.o(i.DRV_DMA2D_ClutInit) for DRV_DMA2D_ClutInit
    dma2d_hal.o(i.HAL_DMA2D_FgClutLoad) refers to dma2d_drv.o(i.DRV_DMA2D_FgClutLoad) for DRV_DMA2D_FgClutLoad
    dma2d_hal.o(i.HAL_DMA2D_IRQHandler) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_Mem2Mem) refers to dma2d_drv.o(i.DRV_DMA2D_Mem2Mem) for DRV_DMA2D_Mem2Mem
    dma2d_hal.o(i.HAL_DMA2D_Mem2Mem) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_Mem2Mem) refers to dma2d_hal.o(i.HAL_DMA2D_Callback) for HAL_DMA2D_Callback
    dma2d_hal.o(i.HAL_DMA2D_PfcHard) refers to dma2d_drv.o(i.DRV_DMA2D_PfcHard) for DRV_DMA2D_PfcHard
    dma2d_hal.o(i.HAL_DMA2D_PfcHard) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_PfcHard) refers to dma2d_hal.o(i.HAL_DMA2D_Callback) for HAL_DMA2D_Callback
    dma2d_hal.o(i.HAL_DMA2D_Reg2Mem) refers to dma2d_drv.o(i.DRV_DMA2D_Reg2Mem) for DRV_DMA2D_Reg2Mem
    dma2d_hal.o(i.HAL_DMA2D_Reg2Mem) refers to dma2d_hal.o(.data) for .data
    dma2d_hal.o(i.HAL_DMA2D_Reg2Mem) refers to dma2d_hal.o(i.HAL_DMA2D_Callback) for HAL_DMA2D_Callback
    dma2d_hal.o(i.HAL_DMA2D_SoftReset) refers to dma2d_drv.o(i.DRV_DMA2D_SoftReset) for DRV_DMA2D_SoftReset
    eflash_hal.o(i.HAL_EFLASH_Init) refers to eflash_drv.o(i.DRV_EFM_Init) for DRV_EFM_Init
    eflash_hal.o(i.HAL_EFLASH_Lock) refers to eflash_drv.o(i.DRV_EFM_MainCmd) for DRV_EFM_MainCmd
    eflash_hal.o(i.HAL_EFLASH_PageErase) refers to eflash_drv.o(i.DRV_EFM_EreasePage) for DRV_EFM_EreasePage
    eflash_hal.o(i.HAL_EFLASH_ProgramBulk) refers to eflash_drv.o(i.DRV_EFM_ProgramBulk) for DRV_EFM_ProgramBulk
    eflash_hal.o(i.HAL_EFLASH_ProgramWord) refers to eflash_drv.o(i.DRV_EFM_ProgramWord) for DRV_EFM_ProgramWord
    eflash_hal.o(i.HAL_EFLASH_Read) refers to eflash_drv.o(i.DRV_EFM_Read) for DRV_EFM_Read
    eflash_hal.o(i.HAL_EFLASH_SetWritePermission) refers to eflash_drv.o(i.DRV_EFLASH_SetWritePermission) for DRV_EFLASH_SetWritePermission
    eflash_hal.o(i.HAL_EFLASH_Unlock) refers to eflash_drv.o(i.DRV_EFM_MainCmd) for DRV_EFM_MainCmd
    eflash_hal.o(i.HAL_EFLASH_Write) refers to memcpya.o(.text) for __aeabi_memcpy
    eflash_hal.o(i.HAL_EFLASH_Write) refers to eflash_drv.o(i.DRV_EFM_EreasePage) for DRV_EFM_EreasePage
    eflash_hal.o(i.HAL_EFLASH_Write) refers to eflash_drv.o(i.DRV_EFM_ProgramBulk) for DRV_EFM_ProgramBulk
    eflash_hal.o(i.HAL_EFLASH_Write) refers to eflash_hal.o(.bss) for .bss
    eport_hal.o(i.HAL_EPORT0_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT0_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT10_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT11_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT12_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT13_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT14_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT15_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT1_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT2_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT3_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT4_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT5_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT6_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT7_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT8_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_0_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_1_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_2_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_3_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_4_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_5_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_6_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT9_7_IRQHandler) refers to eport_drv.o(i.DRV_EPORT_IRQHandler) for DRV_EPORT_IRQHandler
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapintEn) for DRV_IOCTRL_SwapintEn
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapDis) for DRV_IOCTRL_SwapDis
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_Swap2En) for DRV_IOCTRL_Swap2En
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_Swap3En) for DRV_IOCTRL_Swap3En
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_Swap4En) for DRV_IOCTRL_Swap4En
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_SPIMSwapEn) for DRV_IOCTRL_SPIMSwapEn
    eport_hal.o(i.HAL_EPORT_GintSwitch) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2SWAPEn) for DRV_IOCTRL_SetUSI2SWAPEn
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_hal.o(i.HAL_EPORT_GintSwitch) for HAL_EPORT_GintSwitch
    eport_hal.o(i.HAL_EPORT_Init) refers to ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) for HAL_IOCTRL_GINTIint
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_drv.o(i.DRV_EPORT_SetDirection) for DRV_EPORT_SetDirection
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_drv.o(i.DRV_EPORT_SetPullUp) for DRV_EPORT_SetPullUp
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_drv.o(i.DRV_EPORT_SetOpenDrain) for DRV_EPORT_SetOpenDrain
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_drv.o(i.DRV_EPORT_SetTriggerMode) for DRV_EPORT_SetTriggerMode
    eport_hal.o(i.HAL_EPORT_Init) refers to eport_drv.o(i.DRV_EPORT_SetIT) for DRV_EPORT_SetIT
    eport_hal.o(i.HAL_EPORT_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    eport_hal.o(i.HAL_EPORT_WritePinsLevel) refers to eport_drv.o(i.DRV_EPORT_WritePinsLevel) for DRV_EPORT_WritePinsLevel
    hal.o(i.HAL_DisBoot) refers to lib_eflash.o(i.LIB_EFlash_Chip_Mode) for LIB_EFlash_Chip_Mode
    hal.o(i.HAL_GetSN) refers to lib_eflash.o(i.LIB_GetSerialNumber) for LIB_GetSerialNumber
    hal.o(i.HAL_IncTick1) refers to misc_c.o(i.Show32BitValue) for Show32BitValue
    hal.o(i.HAL_IncTick1) refers to hal.o(.data) for .data
    hal.o(i.HAL_Init) refers to cache_hal.o(i.HAL_CACHE_Close) for HAL_CACHE_Close
    hal.o(i.HAL_Init) refers to cpm_hal.o(i.HAL_CPM_SYSCLKConfig) for HAL_CPM_SYSCLKConfig
    hal.o(i.HAL_Init) refers to cache_hal.o(i.HAL_CACHE_Init) for HAL_CACHE_Init
    hal.o(i.HAL_Init) refers to eflash_hal.o(i.HAL_EFLASH_Init) for HAL_EFLASH_Init
    hal.o(i.HAL_Init) refers to cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) for HAL_CPM_SSI_SYSCLKConfig
    hal.o(i.HAL_Init) refers to startup_armcm4.o(RESET) for __Vectors
    hal.o(i.HAL_Init) refers to cpm_drv.o(.data) for g_sys_clk
    hal.o(i.HAL_PrintfVersion) refers to printf8.o(i.__0printf$8) for __2printf
    hal.o(i.HAL_PrintfVersion) refers to rtc_hal.o(i.HAL_RTC_GetTime) for HAL_RTC_GetTime
    hal.o(i.HAL_PrintfVersion) refers to cpm_drv.o(.data) for g_core_clk
    hal.o(i.HAL_PrintfVersion) refers to cpm_drv.o(.data) for g_ips_clk
    hal.o(i.HAL_PrintfVersion) refers to cpm_drv.o(.data) for g_sdram_clk
    hal.o(i.HAL_RebackBoot) refers to eflash_hal.o(i.HAL_EFLASH_SetWritePermission) for HAL_EFLASH_SetWritePermission
    hal.o(i.HAL_RebackBoot) refers to lib_eflash.o(i.LIB_EFLASH_RecoveryToBoot) for LIB_EFLASH_RecoveryToBoot
    hal.o(i.SysClk_SoftRstReconfig) refers to cpm_hal.o(i.HAL_CPM_SYSCLKConfig) for HAL_CPM_SYSCLKConfig
    hal.o(i.SysClk_SoftRstReconfig) refers to cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig) for HAL_CPM_SSI_SYSCLKConfig
    hal.o(i.SysClk_SoftRstReconfig) refers to startup_armcm4.o(RESET) for __Vectors
    i2c_hal.o(i.HAL_I2C_DeInit) refers to i2c_drv.o(i.DRV_I2C_DeInit) for DRV_I2C_DeInit
    i2c_hal.o(i.HAL_I2C_GPIODeInit) refers to i2c_drv.o(i.DRV_I2C_GpioDeInit) for DRV_I2C_GpioDeInit
    i2c_hal.o(i.HAL_I2C_GPIOInit) refers to i2c_drv.o(i.DRV_I2C_GpioInit) for DRV_I2C_GpioInit
    i2c_hal.o(i.HAL_I2C_GPIOReadPin) refers to i2c_drv.o(i.DRV_I2C_ReadPin) for DRV_I2C_ReadPin
    i2c_hal.o(i.HAL_I2C_GPIOTogglePin) refers to i2c_drv.o(i.DRV_I2C_TogglePin) for DRV_I2C_TogglePin
    i2c_hal.o(i.HAL_I2C_GPIOWritePin) refers to i2c_drv.o(i.DRV_I2C_WritePin) for DRV_I2C_WritePin
    i2c_hal.o(i.HAL_I2C_IRQ) refers to i2c_drv.o(i.DRV_I2C_GetItFlags) for DRV_I2C_GetItFlags
    i2c_hal.o(i.HAL_I2C_IRQ) refers to i2c_drv.o(i.DRV_I2C_GetItSource) for DRV_I2C_GetItSource
    i2c_hal.o(i.HAL_I2C_Init) refers to i2c_hal.o(i.HAL_I2C_MspInit) for HAL_I2C_MspInit
    i2c_hal.o(i.HAL_I2C_Init) refers to i2c_drv.o(i.DRV_I2C_Init) for DRV_I2C_Init
    i2c_hal.o(i.HAL_I2C_MasterIRQHandler) refers to i2c_drv.o(i.DRV_I2C_GetDR) for DRV_I2C_GetDR
    i2c_hal.o(i.HAL_I2C_MasterIRQHandler) refers to i2c_drv.o(i.DRV_I2C_MasterGenerateStop) for DRV_I2C_MasterGenerateStop
    i2c_hal.o(i.HAL_I2C_MasterIRQHandler) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler) refers to i2c_drv.o(i.DRV_I2C_GetDR) for DRV_I2C_GetDR
    i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler) refers to i2c_drv.o(i.DRV_I2C_MasterGenerateStop) for DRV_I2C_MasterGenerateStop
    i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MasterRecceive) refers to i2c_drv.o(i.DRV_I2C_Receive) for DRV_I2C_Receive
    i2c_hal.o(i.HAL_I2C_MasterRecceive) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_MasterReceiveIT) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MasterReceiveIT) refers to i2c_hal.o(i.HAL_I2C_MasterIRQHandler) for HAL_I2C_MasterIRQHandler
    i2c_hal.o(i.HAL_I2C_MasterTransmit) refers to i2c_drv.o(i.DRV_I2C_Transmit) for DRV_I2C_Transmit
    i2c_hal.o(i.HAL_I2C_MasterTransmit) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_MasterTransmitIT) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MasterTransmitIT) refers to i2c_hal.o(i.HAL_I2C_MasterIRQHandler) for HAL_I2C_MasterIRQHandler
    i2c_hal.o(i.HAL_I2C_MemRead) refers to i2c_drv.o(i.DRV_I2C_MemRead) for DRV_I2C_MemRead
    i2c_hal.o(i.HAL_I2C_MemRead) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_MemReadIT) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MemReadIT) refers to i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler) for HAL_I2C_MasterMemIRQHandler
    i2c_hal.o(i.HAL_I2C_MemWrite) refers to i2c_drv.o(i.DRV_I2C_MemWrite) for DRV_I2C_MemWrite
    i2c_hal.o(i.HAL_I2C_MemWrite) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_MemWriteIT) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_MemWriteIT) refers to i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler) for HAL_I2C_MasterMemIRQHandler
    i2c_hal.o(i.HAL_I2C_SlaveIRQHandler) refers to i2c_drv.o(i.DRV_I2C_GetDR) for DRV_I2C_GetDR
    i2c_hal.o(i.HAL_I2C_SlaveIRQHandler) refers to i2c_drv.o(i.DRV_I2C_SetDR) for DRV_I2C_SetDR
    i2c_hal.o(i.HAL_I2C_SlaveReceive) refers to i2c_drv.o(i.DRV_I2C_SlaveReceive) for DRV_I2C_SlaveReceive
    i2c_hal.o(i.HAL_I2C_SlaveReceive) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_SlaveReceiveIT) refers to i2c_hal.o(i.HAL_I2C_SlaveIRQHandler) for HAL_I2C_SlaveIRQHandler
    i2c_hal.o(i.HAL_I2C_SlaveTransmit) refers to i2c_drv.o(i.DRV_I2C_SlaveTransmit) for DRV_I2C_SlaveTransmit
    i2c_hal.o(i.HAL_I2C_SlaveTransmit) refers to i2c_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    i2c_hal.o(i.HAL_I2C_SlaveTransmitIT) refers to i2c_hal.o(i.HAL_I2C_SlaveIRQHandler) for HAL_I2C_SlaveIRQHandler
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLDS) for DRV_IOCTRL_SetGINTLDS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLSR) for DRV_IOCTRL_SetGINTLSR
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLIS) for DRV_IOCTRL_SetGINTLIS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLPS) for DRV_IOCTRL_SetGINTLPS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLIE) for DRV_IOCTRL_SetGINTLIE
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHDS) for DRV_IOCTRL_SetGINTHDS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHSR) for DRV_IOCTRL_SetGINTHSR
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHIS) for DRV_IOCTRL_SetGINTHIS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHPS) for DRV_IOCTRL_SetGINTHPS
    ioctrl_hal.o(i.HAL_IOCTRL_GINTIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHIE) for DRV_IOCTRL_SetGINTHIE
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2CDS) for DRV_IOCTRL_SetI2CDS
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2CSR) for DRV_IOCTRL_SetI2CSR
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2CIS) for DRV_IOCTRL_SetI2CIS
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C1PS) for DRV_IOCTRL_SetI2C1PS
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C1IE) for DRV_IOCTRL_SetI2C1IE
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C2PS) for DRV_IOCTRL_SetI2C2PS
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C2IE) for DRV_IOCTRL_SetI2C2IE
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C3PS) for DRV_IOCTRL_SetI2C3PS
    ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetI2C3IE) for DRV_IOCTRL_SetI2C3IE
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPIDS) for DRV_IOCTRL_SetSPIDS
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPISR) for DRV_IOCTRL_SetSPISR
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPIIS) for DRV_IOCTRL_SetSPIIS
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI1PS) for DRV_IOCTRL_SetSPI1PS
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI1IE) for DRV_IOCTRL_SetSPI1IE
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI2PS) for DRV_IOCTRL_SetSPI2PS
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI2IE) for DRV_IOCTRL_SetSPI2IE
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI3PS) for DRV_IOCTRL_SetSPI3PS
    ioctrl_hal.o(i.HAL_IOCTRL_SPIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSPI3IE) for DRV_IOCTRL_SetSPI3IE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1DS) for DRV_IOCTRL_SetSSI1DS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1SR) for DRV_IOCTRL_SetSSI1SR
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1IS) for DRV_IOCTRL_SetSSI1IS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1PUE) for DRV_IOCTRL_SetSSI1PUE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1ODE) for DRV_IOCTRL_SetSSI1ODE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1PS) for DRV_IOCTRL_SetSSI1PS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1IE) for DRV_IOCTRL_SetSSI1IE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2DS) for DRV_IOCTRL_SetSSI2DS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2SR) for DRV_IOCTRL_SetSSI2SR
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2IS) for DRV_IOCTRL_SetSSI2IS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2PUE) for DRV_IOCTRL_SetSSI2PUE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2ODE) for DRV_IOCTRL_SetSSI2ODE
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2PS) for DRV_IOCTRL_SetSSI2PS
    ioctrl_hal.o(i.HAL_IOCTRL_SSIIint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2IE) for DRV_IOCTRL_SetSSI2IE
    ioctrl_hal.o(i.HAL_IOCTRL_Swap) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapDis) for DRV_IOCTRL_SwapDis
    ioctrl_hal.o(i.HAL_IOCTRL_Swap) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapEn) for DRV_IOCTRL_SwapEn
    ioctrl_hal.o(i.HAL_IOCTRL_Swapint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapintDisable) for DRV_IOCTRL_SwapintDisable
    ioctrl_hal.o(i.HAL_IOCTRL_Swapint) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapintEn) for DRV_IOCTRL_SwapintEn
    ioctrl_hal.o(i.HAL_IOCTRL_SwapintDIS) refers to ioctrl_drv.o(i.DRV_IOCTRL_SwapintDisable) for DRV_IOCTRL_SwapintDisable
    ioctrl_hal.o(i.HAL_IOCTRL_UARTInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUARTDS) for DRV_IOCTRL_SetUARTDS
    ioctrl_hal.o(i.HAL_IOCTRL_UARTInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUARTSR) for DRV_IOCTRL_SetUARTSR
    ioctrl_hal.o(i.HAL_IOCTRL_UARTInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUARTIS) for DRV_IOCTRL_SetUARTIS
    ioctrl_hal.o(i.HAL_IOCTRL_UARTInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUART1PS) for DRV_IOCTRL_SetUART1PS
    ioctrl_hal.o(i.HAL_IOCTRL_UARTInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUART2PS) for DRV_IOCTRL_SetUART2PS
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSIDS) for DRV_IOCTRL_SetUSIDS
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSISR) for DRV_IOCTRL_SetUSISR
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSIIS) for DRV_IOCTRL_SetUSIIS
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI1PS) for DRV_IOCTRL_SetUSI1PS
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2DIEN) for DRV_IOCTRL_SetUSI2DIEN
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2DREN) for DRV_IOCTRL_SetUSI2DREN
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3PUEN) for DRV_IOCTRL_SetUSI3PUEN
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3DIEN) for DRV_IOCTRL_SetUSI3DIEN
    ioctrl_hal.o(i.HAL_IOCTRL_USIInit) refers to ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3DREN) for DRV_IOCTRL_SetUSI3DREN
    lowpower_hal.o(i.LOWPOWER_DeepSleep) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet) for DRV_CPM_VccCoreTestModeSet
    lowpower_hal.o(i.LOWPOWER_DeepSleep) refers to sys.o(i.NVIC_Init) for NVIC_Init
    lowpower_hal.o(i.LOWPOWER_DeepSleep) refers to sys.o(i.Sys_Standby) for Sys_Standby
    lowpower_hal.o(i.LOWPOWER_Hiber) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet) for DRV_CPM_VccCoreTestModeSet
    lowpower_hal.o(i.LOWPOWER_Hiber) refers to sys.o(i.NVIC_Init) for NVIC_Init
    lowpower_hal.o(i.LOWPOWER_Hiber) refers to sys.o(i.Sys_Standby) for Sys_Standby
    lowpower_hal.o(i.LOWPOWER_Lowpower) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet) for DRV_CPM_VccCoreTestModeSet
    lowpower_hal.o(i.LOWPOWER_Lowpower) refers to sys.o(i.NVIC_Init) for NVIC_Init
    lowpower_hal.o(i.LOWPOWER_Lowpower) refers to sys.o(i.Sys_Standby) for Sys_Standby
    lowpower_hal.o(i.LOWPOWER_Retention) refers to cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet) for DRV_CPM_VccCoreTestModeSet
    lowpower_hal.o(i.LOWPOWER_Retention) refers to sys.o(i.NVIC_Init) for NVIC_Init
    lowpower_hal.o(i.LOWPOWER_Retention) refers to sys.o(i.Sys_Standby) for Sys_Standby
    pit32_hal.o(i.HAL_PIT32_CMD) refers to pit32_drv.o(i.DRV_PIT32_Cmd) for DRV_PIT32_Cmd
    pit32_hal.o(i.HAL_PIT32_GetCounter) refers to pit32_drv.o(i.DRV_PIT32_GetCounter) for DRV_PIT32_GetCounter
    pit32_hal.o(i.HAL_PIT32_IRQHandler) refers to pit32_hal.o(.data) for .data
    pit32_hal.o(i.HAL_PIT32_ITConfig) refers to pit32_drv.o(i.DRV_PIT32_InterruptCmd) for DRV_PIT32_InterruptCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_Cmd) for DRV_PIT32_Cmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_SetPrescaler) for DRV_PIT32_SetPrescaler
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_ReloadCmd) for DRV_PIT32_ReloadCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_ImmediatelyUpdateCNTCmd) for DRV_PIT32_ImmediatelyUpdateCNTCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_DozeCmd) for DRV_PIT32_DozeCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_DebugCmd) for DRV_PIT32_DebugCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_SetCounter) for DRV_PIT32_SetCounter
    pit32_hal.o(i.HAL_PIT32_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_drv.o(i.DRV_PIT32_InterruptCmd) for DRV_PIT32_InterruptCmd
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_hal.o(i.HAL_PIT32_Callback) for HAL_PIT32_Callback
    pit32_hal.o(i.HAL_PIT32_Init) refers to pit32_hal.o(.data) for .data
    pit32_hal.o(i.HAL_PIT32_SetCounter) refers to pit32_drv.o(i.DRV_PIT32_SetCounter) for DRV_PIT32_SetCounter
    pit32_hal.o(i.HAL_PIT32_SetPrescaler) refers to pit32_drv.o(i.DRV_PIT32_SetPrescaler) for DRV_PIT32_SetPrescaler
    pit32_hal.o(i.HAL_PIT32_Start) refers to pit32_drv.o(i.DRV_PIT32_Cmd) for DRV_PIT32_Cmd
    pit32_hal.o(i.HAL_PIT32_Stop) refers to pit32_drv.o(i.DRV_PIT32_Cmd) for DRV_PIT32_Cmd
    psram_hal.o(i.HAL_PSRAM_Init) refers to ssi_drv.o(i.DRV_PsramInit) for DRV_PsramInit
    psram_hal.o(i.HAL_PSRAM_Init) refers to psram_hal.o(.data) for .data
    psram_hal.o(i.HAL_PSRAM_Read) refers to psram_hal.o(i.get_psram_baseaddress) for get_psram_baseaddress
    psram_hal.o(i.HAL_PSRAM_Write) refers to psram_hal.o(i.get_psram_baseaddress) for get_psram_baseaddress
    psram_hal.o(i.get_psram_baseaddress) refers to psram_hal.o(.data) for .data
    pwm_hal.o(i.HAL_PWM_CHxAutoLoadMode) refers to pwm_drv.o(i.DRV_PWM_CHxAutoLoadMode) for DRV_PWM_CHxAutoLoadMode
    pwm_hal.o(i.HAL_PWM_CHxCaptureCmd) refers to pwm_drv.o(i.DRV_PWM_CHxCaptureCmd) for DRV_PWM_CHxCaptureCmd
    pwm_hal.o(i.HAL_PWM_CHxCmd) refers to pwm_drv.o(i.DRV_PWM_CHxCmd) for DRV_PWM_CHxCmd
    pwm_hal.o(i.HAL_PWM_CHxDeadZoneCmd) refers to pwm_drv.o(i.DRV_PWM_CHxDeadZoneCmd) for DRV_PWM_CHxDeadZoneCmd
    pwm_hal.o(i.HAL_PWM_CHxFallinginterruptCmd) refers to pwm_drv.o(i.DRV_PWM_CHxFallinginterruptCmd) for DRV_PWM_CHxFallinginterruptCmd
    pwm_hal.o(i.HAL_PWM_CHxInverteCmd) refers to pwm_drv.o(i.DRV_PWM_CHxInverteCmd) for DRV_PWM_CHxInverteCmd
    pwm_hal.o(i.HAL_PWM_CHxPullupCmd) refers to pwm_drv.o(i.DRV_PWM_CHxPullupCmd) for DRV_PWM_CHxPullupCmd
    pwm_hal.o(i.HAL_PWM_CHxRisingInterruptCmd) refers to pwm_drv.o(i.DRV_PWM_CHxRisingInterruptCmd) for DRV_PWM_CHxRisingInterruptCmd
    pwm_hal.o(i.HAL_PWM_CHxTimerInverteCmd) refers to pwm_drv.o(i.DRV_PWM_CHxTimerInverteCmd) for DRV_PWM_CHxTimerInverteCmd
    pwm_hal.o(i.HAL_PWM_ConfigCHxClkDiv) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxClkDiv) for DRV_PWM_ConfigCHxClkDiv
    pwm_hal.o(i.HAL_PWM_ConfigCHxDeadZone) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxDeadZone) for DRV_PWM_ConfigCHxDeadZone
    pwm_hal.o(i.HAL_PWM_ConfigCHxEdgeinterrupt) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxEdgeinterrupt) for DRV_PWM_ConfigCHxEdgeinterrupt
    pwm_hal.o(i.HAL_PWM_ConfigCHxPeriod) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPeriod) for DRV_PWM_ConfigCHxPeriod
    pwm_hal.o(i.HAL_PWM_ConfigCHxPerscaler) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPerscaler) for DRV_PWM_ConfigCHxPerscaler
    pwm_hal.o(i.HAL_PWM_ConfigCHxWidth) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxWidth) for DRV_PWM_ConfigCHxWidth
    pwm_hal.o(i.HAL_PWM_GetCHxLevel) refers to pwm_drv.o(i.DRV_PWM_GetCHxLevel) for DRV_PWM_GetCHxLevel
    pwm_hal.o(i.HAL_PWM_GetCHxPeriod) refers to pwm_drv.o(i.DRV_PWM_GetCHxPeriod) for DRV_PWM_GetCHxPeriod
    pwm_hal.o(i.HAL_PWM_GetCHxTimerCounter) refers to pwm_drv.o(i.DRV_PWM_GetCHxTimerCounter) for DRV_PWM_GetCHxTimerCounter
    pwm_hal.o(i.HAL_PWM_GetCHxWidth) refers to pwm_drv.o(i.DRV_PWM_GetCHxWidth) for DRV_PWM_GetCHxWidth
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to printf8.o(i.__0printf$8) for __2printf
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_GetCaptureInterruptFlag) for HAL_PWM_GetCaptureInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_ClrCaptureInterruptFlag) for HAL_PWM_ClrCaptureInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_GetRisingInterruptFlag) for HAL_PWM_GetRisingInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_ClrRisingInterruptFlag) for HAL_PWM_ClrRisingInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_GetFallingInterruptFlag) for HAL_PWM_GetFallingInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(i.HAL_PWM_ClrFallingInterruptFlag) for HAL_PWM_ClrFallingInterruptFlag
    pwm_hal.o(i.HAL_PWM_IRQHandler) refers to pwm_hal.o(.data) for .data
    pwm_hal.o(i.HAL_PWM_Init) refers to ioctrl_hal.o(i.HAL_IOCTRL_Swap) for HAL_IOCTRL_Swap
    pwm_hal.o(i.HAL_PWM_Init) refers to pwm_hal.o(i.HAL_PWM_OutputInit) for HAL_PWM_OutputInit
    pwm_hal.o(i.HAL_PWM_Init) refers to pwm_hal.o(i.HAL_PWM_InputInit) for HAL_PWM_InputInit
    pwm_hal.o(i.HAL_PWM_Init) refers to pwm_hal.o(.data) for .data
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_CHxCmd) for DRV_PWM_CHxCmd
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxDeadZone) for DRV_PWM_ConfigCHxDeadZone
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_CHxDeadZoneCmd) for DRV_PWM_CHxDeadZoneCmd
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPerscaler) for DRV_PWM_ConfigCHxPerscaler
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxClkDiv) for DRV_PWM_ConfigCHxClkDiv
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_CHxAutoLoadMode) for DRV_PWM_CHxAutoLoadMode
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPeriod) for DRV_PWM_ConfigCHxPeriod
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_SetCHxDirection) for DRV_PWM_SetCHxDirection
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_CHxInverteCmd) for DRV_PWM_CHxInverteCmd
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxEdgeinterrupt) for DRV_PWM_ConfigCHxEdgeinterrupt
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_hal.o(i.HAL_PWM_ConfigCallbackRegistry) for HAL_PWM_ConfigCallbackRegistry
    pwm_hal.o(i.HAL_PWM_InputInit) refers to sys.o(i.NVIC_Init) for NVIC_Init
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_hal.o(i.HAL_PWM_RisingCallback) for HAL_PWM_RisingCallback
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_hal.o(i.HAL_PWM_FallingCallback) for HAL_PWM_FallingCallback
    pwm_hal.o(i.HAL_PWM_InputInit) refers to pwm_hal.o(i.HAL_PWM_CaptureCallback) for HAL_PWM_CaptureCallback
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxCmd) for DRV_PWM_CHxCmd
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxDeadZone) for DRV_PWM_ConfigCHxDeadZone
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxDeadZoneCmd) for DRV_PWM_CHxDeadZoneCmd
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to ioctrl_hal.o(i.HAL_IOCTRL_Swap) for HAL_IOCTRL_Swap
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_SetCHxDirection) for DRV_PWM_SetCHxDirection
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxTimerInverteCmd) for DRV_PWM_CHxTimerInverteCmd
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxPullupCmd) for DRV_PWM_CHxPullupCmd
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_SetCHxLevel) for DRV_PWM_SetCHxLevel
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxTimerInterruptCmd) for DRV_PWM_CHxTimerInterruptCmd
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxClkDiv) for DRV_PWM_ConfigCHxClkDiv
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPerscaler) for DRV_PWM_ConfigCHxPerscaler
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_CHxAutoLoadMode) for DRV_PWM_CHxAutoLoadMode
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxWidth) for DRV_PWM_ConfigCHxWidth
    pwm_hal.o(i.HAL_PWM_OutputInit) refers to pwm_drv.o(i.DRV_PWM_ConfigCHxPeriod) for DRV_PWM_ConfigCHxPeriod
    pwm_hal.o(i.HAL_PWM_SetCHxDirection) refers to pwm_drv.o(i.DRV_PWM_SetCHxDirection) for DRV_PWM_SetCHxDirection
    pwm_hal.o(i.HAL_PWM_SetCHxLevel) refers to pwm_drv.o(i.DRV_PWM_SetCHxLevel) for DRV_PWM_SetCHxLevel
    reset_hal.o(i.HAL_RESET_GetStatus) refers to reset_drv.o(i.DRV_RESET_GetStatus) for DRV_RESET_GetStatus
    reset_hal.o(i.HAL_RESET_SoftReset) refers to reset_drv.o(i.DRV_RESET_SoftReset) for DRV_RESET_SoftReset
    rtc_hal.o(i.HAL_RTC_AralmConfig) refers to sys.o(i.NVIC_Init) for NVIC_Init
    rtc_hal.o(i.HAL_RTC_GetTime) refers to rtc_drv.o(i.DRV_RTC_GetTimeCounter) for DRV_RTC_GetTimeCounter
    rtc_hal.o(i.HAL_RTC_IRQHandler) refers to rtc_drv.o(i.DRV_RTC_IRQHandler) for DRV_RTC_IRQHandler
    rtc_hal.o(i.HAL_RTC_Init) refers to rtc_drv.o(i.DRV_RTC_SetTimeCounter) for DRV_RTC_SetTimeCounter
    rtc_hal.o(i.HAL_RTC_Init) refers to rtc_hal.o(i.HAL_RTC_AralmConfig) for HAL_RTC_AralmConfig
    rtc_hal.o(i.HAL_RTC_Init) refers to delay.o(i.DelayMS) for DelayMS
    rtc_hal.o(i.HAL_RTC_SetTime) refers to rtc_drv.o(i.DRV_RTC_SetTimeCounter) for DRV_RTC_SetTimeCounter
    sdcard_hal.o(i.HAL_SD_EnWideBus) refers to sdio_drv.o(i.ACMD6_SD_tsk) for ACMD6_SD_tsk
    sdcard_hal.o(i.HAL_SD_EnWideBus) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_EnWideBus) refers to sdio_drv.o(i.CMD16_SD_tsk) for CMD16_SD_tsk
    sdcard_hal.o(i.HAL_SD_EnWideBus) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.HAL_SD_Init) for HAL_SD_Init
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to printf8.o(i.__0printf$8) for __2printf
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.HAL_SD_GetCardInfo) for HAL_SD_GetCardInfo
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.HAL_SD_SelectDeselect) for HAL_SD_SelectDeselect
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.HAL_SD_EnWideBus) for HAL_SD_EnWideBus
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.HAL_SD_SendSCR) for HAL_SD_SendSCR
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.SD_SwitchFunc_V2_0) for SD_SwitchFunc_V2_0
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(i.SD_SwitchFunc_V3_0) for SD_SwitchFunc_V3_0
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(.bss) for .bss
    sdcard_hal.o(i.HAL_SD_EnumCard) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_GetCardInfo) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_GetCardInfo) refers to sdcard_hal.o(.bss) for .bss
    sdcard_hal.o(i.HAL_SD_Init) refers to sdio_drv.o(i.SDIO_Reset) for SDIO_Reset
    sdcard_hal.o(i.HAL_SD_Init) refers to sdio_drv.o(i.SDIO_Init_NOINT) for SDIO_Init_NOINT
    sdcard_hal.o(i.HAL_SD_Init) refers to sdio_drv.o(i.SDIO_SetClk) for SDIO_SetClk
    sdcard_hal.o(i.HAL_SD_Init) refers to sdcard_hal.o(i.HAL_SD_PowerON) for HAL_SD_PowerON
    sdcard_hal.o(i.HAL_SD_Init) refers to printf8.o(i.__0printf$8) for __2printf
    sdcard_hal.o(i.HAL_SD_Init) refers to sdcard_hal.o(i.HAL_SD_InitializeCards) for HAL_SD_InitializeCards
    sdcard_hal.o(i.HAL_SD_Init) refers to sdcard_hal.o(.bss) for .bss
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to sdio_drv.o(i.CMD2_SD_tsk) for CMD2_SD_tsk
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to delay.o(i.DelayMS) for DelayMS
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to sdio_drv.o(i.CMD3_SD_tsk) for CMD3_SD_tsk
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to printf8.o(i.__0printf$8) for __2printf
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to sdio_drv.o(i.CMD9_SD_tsk) for CMD9_SD_tsk
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to sdcard_hal.o(.bss) for .bss
    sdcard_hal.o(i.HAL_SD_InitializeCards) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_PowerON) refers to sdio_drv.o(i.CMD0_SD_tsk) for CMD0_SD_tsk
    sdcard_hal.o(i.HAL_SD_PowerON) refers to delay.o(i.DelayMS) for DelayMS
    sdcard_hal.o(i.HAL_SD_PowerON) refers to sdio_drv.o(i.CMD8_SD_tsk) for CMD8_SD_tsk
    sdcard_hal.o(i.HAL_SD_PowerON) refers to sdio_drv.o(i.ACMD41_SD_tsk) for ACMD41_SD_tsk
    sdcard_hal.o(i.HAL_SD_PowerON) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_ReadBlock) refers to sdio_drv.o(i.CMD18_SD_tsk) for CMD18_SD_tsk
    sdcard_hal.o(i.HAL_SD_ReadBlock) refers to sdio_drv.o(i.CMD17_SD_tsk) for CMD17_SD_tsk
    sdcard_hal.o(i.HAL_SD_ReadBlock) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_ReadBlock) refers to sdcard_hal.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    sdcard_hal.o(i.HAL_SD_SelectDeselect) refers to sdio_drv.o(i.CMD7_SD_tsk) for CMD7_SD_tsk
    sdcard_hal.o(i.HAL_SD_SelectDeselect) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_SelectDeselect) refers to sdio_drv.o(i.ACMD42_SD_tsk) for ACMD42_SD_tsk
    sdcard_hal.o(i.HAL_SD_SendSCR) refers to sdio_drv.o(i.ACMD51_SD_tsk) for ACMD51_SD_tsk
    sdcard_hal.o(i.HAL_SD_SendSCR) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_SendSCR) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.HAL_SD_StopTransfer) refers to sdio_drv.o(i.CMD12_SD_tsk) for CMD12_SD_tsk
    sdcard_hal.o(i.HAL_SD_StopTransfer) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdio_drv.o(i.CMD25_SD_tsk) for CMD25_SD_tsk
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdio_drv.o(i.CMD24_SD_tsk) for CMD24_SD_tsk
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdcard_hal.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdio_drv.o(i.CMD13_SD_tsk) for CMD13_SD_tsk
    sdcard_hal.o(i.HAL_SD_WriteBlock) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.SDIO_CMD53_Xfer) refers to sdio_drv.o(i.SDIO_PollStatus) for SDIO_PollStatus
    sdcard_hal.o(i.SDIO_CMD53_Xfer) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SDIO_CMD53_Xfer) refers to sdio_drv.o(.bss) for sddesbuf
    sdcard_hal.o(i.SDIO_EnableAsyncInterrupt) refers to sdcard_hal.o(i.SDIO_IO_RW_Direct) for SDIO_IO_RW_Direct
    sdcard_hal.o(i.SDIO_GetCardCapability) refers to memseta.o(.text) for __aeabi_memclr4
    sdcard_hal.o(i.SDIO_GetCardCapability) refers to sdcard_hal.o(i.SDIO_IO_RW_Direct) for SDIO_IO_RW_Direct
    sdcard_hal.o(i.SDIO_GetCardCapability) refers to sdcard_hal.o(.bss) for .bss
    sdcard_hal.o(i.SDIO_IO_RW_Direct) refers to sdio_drv.o(i.CMD52_SD_tsk) for CMD52_SD_tsk
    sdcard_hal.o(i.SDIO_SetDriverStrength) refers to sdcard_hal.o(i.SDIO_IO_RW_Direct) for SDIO_IO_RW_Direct
    sdcard_hal.o(i.SDIO_SwitchToHighSpeed) refers to sdcard_hal.o(i.SDIO_IO_RW_Direct) for SDIO_IO_RW_Direct
    sdcard_hal.o(i.SDIO_SwitchToHighSpeed) refers to sdcard_hal.o(i.SDIO_SetDriverStrength) for SDIO_SetDriverStrength
    sdcard_hal.o(i.SDIO_SwitchToHighSpeed) refers to sdio_drv.o(i.SDIO_SetClk) for SDIO_SetClk
    sdcard_hal.o(i.SD_ReadBlock_Start) refers to sdio_drv.o(i.CMD18_SD_tsk) for CMD18_SD_tsk
    sdcard_hal.o(i.SD_ReadBlock_Start) refers to sdio_drv.o(i.CMD17_SD_tsk) for CMD17_SD_tsk
    sdcard_hal.o(i.SD_ReadBlock_Start) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SD_ReadBlock_Stop) refers to sdcard_hal.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    sdcard_hal.o(i.SD_SwitchFunc_V2_0) refers to sdio_drv.o(i.CMD6_SD_tsk) for CMD6_SD_tsk
    sdcard_hal.o(i.SD_SwitchFunc_V2_0) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SD_SwitchFunc_V2_0) refers to sdio_drv.o(i.SDIO_SetClk) for SDIO_SetClk
    sdcard_hal.o(i.SD_SwitchFunc_V3_0) refers to sdio_drv.o(i.CMD6_SD_tsk) for CMD6_SD_tsk
    sdcard_hal.o(i.SD_SwitchFunc_V3_0) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SD_SwitchFunc_V3_0) refers to sdio_drv.o(i.SDIO_SetClk) for SDIO_SetClk
    sdcard_hal.o(i.SD_WriteBlock_Start) refers to sdio_drv.o(i.CMD25_SD_tsk) for CMD25_SD_tsk
    sdcard_hal.o(i.SD_WriteBlock_Start) refers to sdio_drv.o(i.CMD24_SD_tsk) for CMD24_SD_tsk
    sdcard_hal.o(i.SD_WriteBlock_Start) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SD_WriteBlock_Start) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.SD_WriteBlock_Stop) refers to sdcard_hal.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    sdcard_hal.o(i.SD_WriteBlock_Stop) refers to sdio_drv.o(i.CMD13_SD_tsk) for CMD13_SD_tsk
    sdcard_hal.o(i.SD_WriteBlock_Stop) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.SD_WriteBlock_Stop) refers to sdcard_hal.o(.data) for .data
    sdcard_hal.o(i.core_sdio_xfer) refers to sdio_drv.o(i.CMD0_SD_tsk) for CMD0_SD_tsk
    sdcard_hal.o(i.core_sdio_xfer) refers to sdio_drv.o(i.CMD3_SD_tsk) for CMD3_SD_tsk
    sdcard_hal.o(i.core_sdio_xfer) refers to sdio_drv.o(i.CMD5_SD_tsk) for CMD5_SD_tsk
    sdcard_hal.o(i.core_sdio_xfer) refers to delay.o(i.delay) for delay
    sdcard_hal.o(i.core_sdio_xfer) refers to sdio_drv.o(i.CMD7_SD_tsk) for CMD7_SD_tsk
    sdcard_hal.o(i.core_sdio_xfer) refers to sdcard_hal.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    sdcard_hal.o(i.core_sdio_xfer) refers to sdio_drv.o(i.CMD52_SD_tsk) for CMD52_SD_tsk
    sdcard_hal.o(i.core_sdio_xfer) refers to sdcard_hal.o(i.SDIO_CMD53_Xfer) for SDIO_CMD53_Xfer
    sdcard_hal.o(i.core_sdio_xfer) refers to sdcard_hal.o(.data) for .data
    sdram_hal.o(i.HAL_SDRAM_Init) refers to sdram_drv.o(i.DRV_SDRAM_Init) for DRV_SDRAM_Init
    sdram2lcd_hal.o(i.HAL_SDRAM2LCD_Init) refers to sdram2lcd_drv.o(i.DRV_SDRAM2LCD_Init) for DRV_SDRAM2LCD_Init
    spi_hal.o(i.HAL_SPI_ClrFlag) refers to spi_drv.o(i.DRV_SPI_ClrFlag) for DRV_SPI_ClrFlag
    spi_hal.o(i.HAL_SPI_ClrFlag) refers to spi_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    spi_hal.o(i.HAL_SPI_DeInit) refers to spi_drv.o(i.DRV_SPI_DeInit) for DRV_SPI_DeInit
    spi_hal.o(i.HAL_SPI_GPIODeInit) refers to spi_drv.o(i.DRV_SPI_GPIODeInit) for DRV_SPI_GPIODeInit
    spi_hal.o(i.HAL_SPI_GPIOInit) refers to spi_drv.o(i.DRV_SPI_GPIOInit) for DRV_SPI_GPIOInit
    spi_hal.o(i.HAL_SPI_GPIOReadPin) refers to spi_drv.o(i.DRV_SPI_ReadPin) for DRV_SPI_ReadPin
    spi_hal.o(i.HAL_SPI_GPIOTogglePin) refers to spi_drv.o(i.DRV_SPI_TogglePin) for DRV_SPI_TogglePin
    spi_hal.o(i.HAL_SPI_GPIOWritePin) refers to spi_drv.o(i.DRV_SPI_WritePin) for DRV_SPI_WritePin
    spi_hal.o(i.HAL_SPI_GetFlag) refers to spi_drv.o(i.DRV_SPI_GetFlag) for DRV_SPI_GetFlag
    spi_hal.o(i.HAL_SPI_GetFlag) refers to spi_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    spi_hal.o(i.HAL_SPI_IRQ) refers to spi_drv.o(i.DRV_SPI_SetDR) for DRV_SPI_SetDR
    spi_hal.o(i.HAL_SPI_Init) refers to spi_hal.o(i.HAL_SPI_MspInit) for HAL_SPI_MspInit
    spi_hal.o(i.HAL_SPI_Init) refers to spi_drv.o(i.DRV_SPI_Init) for DRV_SPI_Init
    spi_hal.o(i.HAL_SPI_Receive) refers to spi_drv.o(i.DRV_SPI_ReceiveBytes) for DRV_SPI_ReceiveBytes
    spi_hal.o(i.HAL_SPI_Receive) refers to spi_drv.o(i.DRV_SPI_SlaveReceiveBytes) for DRV_SPI_SlaveReceiveBytes
    spi_hal.o(i.HAL_SPI_Receive) refers to spi_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    spi_hal.o(i.HAL_SPI_Transmit) refers to spi_drv.o(i.DRV_SPI_TransmitBytes) for DRV_SPI_TransmitBytes
    spi_hal.o(i.HAL_SPI_Transmit) refers to spi_drv.o(i.DRV_SPI_SlaveTransmitBytes) for DRV_SPI_SlaveTransmitBytes
    spi_hal.o(i.HAL_SPI_Transmit) refers to spi_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    spi_hal.o(i.HAL_SPI_TransmitIT) refers to spi_drv.o(i.DRV_SPI_SetDR) for DRV_SPI_SetDR
    spi_hal.o(i.HAL_SPI_TransmitReceive) refers to spi_hal.o(i.HAL_SPI_Transmit) for HAL_SPI_Transmit
    spi_hal.o(i.HAL_SPI_TransmitReceive) refers to spi_hal.o(i.HAL_SPI_Receive) for HAL_SPI_Receive
    spi_hal.o(i.HAL_SPI_WaitonFlagTimeout) refers to spi_drv.o(i.DRV_SPI_WaitonFlagTimeout) for DRV_SPI_WaitonFlagTimeout
    spi_hal.o(i.HAL_SPI_WaitonFlagTimeout) refers to spi_hal.o(i.DrvStatusToHalStatus) for DrvStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_DMA_Receive_level) refers to ssi_drv.o(i.DRV_SSI_DMA_Receive_level) for DRV_SSI_DMA_Receive_level
    ssi_hal.o(i.HAL_SSI_DMA_Transmit_level) refers to ssi_drv.o(i.DRV_SSI_DMA_Transmit_level) for DRV_SSI_DMA_Transmit_level
    ssi_hal.o(i.HAL_SSI_DUAL_DMA_Trig) refers to ssi_drv.o(i.DRV_SSI_DUAL_DMA_Trig) for DRV_SSI_DUAL_DMA_Trig
    ssi_hal.o(i.HAL_SSI_DeInit) refers to ssi_drv.o(i.DRV_SSI_StructInit) for DRV_SSI_StructInit
    ssi_hal.o(i.HAL_SSI_DeInit) refers to ssi_drv.o(i.DRV_SSI_DeInit) for DRV_SSI_DeInit
    ssi_hal.o(i.HAL_SSI_DeInit) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_STD_Program) for DRV_SSI_EFlash_STD_Program
    ssi_hal.o(i.HAL_SSI_EFlash_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program) for DRV_SSI_EFlash_QUAD_Program
    ssi_hal.o(i.HAL_SSI_EFlash_Program) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_EXIT) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT) for DRV_SSI_EFlash_QPI_EXIT
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_EXIT) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_STD_Init) for DRV_SSI_STD_Init
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter) for DRV_SSI_EFlash_QPI_Enter
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Enter) refers to ssi_drv.o(i.DRV_EFlash_Set_Read_Para) for DRV_EFlash_Set_Read_Para
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Enter) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Program) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program) for DRV_SSI_EFlash_QPI_Program
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Program) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Read) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Read) for DRV_SSI_EFlash_QPI_Read
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Read) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase) for DRV_SSI_EFlash_QPI_Sector_Erase
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Sector_Erase) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable) for DRV_SSI_EFlash_QPI_Write_Enable
    ssi_hal.o(i.HAL_SSI_EFlash_QPI_Write_Enable) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_Read) refers to ssi_drv.o(i.DRV_SSI_EFlash_STD_Read) for DRV_SSI_EFlash_STD_Read
    ssi_hal.o(i.HAL_SSI_EFlash_Read) refers to ssi_drv.o(i.DRV_SSI_EFlash_DUAL_Read) for DRV_SSI_EFlash_DUAL_Read
    ssi_hal.o(i.HAL_SSI_EFlash_Read) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_Read) refers to ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Read) for DRV_SSI_EFlash_QUAD_Read
    ssi_hal.o(i.HAL_SSI_EFlash_Sector_Erase) refers to ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase) for DRV_SSI_EFlash_STD_Sector_Erase
    ssi_hal.o(i.HAL_SSI_EFlash_Sector_Erase) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_EFlash_Write_Enable) refers to ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable) for DRV_SSI_EFlash_Write_Enable
    ssi_hal.o(i.HAL_SSI_EFlash_Write_Enable) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_FLASH_Reset) refers to ssi_drv.o(i.DRV_SSI_STD_Reset_Enable) for DRV_SSI_STD_Reset_Enable
    ssi_hal.o(i.HAL_SSI_FLASH_Reset) refers to ssi_drv.o(i.DRV_SSI_STD_Reset) for DRV_SSI_STD_Reset
    ssi_hal.o(i.HAL_SSI_FLASH_Reset) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_Init) refers to ssi_hal.o(i.HAL_SSI_MspInit) for HAL_SSI_MspInit
    ssi_hal.o(i.HAL_SSI_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    ssi_hal.o(i.HAL_SSI_Init) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_QPI_DMA_Trig) refers to ssi_drv.o(i.DRV_SSI_QPI_DMA_Trig) for DRV_SSI_QPI_DMA_Trig
    ssi_hal.o(i.HAL_SSI_QUAD_DMA_Trig) refers to ssi_drv.o(i.DRV_SSI_QUAD_DMA_Trig) for DRV_SSI_QUAD_DMA_Trig
    ssi_hal.o(i.HAL_SSI_Read_ID) refers to ssi_drv.o(i.DRV_SSI_STD_Read_ID) for DRV_SSI_STD_Read_ID
    ssi_hal.o(i.HAL_SSI_Read_ID) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_SSI_STD_DMA_Program) refers to ssi_drv.o(i.SSI_STD_DMA_Program) for SSI_STD_DMA_Program
    ssi_hal.o(i.HAL_SSI_STD_DMA_Read) refers to ssi_drv.o(i.SSI_STD_DMA_Read) for SSI_STD_DMA_Read
    ssi_hal.o(i.HAL_SSI_STD_DMA_Trig) refers to ssi_drv.o(i.DRV_SSI_STD_DMA_Trig) for DRV_SSI_STD_DMA_Trig
    ssi_hal.o(i.HAL_SSI_Standard_Init) refers to ssi_drv.o(i.SSI_Standard_Init) for SSI_Standard_Init
    ssi_hal.o(i.HAL_SSI_WAIT_IDLE) refers to ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout) for DRV_SSI_WaitonFlagTimeout
    ssi_hal.o(i.HAL_SSI_WAIT_IDLE) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_XIP_EXIT) refers to ssi_drv.o(i.DRV_XIP_EXIT) for DRV_XIP_EXIT
    ssi_hal.o(i.HAL_XIP_EXIT) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    ssi_hal.o(i.HAL_XIP_Enter) refers to ssi_drv.o(i.DRV_XIP_Enter) for DRV_XIP_Enter
    ssi_hal.o(i.HAL_XIP_Enter) refers to ssi_hal.o(i.DrvSSIStatusToHalStatus) for DrvSSIStatusToHalStatus
    systick_hal.o(i.HAL_Delay_ms) refers to systick_hal.o(.data) for .data
    systick_hal.o(i.HAL_SYSTICK_Init) refers to cpm_drv.o(.data) for g_core_clk
    systick_hal.o(i.HAL_TimingDelay_Decrement) refers to systick_hal.o(.data) for .data
    tc_hal.o(i.HAL_TC_Callback) refers to printf8.o(i.__0printf$8) for __2printf
    tc_hal.o(i.HAL_TC_IRQHandler) refers to tc_hal.o(.data) for .data
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_DebugCmd) for DRV_TC_DebugCmd
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_DozeCmd) for DRV_TC_DozeCmd
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_WaitCmd) for DRV_TC_WaitCmd
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_StopCmd) for DRV_TC_StopCmd
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_ResetCmd) for DRV_TC_ResetCmd
    tc_hal.o(i.HAL_TC_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    tc_hal.o(i.HAL_TC_Init) refers to tc_drv.o(i.DRV_TC_InterruptCmd) for DRV_TC_InterruptCmd
    tc_hal.o(i.HAL_TC_Init) refers to tc_hal.o(i.HAL_TC_Callback) for HAL_TC_Callback
    tc_hal.o(i.HAL_TC_Init) refers to tc_hal.o(.data) for .data
    uart_hal.o(i.HAL_UART_DeInit) refers to uart_drv.o(i.DRV_UART_Deinit) for DRV_UART_Deinit
    uart_hal.o(i.HAL_UART_DisItRe) refers to uart_drv.o(i.DRV_UART_DisItRe) for DRV_UART_DisItRe
    uart_hal.o(i.HAL_UART_DisItTcie) refers to uart_drv.o(i.DRV_UART_DisItTcie) for DRV_UART_DisItTcie
    uart_hal.o(i.HAL_UART_DisItTie) refers to uart_drv.o(i.DRV_UART_DisItTie) for DRV_UART_DisItTie
    uart_hal.o(i.HAL_UART_EnIt) refers to uart_drv.o(i.DRV_UART_EnIt) for DRV_UART_EnIt
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_DisRx) for DRV_UART_DisRx
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_SetRxdDirOutput) for DRV_UART_SetRxdDirOutput
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_DisTx) for DRV_UART_DisTx
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_SetTxdDirOutput) for DRV_UART_SetTxdDirOutput
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_SetTxdDirInput) for DRV_UART_SetTxdDirInput
    uart_hal.o(i.HAL_UART_GPIOInit) refers to uart_drv.o(i.DRV_UART_SetRxdDirInput) for DRV_UART_SetRxdDirInput
    uart_hal.o(i.HAL_UART_GPIOReadPin) refers to uart_drv.o(i.DRV_UART_GetRxdPinBit) for DRV_UART_GetRxdPinBit
    uart_hal.o(i.HAL_UART_GPIOTogglePin) refers to uart_drv.o(i.DRV_UART_TxdPinToggle) for DRV_UART_TxdPinToggle
    uart_hal.o(i.HAL_UART_GPIOTogglePin) refers to uart_drv.o(i.DRV_UART_RxdPinToggle) for DRV_UART_RxdPinToggle
    uart_hal.o(i.HAL_UART_GPIOWritePin) refers to uart_drv.o(i.DRV_UART_ResetTxdPinBit) for DRV_UART_ResetTxdPinBit
    uart_hal.o(i.HAL_UART_GPIOWritePin) refers to uart_drv.o(i.DRV_UART_ResetRxdPinBit) for DRV_UART_ResetRxdPinBit
    uart_hal.o(i.HAL_UART_GPIOWritePin) refers to uart_drv.o(i.DRV_UART_SetRxdPinBit) for DRV_UART_SetRxdPinBit
    uart_hal.o(i.HAL_UART_GPIOWritePin) refers to uart_drv.o(i.DRV_UART_SetTxdPinBit) for DRV_UART_SetTxdPinBit
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_GetStatus) for DRV_UART_GetStatus
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_GetItSource) for DRV_UART_GetItSource
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_DisIt) for DRV_UART_DisIt
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_hal.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_SendData) for DRV_UART_SendData
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_EnIt) for DRV_UART_EnIt
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_drv.o(i.DRV_UART_GetData) for DRV_UART_GetData
    uart_hal.o(i.HAL_UART_IRQHandler) refers to uart_hal.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    uart_hal.o(i.HAL_UART_ISR_IRQHandler) refers to uart_drv.o(i.UART_ISR) for UART_ISR
    uart_hal.o(i.HAL_UART_Init) refers to uart_hal.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    uart_hal.o(i.HAL_UART_Init) refers to uart_drv.o(i.DRV_UART_Dis) for DRV_UART_Dis
    uart_hal.o(i.HAL_UART_Init) refers to uart_drv.o(i.DRV_UART_Init) for DRV_UART_Init
    uart_hal.o(i.HAL_UART_Init) refers to uart_drv.o(i.DRV_UART_EnTx) for DRV_UART_EnTx
    uart_hal.o(i.HAL_UART_Init) refers to uart_drv.o(i.DRV_UART_EnRx) for DRV_UART_EnRx
    uart_hal.o(i.HAL_UART_Receive) refers to uart_drv.o(i.DRV_UART_WaitonFlagTimeout) for DRV_UART_WaitonFlagTimeout
    uart_hal.o(i.HAL_UART_Receive) refers to uart_drv.o(i.DRV_UART_GetData) for DRV_UART_GetData
    uart_hal.o(i.HAL_UART_ReceiveIT) refers to uart_drv.o(i.DRV_UART_EnIt) for DRV_UART_EnIt
    uart_hal.o(i.HAL_UART_RecvByteIT) refers to uart_drv.o(i.UART_RecvByte) for UART_RecvByte
    uart_hal.o(i.HAL_UART_SendByteIT) refers to uart_drv.o(i.UART_SendByte) for UART_SendByte
    uart_hal.o(i.HAL_UART_SendData) refers to uart_drv.o(i.DRV_UART_SendData) for DRV_UART_SendData
    uart_hal.o(i.HAL_UART_Transmit) refers to uart_drv.o(i.DRV_UART_WaitonFlagTimeout) for DRV_UART_WaitonFlagTimeout
    uart_hal.o(i.HAL_UART_Transmit) refers to uart_drv.o(i.DRV_UART_SendData) for DRV_UART_SendData
    uart_hal.o(i.HAL_UART_TransmitIT) refers to uart_drv.o(i.DRV_UART_DisIt) for DRV_UART_DisIt
    uart_hal.o(i.HAL_UART_TransmitIT) refers to uart_drv.o(i.DRV_UART_EnIt) for DRV_UART_EnIt
    wdt_hal.o(i.HAL_WDT_CMD) refers to wdt_drv.o(i.DRV_WDT_Close) for DRV_WDT_Close
    wdt_hal.o(i.HAL_WDT_CMD) refers to wdt_drv.o(i.DRV_WDT_Open) for DRV_WDT_Open
    wdt_hal.o(i.HAL_WDT_FeedWatchdog) refers to wdt_drv.o(i.DRV_WDT_FeedDog) for DRV_WDT_FeedDog
    wdt_hal.o(i.HAL_WDT_GetCounter) refers to wdt_drv.o(i.DRV_WDT_GetCount) for DRV_WDT_GetCount
    wdt_hal.o(i.HAL_WDT_Init) refers to wdt_drv.o(i.DRV_WDT_Init) for DRV_WDT_Init
    sys.o(i.NVIC_Init) refers to sys.o(i.NVIC_PriorityGroupConfig) for NVIC_PriorityGroupConfig
    system_armcm4.o(i.SystemInit) refers to cpm_hal.o(i.HAL_CPM_SetCLKDiv) for HAL_CPM_SetCLKDiv
    system_armcm4.o(i.SystemInit) refers to cache_hal.o(i.HAL_CACHE_Init) for HAL_CACHE_Init
    system_armcm4.o(i.SystemInit) refers to startup_armcm4.o(RESET) for __Vectors
    startup_armcm4.o(RESET) refers to startup_armcm4.o(STACK) for __initial_sp
    startup_armcm4.o(RESET) refers to startup_armcm4.o(.text) for Reset_Handler
    startup_armcm4.o(RESET) refers to interrupt.o(i.HardFault_Handler) for HardFault_Handler
    startup_armcm4.o(RESET) refers to interrupt.o(i.MemManage_Handler) for MemManage_Handler
    startup_armcm4.o(RESET) refers to interrupt.o(i.BusFault_Handler) for BusFault_Handler
    startup_armcm4.o(RESET) refers to interrupt.o(i.UsageFault_Handler) for UsageFault_Handler
    startup_armcm4.o(RESET) refers to port.o(.emb_text) for SVC_Handler
    startup_armcm4.o(RESET) refers to port.o(i.SysTick_Handler) for SysTick_Handler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EFM_IRQHandler) for EFM_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PMU_IRQHandler) for PMU_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.TC_IRQHandler) for TC_IRQHandler
    startup_armcm4.o(RESET) refers to pit.o(i.PIT1_IRQHandler) for PIT1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.ENCR_IRQHandler) for ENCR_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.ENCR1_IRQHandler) for ENCR1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.DMA1_IRQHandler) for DMA1_IRQHandler
    startup_armcm4.o(RESET) refers to dac_wav.o(i.DMA2_IRQHandler) for DMA2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.DMA2D_IRQHandler) for DMA2D_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.TRNG_IRQHandler) for TRNG_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SEC_PGD_LD_FD_IRQHandler) for SEC_PGD_LD_FD_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PCI_DET_IRQHandler) for PCI_DET_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.ASYNC_TIMER_IRQHandler) for ASYNC_TIMER_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PCI_IRQHandler) for PCI_IRQHandler
    startup_armcm4.o(RESET) refers to rtc.o(i.PMU_RTC_IRQHandler) for PMU_RTC_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.RSA_IRQHandler) for RSA_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SHA_IRQHandler) for SHA_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.AES_IRQHandler) for AES_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SMS4_IRQHandler) for SMS4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.QADC_IRQHandler) for QADC_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.DAC_IRQHandler) for DAC_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.MCC_IRQHandler) for MCC_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.TSI_IRQHandler) for TSI_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.USB_IRQHandler) for USB_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.MIPI_IRQHandler) for MIPI_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPI1_IRQHandler) for SPI1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPI2_IRQHandler) for SPI2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPI3_IRQHandler) for SPI3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPIM1_IRQHandler) for SPIM1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPIM2_IRQHandler) for SPIM2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.SPIM3_IRQHandler) for SPIM3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.UART1_IRQHandler) for UART1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.UART2_IRQHandler) for UART2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.USI3_IRQHandler) for USI3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.I2C1_IRQHandler) for I2C1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM0_IRQHandler) for PWM0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM1_IRQHandler) for PWM1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM2_IRQHandler) for PWM2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM3_IRQHandler) for PWM3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_0_IRQHandler) for EPORT0_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_1_IRQHandler) for EPORT0_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_2_IRQHandler) for EPORT0_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_3_IRQHandler) for EPORT0_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_4_IRQHandler) for EPORT0_4_IRQHandler
    startup_armcm4.o(RESET) refers to ft5216.o(i.EPORT0_5_IRQHandler) for EPORT0_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_6_IRQHandler) for EPORT0_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT0_7_IRQHandler) for EPORT0_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_0_IRQHandler) for EPORT1_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_1_IRQHandler) for EPORT1_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_2_IRQHandler) for EPORT1_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_3_IRQHandler) for EPORT1_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_4_IRQHandler) for EPORT1_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_5_IRQHandler) for EPORT1_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_6_IRQHandler) for EPORT1_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT1_7_IRQHandler) for EPORT1_7_IRQHandler
    startup_armcm4.o(RESET) refers to lcd.o(i.CLCD_IRQHandler) for CLCD_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.I2C2_IRQHandler) for I2C2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.I2C3_IRQHandler) for I2C3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.UART3_IRQHandler) for UART3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.UART4_IRQHandler) for UART4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_0_IRQHandler) for EPORT2_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_1_IRQHandler) for EPORT2_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_2_IRQHandler) for EPORT2_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_3_IRQHandler) for EPORT2_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_4_IRQHandler) for EPORT2_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_5_IRQHandler) for EPORT2_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_6_IRQHandler) for EPORT2_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT2_7_IRQHandler) for EPORT2_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_0_IRQHandler) for EPORT3_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_1_IRQHandler) for EPORT3_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_2_IRQHandler) for EPORT3_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_3_IRQHandler) for EPORT3_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_4_IRQHandler) for EPORT3_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_5_IRQHandler) for EPORT3_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_6_IRQHandler) for EPORT3_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT3_7_IRQHandler) for EPORT3_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_0_IRQHandler) for EPORT4_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_1_IRQHandler) for EPORT4_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_2_IRQHandler) for EPORT4_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_3_IRQHandler) for EPORT4_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_4_IRQHandler) for EPORT4_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_5_IRQHandler) for EPORT4_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_6_IRQHandler) for EPORT4_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT4_7_IRQHandler) for EPORT4_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_0_IRQHandler) for EPORT5_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_1_IRQHandler) for EPORT5_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_2_IRQHandler) for EPORT5_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_3_IRQHandler) for EPORT5_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_4_IRQHandler) for EPORT5_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_5_IRQHandler) for EPORT5_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_6_IRQHandler) for EPORT5_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT5_7_IRQHandler) for EPORT5_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_0_IRQHandler) for EPORT6_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_1_IRQHandler) for EPORT6_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_2_IRQHandler) for EPORT6_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_3_IRQHandler) for EPORT6_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_4_IRQHandler) for EPORT6_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_5_IRQHandler) for EPORT6_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_6_IRQHandler) for EPORT6_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT6_7_IRQHandler) for EPORT6_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_0_IRQHandler) for EPORT7_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_1_IRQHandler) for EPORT7_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_2_IRQHandler) for EPORT7_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_3_IRQHandler) for EPORT7_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_4_IRQHandler) for EPORT7_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_5_IRQHandler) for EPORT7_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_6_IRQHandler) for EPORT7_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT7_7_IRQHandler) for EPORT7_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_0_IRQHandler) for EPORT8_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_1_IRQHandler) for EPORT8_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_2_IRQHandler) for EPORT8_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_3_IRQHandler) for EPORT8_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_4_IRQHandler) for EPORT8_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_5_IRQHandler) for EPORT8_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_6_IRQHandler) for EPORT8_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT8_7_IRQHandler) for EPORT8_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_0_IRQHandler) for EPORT9_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_1_IRQHandler) for EPORT9_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_2_IRQHandler) for EPORT9_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_3_IRQHandler) for EPORT9_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_4_IRQHandler) for EPORT9_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_5_IRQHandler) for EPORT9_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_6_IRQHandler) for EPORT9_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT9_7_IRQHandler) for EPORT9_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_0_IRQHandler) for EPORT10_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_1_IRQHandler) for EPORT10_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_2_IRQHandler) for EPORT10_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_3_IRQHandler) for EPORT10_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_4_IRQHandler) for EPORT10_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_5_IRQHandler) for EPORT10_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_6_IRQHandler) for EPORT10_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT10_7_IRQHandler) for EPORT10_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_0_IRQHandler) for EPORT11_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_1_IRQHandler) for EPORT11_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_2_IRQHandler) for EPORT11_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_3_IRQHandler) for EPORT11_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_4_IRQHandler) for EPORT11_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_5_IRQHandler) for EPORT11_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_6_IRQHandler) for EPORT11_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT11_7_IRQHandler) for EPORT11_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_0_IRQHandler) for EPORT12_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_1_IRQHandler) for EPORT12_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_2_IRQHandler) for EPORT12_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_3_IRQHandler) for EPORT12_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_4_IRQHandler) for EPORT12_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_5_IRQHandler) for EPORT12_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_6_IRQHandler) for EPORT12_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT12_7_IRQHandler) for EPORT12_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_0_IRQHandler) for EPORT13_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_1_IRQHandler) for EPORT13_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_2_IRQHandler) for EPORT13_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_3_IRQHandler) for EPORT13_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_4_IRQHandler) for EPORT13_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_5_IRQHandler) for EPORT13_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_6_IRQHandler) for EPORT13_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT13_7_IRQHandler) for EPORT13_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_0_IRQHandler) for EPORT14_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_1_IRQHandler) for EPORT14_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_2_IRQHandler) for EPORT14_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_3_IRQHandler) for EPORT14_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_4_IRQHandler) for EPORT14_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_5_IRQHandler) for EPORT14_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_6_IRQHandler) for EPORT14_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT14_7_IRQHandler) for EPORT14_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_0_IRQHandler) for EPORT15_0_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_1_IRQHandler) for EPORT15_1_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_2_IRQHandler) for EPORT15_2_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_3_IRQHandler) for EPORT15_3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_4_IRQHandler) for EPORT15_4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_5_IRQHandler) for EPORT15_5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_6_IRQHandler) for EPORT15_6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.EPORT15_7_IRQHandler) for EPORT15_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PIT3_IRQHandler) for PIT3_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PIT4_IRQHandler) for PIT4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM4_IRQHandler) for PWM4_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM5_IRQHandler) for PWM5_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM6_IRQHandler) for PWM6_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.PWM7_IRQHandler) for PWM7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN32_63_IRQHandler) for CAN32_63_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN16_31_IRQHandler) for CAN16_31_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN12_15_IRQHandler) for CAN12_15_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN8_11_IRQHandler) for CAN8_11_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN4_7_IRQHandler) for CAN4_7_IRQHandler
    startup_armcm4.o(RESET) refers to interrupt.o(i.CAN0_3_IRQHandler) for CAN0_3_IRQHandler
    startup_armcm4.o(.text) refers to system_armcm4.o(i.SystemInit) for SystemInit
    startup_armcm4.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    misc_c.o(i.ByteToHexAscii) refers to misc_c.o(i.DigitToHexAscii) for DigitToHexAscii
    misc_c.o(i.Show16BitDecimal) refers to misc_c.o(i.DigitToHexAscii) for DigitToHexAscii
    misc_c.o(i.Show16BitDecimal) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    misc_c.o(i.Show16BitValue) refers to misc_c.o(i.ByteToHexAscii) for ByteToHexAscii
    misc_c.o(i.Show16BitValue) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    misc_c.o(i.Show32BitDecimal) refers to misc_c.o(i.DigitToHexAscii) for DigitToHexAscii
    misc_c.o(i.Show32BitDecimal) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    misc_c.o(i.Show32BitValue) refers to misc_c.o(i.ByteToHexAscii) for ByteToHexAscii
    misc_c.o(i.Show32BitValue) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    misc_c.o(i.Show8BitValue) refers to misc_c.o(i.ByteToHexAscii) for ByteToHexAscii
    misc_c.o(i.Show8BitValue) refers to bsp.o(i.LT768_TFT_ShowAscii) for LT768_TFT_ShowAscii
    ft5216.o(i.CTP_Init) refers to ft5216.o(i.CTP_io_Init) for CTP_io_Init
    ft5216.o(i.CTP_Init) refers to ft5216.o(i.FT5216_Scan) for FT5216_Scan
    ft5216.o(i.CTP_Init) refers to data.o(.bss) for gTpInfo
    ft5216.o(i.CTP_io_Init) refers to i2c.o(i.SCL_OUTPUT) for SCL_OUTPUT
    ft5216.o(i.CTP_io_Init) refers to i2c.o(i.SDA_OUTPUT) for SDA_OUTPUT
    ft5216.o(i.CTP_io_Init) refers to ioctrl_hal.o(i.HAL_IOCTRL_Swapint) for HAL_IOCTRL_Swapint
    ft5216.o(i.CTP_io_Init) refers to delay.o(i.DelayMS) for DelayMS
    ft5216.o(i.CTP_io_Init) refers to i2c.o(i.CT_Read_Nbyte) for CT_Read_Nbyte
    ft5216.o(i.CTP_io_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    ft5216.o(i.CTP_io_Init) refers to eport_drv.o(i.DRV_EPORT_SetTriggerMode) for DRV_EPORT_SetTriggerMode
    ft5216.o(i.CTP_io_Init) refers to eport_drv.o(i.DRV_EPORT_SetIT) for DRV_EPORT_SetIT
    ft5216.o(i.Checksum) refers to printf8.o(i.__0printf$8) for __2printf
    ft5216.o(i.EPORT0_5_IRQHandler) refers to ft5216.o(.data) for .data
    ft5216.o(i.FT5216_Scan) refers to ft5216.o(i.TP_read_XY) for TP_read_XY
    ft5216.o(i.FT5216_Scan) refers to ft5216.o(.data) for .data
    ft5216.o(i.I2C_ReadBytes) refers to i2c_hal.o(i.HAL_I2C_MemRead) for HAL_I2C_MemRead
    ft5216.o(i.I2C_ReadBytes) refers to tp.o(.bss) for I2C1_Handle
    ft5216.o(i.I2C_WriteBytes) refers to i2c_hal.o(i.HAL_I2C_MemWrite) for HAL_I2C_MemWrite
    ft5216.o(i.I2C_WriteBytes) refers to tp.o(.bss) for I2C1_Handle
    ft5216.o(i.TP_read_XY) refers to i2c.o(i.CT_Read_Nbyte) for CT_Read_Nbyte
    ft5216.o(i.TP_read_XY) refers to i2c.o(i.CT_Write_Nbyte) for CT_Write_Nbyte
    ft5216.o(i.TP_read_XY) refers to ft5216.o(.bss) for .bss
    ft5216.o(i.TP_read_XY) refers to data.o(.bss) for gTpInfo
    ft5216.o(i.TP_read_XY) refers to data.o(.data) for First_press
    ft5216.o(i.TP_read_XY) refers to data.o(.data) for First_pressX
    ft5216.o(i.TP_read_XY) refers to data.o(.data) for First_pressY
    inputhz.o(i.Init_PY) refers to inputhz.o(.bss) for .bss
    inputhz.o(i.Search_py) refers to memseta.o(.text) for __aeabi_memclr4
    inputhz.o(i.Search_py) refers to strstr.o(.text) for strstr
    inputhz.o(i.Search_py) refers to bsp.o(i.LT_ReadFlash) for LT_ReadFlash
    inputhz.o(i.Search_py) refers to inputhz.o(.bss) for .bss
    inputhz.o(i.Search_py) refers to inputhz.o(.data) for .data
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.conststring) for .conststring
    inputhz.o(.data) refers to inputhz.o(.constdata) for t9PY_index0
    inputhz.o(.data) refers to inputhz.o(.constdata) for t9PY_index1
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index2
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index3
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index4
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index5
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index6
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index7
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index8
    inputhz.o(.data) refers to inputhz.o(.data) for t9PY_index9
    lcd.o(i.CLCD_IRQHandler) refers to lcd.o(.data) for .data
    lcd.o(i.InitLcd) refers to clcd_hal.o(i.HAL_CLCD_Init) for HAL_CLCD_Init
    lcd.o(i.InitLcd) refers to clcd_hal.o(i.HLA_CLCD_UpuerPannelBaseAddr) for HLA_CLCD_UpuerPannelBaseAddr
    lcd.o(i.InitLcd) refers to clcd_hal.o(i.HLA_CLCD_Cmd) for HLA_CLCD_Cmd
    lcd.o(i.InitLcd) refers to bsp.o(.data) for LCD_XSIZE_TFT
    lcd.o(i.InitLcd) refers to cpm_drv.o(.data) for g_core_clk
    lcd.o(i.InitLcd) refers to lcd.o(.bss) for .bss
    pwm.o(i.ConfigBacklight) refers to pwm_hal.o(i.HAL_PWM_CHxCmd) for HAL_PWM_CHxCmd
    pwm.o(i.ConfigBacklight) refers to pwm.o(.bss) for .bss
    pwm.o(i.ConfigBeep) refers to pwm_hal.o(i.HAL_PWM_CHxCmd) for HAL_PWM_CHxCmd
    pwm.o(i.ConfigBeep) refers to pwm.o(.bss) for .bss
    pwm.o(i.InitBacklight) refers to pwm_hal.o(i.HAL_PWM_Init) for HAL_PWM_Init
    pwm.o(i.InitBacklight) refers to pwm.o(i.ConfigBacklight) for ConfigBacklight
    pwm.o(i.InitBacklight) refers to pwm.o(.bss) for .bss
    pwm.o(i.InitBeep) refers to pwm_hal.o(i.HAL_PWM_Init) for HAL_PWM_Init
    pwm.o(i.InitBeep) refers to pwm.o(i.ConfigBeep) for ConfigBeep
    pwm.o(i.InitBeep) refers to pwm.o(.bss) for .bss
    pwm.o(i.InitPort) refers to ioctrl_hal.o(i.HAL_IOCTRL_Swapint) for HAL_IOCTRL_Swapint
    pwm.o(i.InitPort) refers to eport_hal.o(i.HAL_EPORT_Init) for HAL_EPORT_Init
    tp.o(i.InitTouch) refers to ioctrl_hal.o(i.HAL_IOCTRL_I2CInit) for HAL_IOCTRL_I2CInit
    tp.o(i.InitTouch) refers to i2c_hal.o(i.HAL_I2C_Init) for HAL_I2C_Init
    tp.o(i.InitTouch) refers to ioctrl_hal.o(i.HAL_IOCTRL_Swapint) for HAL_IOCTRL_Swapint
    tp.o(i.InitTouch) refers to delay.o(i.DelayMS) for DelayMS
    tp.o(i.InitTouch) refers to tp.o(i.ReadBytes) for ReadBytes
    tp.o(i.InitTouch) refers to tp.o(.data) for .data
    tp.o(i.InitTouch) refers to tp.o(.bss) for .bss
    tp.o(i.ReadBytes) refers to i2c_hal.o(i.HAL_I2C_MemRead) for HAL_I2C_MemRead
    tp.o(i.ReadBytes) refers to tp.o(.bss) for .bss
    tp.o(i.ReadTouchData) refers to tp.o(i.ReadBytes) for ReadBytes
    tp.o(i.ReadTouchData) refers to tp.o(i.CtpX) for CtpX
    tp.o(i.ReadTouchData) refers to tp.o(i.CtpY) for CtpY
    tp.o(i.ReadTouchData2) refers to i2c_hal.o(i.HAL_I2C_MemRead) for HAL_I2C_MemRead
    tp.o(i.ReadTouchData2) refers to i2c_hal.o(i.HAL_I2C_MemWrite) for HAL_I2C_MemWrite
    tp.o(i.ReadTouchData2) refers to printf8.o(i.__0printf$8) for __2printf
    tp.o(i.ReadTouchData2) refers to tp.o(.bss) for .bss
    winbond.o(i.CS_FLash_RESET) refers to bsp.o(.data) for Flash_type
    winbond.o(i.CS_FLash_SET) refers to bsp.o(.data) for Flash_type
    winbond.o(i.Flash_Enter_QPI) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.Flash_Enter_QPI) refers to winbond.o(i.W25QXX_Enter_QPI_STD) for W25QXX_Enter_QPI_STD
    winbond.o(i.Flash_Enter_QPI) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.SPI5_Dual_Read_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    winbond.o(i.SPI5_Dual_Read_Init) refers to winbond.o(.bss) for .bss
    winbond.o(i.SPI5_Dual_Read_Init_test) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    winbond.o(i.SPI5_Dual_Read_Init_test) refers to winbond.o(.bss) for .bss
    winbond.o(i.SPI5_QPI_Set_DataNum) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    winbond.o(i.SPI5_Quad_Read_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    winbond.o(i.SPI5_Quad_Read_Init) refers to winbond.o(.bss) for .bss
    winbond.o(i.SPI5_Quad_Write_Init) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    winbond.o(i.SPI5_Quad_Write_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    winbond.o(i.SPI5_Quad_Write_Init) refers to winbond.o(.bss) for .bss
    winbond.o(i.SPI5_STD_Init) refers to ssi_drv.o(i.DRV_SSI_Init) for DRV_SSI_Init
    winbond.o(i.SPI5_STD_Init) refers to winbond.o(.bss) for .bss
    winbond.o(i.SPI5_STD_Init) refers to bsp.o(.data) for Flash_type
    winbond.o(i.SPI5_Set_DataNum) refers to ssi_drv.o(i.DRV_SSI_Cmd) for DRV_SSI_Cmd
    winbond.o(i.SSI2_DMA_RX) refers to dma_hal.o(i.HAL_DMAC_Deinit) for HAL_DMAC_Deinit
    winbond.o(i.SSI2_DMA_RX) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    winbond.o(i.SSI2_DMA_RX) refers to dma_hal.o(i.HAL_DMAC_StartPolling) for HAL_DMAC_StartPolling
    winbond.o(i.SSI2_DMA_RX) refers to dma_hal.o(i.HAL_DMAC_PollForTransfer) for HAL_DMAC_PollForTransfer
    winbond.o(i.SSI2_DMA_RX_Continue) refers to dma_hal.o(i.HAL_DMAC_Deinit) for HAL_DMAC_Deinit
    winbond.o(i.SSI2_DMA_RX_Continue) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    winbond.o(i.SSI2_DMA_RX_Continue) refers to dma_hal.o(i.HAL_DMAC_StartPolling) for HAL_DMAC_StartPolling
    winbond.o(i.SSI2_DMA_RX_Continue) refers to dma_hal.o(i.HAL_DMAC_PollForTransfer) for HAL_DMAC_PollForTransfer
    winbond.o(i.SSI2_DMA_TX) refers to dma_hal.o(i.HAL_DMAC_Deinit) for HAL_DMAC_Deinit
    winbond.o(i.SSI2_DMA_TX) refers to dma_hal.o(i.HAL_DMAC_Init) for HAL_DMAC_Init
    winbond.o(i.SSI2_DMA_TX) refers to dma_hal.o(i.HAL_DMAC_StartPolling) for HAL_DMAC_StartPolling
    winbond.o(i.SSI2_DMA_TX) refers to dma_hal.o(i.HAL_DMAC_PollForTransfer) for HAL_DMAC_PollForTransfer
    winbond.o(i.W25N01GV_PageRead_Mode) refers to winbond.o(i.W25NXX_ReadSR) for W25NXX_ReadSR
    winbond.o(i.W25N01GV_PageRead_Mode) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_ContinuousRead_Mode) refers to winbond.o(i.W25NXX_ReadSR) for W25NXX_ReadSR
    winbond.o(i.W25NXX_ContinuousRead_Mode) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_EraseFlash) refers to printf8.o(i.__0printf$8) for __2printf
    winbond.o(i.W25NXX_EraseFlash) refers to winbond.o(i.W25NXX_Erase_Block) for W25NXX_Erase_Block
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.W25NXX_Write_Enable) for W25NXX_Write_Enable
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_Erase_Block) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_ReadID) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_ReadID) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_ReadID) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_ReadSR) for W25NXX_ReadSR
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.SPI5_Quad_Read_Init) for SPI5_Quad_Read_Init
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.SSI2_DMA_RX) for SSI2_DMA_RX
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.Check_SSI2_Busy) for Check_SSI2_Busy
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25NXX_ReadPageAddr_Data_STD) refers to winbond.o(i.W25N01GV_PageRead_Mode) for W25N01GV_PageRead_Mode
    winbond.o(i.W25NXX_ReadPageAddr_Data_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_ReadPageAddr_Data_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_ReadPageAddr_Data_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_ReadPageAddr_Data_STD) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    winbond.o(i.W25NXX_ReadSR) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_ReadSR) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_ReadSR) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_Read_NoCheck) refers to winbond.o(i.W25NXX_ReadPageAddr_Data_STD) for W25NXX_ReadPageAddr_Data_STD
    winbond.o(i.W25NXX_Read_NoCheck) refers to winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD) for W25NXX_ReadPageAddr_Data_QUAD
    winbond.o(i.W25NXX_Wait_Busy) refers to winbond.o(i.W25NXX_ReadSR) for W25NXX_ReadSR
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_Write_Enable) for W25NXX_Write_Enable
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.SPI5_Quad_Write_Init) for SPI5_Quad_Write_Init
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.SSI2_DMA_TX) for SSI2_DMA_TX
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.Check_SSI2_Busy) for Check_SSI2_Busy
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.W25N01GV_PageRead_Mode) for W25N01GV_PageRead_Mode
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.W25NXX_Write_SR) for W25NXX_Write_SR
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.W25NXX_Write_Enable) for W25NXX_Write_Enable
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_WritePageAddr_Data_STD) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    winbond.o(i.W25NXX_Write_Disable) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_Write_Disable) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_Write_Disable) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_Write_Enable) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_Write_Enable) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_Write_Enable) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_Write_NoCheck) refers to winbond.o(i.W25NXX_WritePageAddr_Data_STD) for W25NXX_WritePageAddr_Data_STD
    winbond.o(i.W25NXX_Write_NoCheck) refers to winbond.o(i.W25NXX_WritePageAddr_Data_QUAD) for W25NXX_WritePageAddr_Data_QUAD
    winbond.o(i.W25NXX_Write_SR) refers to winbond.o(i.W25NXX_Write_Enable) for W25NXX_Write_Enable
    winbond.o(i.W25NXX_Write_SR) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25NXX_Write_SR) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25NXX_Write_SR) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25NXX_Write_SR) refers to winbond.o(i.W25NXX_Write_Disable) for W25NXX_Write_Disable
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_BlockErase64KB_STD) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Enter_4Byte_AddressMode_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Enter_4Byte_AddressMode_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Enter_4Byte_AddressMode_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Enter_QPI_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Enter_QPI_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Enter_QPI_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Erase_Chip_STD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_Erase_Chip_STD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_Erase_Chip_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Erase_Chip_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Open_QUAD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Open_QUAD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Open_QUAD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Open_QUAD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_Open_QUAD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_ReadID_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_ReadID_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_ReadID_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_ReadID_STD_9F) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_ReadID_STD_9F) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_ReadID_STD_9F) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_ReadSR_1_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_ReadSR_1_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_ReadSR_1_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(i.SPI5_Dual_Read_Init) for SPI5_Dual_Read_Init
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(i.SPI5_Set_DataNum) for SPI5_Set_DataNum
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(i.SSI2_DMA_RX) for SSI2_DMA_RX
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(i.Check_SSI2_Busy) for Check_SSI2_Busy
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Read_DUAL) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(i.SPI5_Quad_Read_Init) for SPI5_Quad_Read_Init
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(i.SSI2_DMA_RX) for SSI2_DMA_RX
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(i.Check_SSI2_Busy) for Check_SSI2_Busy
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Read_QUAD) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(i.SPI5_Quad_Read_Init) for SPI5_Quad_Read_Init
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(i.SPI5_Set_DataNum) for SPI5_Set_DataNum
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(i.SSI2_DMA_RX) for SSI2_DMA_RX
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(i.Check_SSI2_Busy) for Check_SSI2_Busy
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Read_QUAD_DMA) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25QXX_Read_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Read_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Read_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Read_STD) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_SectorErase4KB_STD) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Wait_Busy_STD) refers to winbond.o(i.W25QXX_ReadSR_1_STD) for W25QXX_ReadSR_1_STD
    winbond.o(i.W25QXX_Write_Disable_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Write_Disable_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Write_Disable_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Write_Enable_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Write_Enable_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Write_Enable_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Write_NoCheck_QUAD) refers to winbond.o(i.W25QXX_Write_Page_QUAD) for W25QXX_Write_Page_QUAD
    winbond.o(i.W25QXX_Write_NoCheck_STD) refers to winbond.o(i.W25QXX_Write_Page_STD) for W25QXX_Write_Page_STD
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(i.SPI5_STD_Init) for SPI5_STD_Init
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(i.SPI5_Quad_Write_Init) for SPI5_Quad_Write_Init
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(i.SSI2_DMA_TX) for SSI2_DMA_TX
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(.data) for .data
    winbond.o(i.W25QXX_Write_Page_QUAD) refers to winbond.o(.bss) for .bss
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(i.W25QXX_Write_Enable_STD) for W25QXX_Write_Enable_STD
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(i.W25QXX_Wait_Busy_STD) for W25QXX_Wait_Busy_STD
    winbond.o(i.W25QXX_Write_Page_STD) refers to winbond.o(.data) for .data
    winbond.o(i.Write_Page) refers to winbond.o(i.CS_FLash_RESET) for CS_FLash_RESET
    winbond.o(i.Write_Page) refers to winbond.o(i.SSI2_ReadWriteByte) for SSI2_ReadWriteByte
    winbond.o(i.Write_Page) refers to winbond.o(i.CS_FLash_SET) for CS_FLash_SET
    winbond.o(i.Write_Page) refers to winbond.o(i.W25NXX_Wait_Busy) for W25NXX_Wait_Busy
    rtc.o(i.LT_RtcInit) refers to rtc.o(i.RTC_Get) for RTC_Get
    rtc.o(i.LT_RtcInit) refers to sys.o(i.NVIC_Init) for NVIC_Init
    rtc.o(i.LT_RtcInit) refers to rtc.o(i.RTC_Set) for RTC_Set
    rtc.o(i.LT_RtcInit) refers to cpm_drv.o(.data) for g_sys_clk
    rtc.o(i.LT_RtcInit) refers to rtc.o(.data) for .data
    rtc.o(i.PMU_RTC_IRQHandler) refers to rtc.o(i.RTC_Get) for RTC_Get
    rtc.o(i.RTC_Get) refers to rtc_drv.o(i.DRV_RTC_GetTimeCounter) for DRV_RTC_GetTimeCounter
    rtc.o(i.RTC_Get) refers to rtc.o(i.Is_Leap_Year) for Is_Leap_Year
    rtc.o(i.RTC_Get) refers to rtc.o(i.RTC_Get_Week) for RTC_Get_Week
    rtc.o(i.RTC_Get) refers to rtc.o(.data) for .data
    rtc.o(i.RTC_Get) refers to rtc.o(.constdata) for .constdata
    rtc.o(i.RTC_Get_Week) refers to rtc.o(.constdata) for .constdata
    rtc.o(i.RTC_Set) refers to rtc.o(i.Is_Leap_Year) for Is_Leap_Year
    rtc.o(i.RTC_Set) refers to rtc_drv.o(i.DRV_RTC_SetTimeCounter) for DRV_RTC_SetTimeCounter
    rtc.o(i.RTC_Set) refers to rtc.o(.constdata) for .constdata
    dac.o(i.LT_PlayWav) refers to bsp.o(i.LT_ReadFlash) for LT_ReadFlash
    dac.o(i.LT_PlayWav) refers to dac.o(i.WAV_amplifier_EN) for WAV_amplifier_EN
    dac.o(i.LT_PlayWav) refers to dac.o(i.close_wav) for close_wav
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavState
    dac.o(i.LT_PlayWav) refers to data.o(.data) for wbuf0_Stat
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavFlashAddr
    dac.o(i.LT_PlayWav) refers to data.o(.data) for wbuf1_Stat
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gTempWavFlashAddr
    dac.o(i.LT_PlayWav) refers to data.o(.bss) for wavBuf0
    dac.o(i.LT_PlayWav) refers to data.o(.bss) for wavBuf1
    dac.o(i.LT_PlayWav) refers to data.o(.data) for wbuf_select
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavOpen
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavLen
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavAddrFull_Flag
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavFinish_Flag
    dac.o(i.LT_PlayWav) refers to data.o(.data) for gWavType
    dac.o(i.close_wav) refers to dac.o(i.WAV_amplifier_DIS) for WAV_amplifier_DIS
    dac.o(i.close_wav) refers to data.o(.data) for bufPos
    dac.o(i.close_wav) refers to data.o(.data) for gWavAddrFull_Flag
    dac.o(i.close_wav) refers to data.o(.data) for gWavFinish_Flag
    dac.o(i.close_wav) refers to data.o(.data) for gWavState
    dac.o(i.close_wav) refers to data.o(.data) for gWavFlag
    dac_wav.o(i.DMA2_IRQHandler) refers to dac_wav.o(i.DMA_Tran) for DMA_Tran
    dac_wav.o(i.DMA2_IRQHandler) refers to dma_drv.o(.data) for m_dma_control
    dac_wav.o(i.DMA2_IRQHandler) refers to dac_wav.o(.data) for .data
    dac_wav.o(i.DMA2_IRQHandler) refers to data.o(.data) for wbuf_select
    dac_wav.o(i.DMA2_IRQHandler) refers to dac_wav.o(.bss) for .bss
    dac_wav.o(i.DMA_DAC_Tran) refers to dma_drv.o(.bss) for m_dma_channel
    dac_wav.o(i.DMA_DAC_Tran) refers to dma_drv.o(.data) for m_dma_control
    dac_wav.o(i.DMA_REG_Init_my) refers to dma_drv.o(.data) for m_dma_control
    dac_wav.o(i.DMA_REG_Init_my) refers to dma_drv.o(.bss) for m_dma_channel
    dac_wav.o(i.DMA_Tran) refers to dac_wav.o(i.DMA_DAC_Tran) for DMA_DAC_Tran
    dac_wav.o(i.DMA_dis) refers to dma_drv.o(.bss) for m_dma_channel
    dac_wav.o(i.DMA_dis) refers to dma_drv.o(.data) for m_dma_control
    dac_wav.o(i.LT_PlayWav_DAC) refers to bsp.o(i.LT_ReadFlash) for LT_ReadFlash
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_drv.o(i.DRV_DAC_Init) for DRV_DAC_Init
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_wav.o(i.DMA_REG_Init_my) for DMA_REG_Init_my
    dac_wav.o(i.LT_PlayWav_DAC) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac.o(i.WAV_amplifier_EN) for WAV_amplifier_EN
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_wav.o(i.DMA_Tran) for DMA_Tran
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_wav.o(i.close_wav_dac) for close_wav_dac
    dac_wav.o(i.LT_PlayWav_DAC) refers to data.o(.data) for gWavState
    dac_wav.o(i.LT_PlayWav_DAC) refers to data.o(.data) for gWavFlashAddr
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_wav.o(.data) for .data
    dac_wav.o(i.LT_PlayWav_DAC) refers to data.o(.data) for wbuf_select
    dac_wav.o(i.LT_PlayWav_DAC) refers to dac_wav.o(.bss) for .bss
    dac_wav.o(i.LT_PlayWav_DAC) refers to cpm_drv.o(.data) for g_ips_clk
    dac_wav.o(i.LT_PlayWav_DAC) refers to data.o(.data) for gWavFlag
    dac_wav.o(i.close_wav_dac) refers to dac.o(i.WAV_amplifier_DIS) for WAV_amplifier_DIS
    dac_wav.o(i.close_wav_dac) refers to dac_wav.o(i.DMA_dis) for DMA_dis
    debug.o(i.DRV_CAN4_7_Handler) refers to can_drv.o(.data) for gCanIFlag1
    debug.o(i.DRV_CAN4_7_Handler) refers to debug.o(.data) for .data
    debug.o(i.DRV_CAN4_7_Handler) refers to debug.o(.bss) for .bss
    debug.o(i.DRV_CAN4_7_Handler) refers to bsp.o(.data) for ENDBYTE_Buf
    debug.o(i.DRV_CAN4_7_Handler) refers to can_drv.o(.bss) for gCantRxMsg
    debug.o(i.DRV_CAN4_7_Handler) refers to can_drv.o(.data) for canDataBuf
    debug.o(i.GETCHAR) refers to debug.o(.data) for .data
    debug.o(i.HandleUartEvent) refers to debug.o(i.UARTRecvByte) for UARTRecvByte
    debug.o(i.HandleUartEvent) refers to delay.o(i.DelayMS) for DelayMS
    debug.o(i.HandleUartEvent) refers to debug.o(i.configRtc) for configRtc
    debug.o(i.HandleUartEvent) refers to printf8.o(i.__0printf$8) for __2printf
    debug.o(i.HandleUartEvent) refers to debug.o(i.UARTRecieved) for UARTRecieved
    debug.o(i.HandleUartEvent) refers to debug.o(.data) for .data
    debug.o(i.HandleUartEvent) refers to debug.o(.bss) for .bss
    debug.o(i.LT_ClearRxBuf) refers to data.o(.bss) for gUsartRx
    debug.o(i.LT_DataToPc) refers to memseta.o(.text) for __aeabi_memclr4
    debug.o(i.LT_DataToPc) refers to bsp.o(i.Rx_CRC_CCITT) for Rx_CRC_CCITT
    debug.o(i.LT_DataToPc) refers to bsp.o(.data) for ENDBYTE_Buf
    debug.o(i.LT_DataToPc_NoFrame) refers to memseta.o(.text) for __aeabi_memclr4
    debug.o(i.LT_DataToPc_NoFrame) refers to bsp.o(i.Rx_CRC_CCITT) for Rx_CRC_CCITT
    debug.o(i.PUTCHAR) refers to debug.o(.data) for .data
    debug.o(i.PrintfBuf) refers to printf8.o(i.__0printf$8) for __2printf
    debug.o(i.UART1_IRQHandlerEvent) refers to pit.o(i.LT_UsartTimeDisable) for LT_UsartTimeDisable
    debug.o(i.UART1_IRQHandlerEvent) refers to pit.o(i.LT_UsartTimeSetCounter) for LT_UsartTimeSetCounter
    debug.o(i.UART1_IRQHandlerEvent) refers to bsp.o(.data) for FF_Update_Flag
    debug.o(i.UART1_IRQHandlerEvent) refers to data.o(.bss) for gUsartRx
    debug.o(i.UART1_IRQHandlerEvent) refers to debug.o(.data) for .data
    debug.o(i.UART1_IRQHandlerEvent) refers to debug.o(.bss) for .bss
    debug.o(i.UART1_IRQHandlerEvent) refers to bsp.o(.data) for ENDBYTE_Buf
    debug.o(i.UART1_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    debug.o(i.UART1_Init) refers to memseta.o(.text) for __aeabi_memclr
    debug.o(i.UART1_Init) refers to debug.o(.bss) for .bss
    debug.o(i.UARTRecieved) refers to debug.o(.bss) for .bss
    debug.o(i.UARTRecvByte) refers to debug.o(.bss) for .bss
    debug.o(i.UART_Debug_Init) refers to memseta.o(.text) for __aeabi_memclr
    debug.o(i.UART_Debug_Init) refers to debug.o(.data) for .data
    debug.o(i.UART_Debug_Init) refers to debug.o(.bss) for .bss
    debug.o(i.assert_failed) refers to printf8.o(i.__0printf$8) for __2printf
    debug.o(i.configRtc) refers to rtc_hal.o(i.HAL_RTC_Init) for HAL_RTC_Init
    debug.o(i.configRtc) refers to cpm_drv.o(.data) for g_sys_clk
    debug.o(i.configRtc) refers to debug.o(.data) for .data
    debug.o(i.fputc) refers to debug.o(.data) for .data
    delay.o(i.DelayMS) refers to cpm_drv.o(.data) for g_sys_clk
    delay.o(i.GetTickTime) refers to delay.o(.data) for .data
    delay.o(i.InitSysTick) refers to cpm_drv.o(.data) for g_core_clk
    delay.o(i.InitTickTime) refers to delay.o(.data) for .data
    delay.o(i.SysTick_Handler1) refers to delay.o(.data) for .data
    delay.o(i.SysTick_Handler1) refers to debug.o(.data) for uartCountDown
    i2c.o(i.CTI2C_read_byte) refers to i2c.o(i.SDA_INPUT) for SDA_INPUT
    i2c.o(i.CTI2C_read_byte) refers to i2c.o(i.CT_DELAY_US) for CT_DELAY_US
    i2c.o(i.CTI2C_read_byte) refers to i2c_hal.o(i.HAL_I2C_GPIOReadPin) for HAL_I2C_GPIOReadPin
    i2c.o(i.CTI2C_read_byte) refers to i2c.o(i.SDA_OUTPUT) for SDA_OUTPUT
    i2c.o(i.CTI2C_start) refers to i2c.o(i.SDA_OUTPUT) for SDA_OUTPUT
    i2c.o(i.CTI2C_start) refers to i2c.o(i.CT_DELAY_US) for CT_DELAY_US
    i2c.o(i.CTI2C_stop) refers to i2c.o(i.SDA_OUTPUT) for SDA_OUTPUT
    i2c.o(i.CTI2C_stop) refers to i2c.o(i.CT_DELAY_US) for CT_DELAY_US
    i2c.o(i.CTI2C_write_byte) refers to i2c.o(i.SDA_OUTPUT) for SDA_OUTPUT
    i2c.o(i.CTI2C_write_byte) refers to i2c.o(i.CT_DELAY_US) for CT_DELAY_US
    i2c.o(i.CTI2C_write_byte) refers to i2c.o(i.SDA_INPUT) for SDA_INPUT
    i2c.o(i.CTI2C_write_byte) refers to i2c_hal.o(i.HAL_I2C_GPIOReadPin) for HAL_I2C_GPIOReadPin
    i2c.o(i.CT_Read_Nbyte) refers to i2c.o(i.CTI2C_start) for CTI2C_start
    i2c.o(i.CT_Read_Nbyte) refers to i2c.o(i.CTI2C_write_byte) for CTI2C_write_byte
    i2c.o(i.CT_Read_Nbyte) refers to i2c.o(i.CTI2C_stop) for CTI2C_stop
    i2c.o(i.CT_Read_Nbyte) refers to i2c.o(i.CTI2C_read_byte) for CTI2C_read_byte
    i2c.o(i.CT_Write_Nbyte) refers to i2c.o(i.CTI2C_start) for CTI2C_start
    i2c.o(i.CT_Write_Nbyte) refers to i2c.o(i.CTI2C_write_byte) for CTI2C_write_byte
    i2c.o(i.CT_Write_Nbyte) refers to i2c.o(i.CTI2C_stop) for CTI2C_stop
    i2c.o(i.SCL_OUTPUT) refers to i2c_hal.o(i.HAL_I2C_GPIOInit) for HAL_I2C_GPIOInit
    i2c.o(i.SDA_INPUT) refers to i2c_hal.o(i.HAL_I2C_GPIOInit) for HAL_I2C_GPIOInit
    i2c.o(i.SDA_OUTPUT) refers to i2c_hal.o(i.HAL_I2C_GPIOInit) for HAL_I2C_GPIOInit
    pit.o(i.LT_UsartTimeSetCounter) refers to pit.o(i.LT_UsartTimeEnable) for LT_UsartTimeEnable
    pit.o(i.PIT1_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    pit.o(i.PIT1_Init_1) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dcmi_drv.o(i.DRV_DCMI_Getgray) refers to dcmi_drv.o(i.DRV_DCMI_Getgray_Edma) for DRV_DCMI_Getgray_Edma
    dcmi_drv.o(i.DRV_DCMI_Getgray) refers to dcmi_drv.o(i.DRV_DCMI_Getgray_Idma) for DRV_DCMI_Getgray_Idma
    dcmi_drv.o(i.DRV_DCMI_Getgray_Edma) refers to dcmi_drv.o(i.dma_register_init) for dma_register_init
    dcmi_drv.o(i.DRV_DCMI_Getgray_Edma) refers to dcmi_drv.o(i.dma_dcmi_xfer) for dma_dcmi_xfer
    dcmi_drv.o(i.DRV_DCMI_Getgray_Edma) refers to delay.o(i.delay) for delay
    dcmi_drv.o(i.DRV_DCMI_Getgray_Edma) refers to dcmi_drv.o(i.dma_wait_for_done) for dma_wait_for_done
    dcmi_drv.o(i.DRV_DCMI_Init) refers to dcmi_drv.o(i.dma_register_init) for dma_register_init
    dcmi_drv.o(i.DRV_DCMI_Init) refers to dcmi_drv.o(i.dma_dcmi_xfer_mcu_lcd) for dma_dcmi_xfer_mcu_lcd
    dcmi_drv.o(i.DRV_DCMI_Init) refers to sys.o(i.NVIC_Init) for NVIC_Init
    dcmi_drv.o(i.dma_dcmi_xfer) refers to dcmi_drv.o(.bss) for g_dma_lli
    dcmi_drv.o(i.dma_dcmi_xfer) refers to dcmi_drv.o(.data) for m_dma_control
    dcmi_drv.o(i.dma_dcmi_xfer_mcu_lcd) refers to dcmi_drv.o(.bss) for g_dma_lli
    dcmi_drv.o(i.dma_dcmi_xfer_mcu_lcd) refers to dcmi_drv.o(.data) for m_dma_control
    dcmi_drv.o(i.dma_register_init) refers to dcmi_drv.o(.data) for m_dma_control
    dcmi_drv.o(i.dma_register_init) refers to dcmi_drv.o(.bss) for m_dma_channel
    dcmi_drv.o(i.dma_wait_for_done) refers to dcmi_drv.o(.data) for m_dma_control
    lib_eflash.o(i.LIB_EFLASH_BulkProgram) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_ClrWritePermission) refers to lib_eflash.o(i.LIB_EFLASH_SetMainPermission) for LIB_EFLASH_SetMainPermission
    lib_eflash.o(i.LIB_EFLASH_Disboot) refers to lib_eflash.o(i.LIB_EFLASH_UpdateWord) for LIB_EFLASH_UpdateWord
    lib_eflash.o(i.LIB_EFLASH_Init) refers to lib_eflash.o(i.LIB_EFLASH_SetVerifyCnt) for LIB_EFLASH_SetVerifyCnt
    lib_eflash.o(i.LIB_EFLASH_Init) refers to lib_eflash.o(i.LIB_EFLASH_SetRWSC) for LIB_EFLASH_SetRWSC
    lib_eflash.o(i.LIB_EFLASH_Init) refers to lib_eflash.o(i.LIB_EFLASH_SetMainPermission) for LIB_EFLASH_SetMainPermission
    lib_eflash.o(i.LIB_EFLASH_Init) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_PageErase) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_RecoveryToBoot) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_SetWritePermission) refers to lib_eflash.o(i.LIB_EFLASH_SetMainPermission) for LIB_EFLASH_SetMainPermission
    lib_eflash.o(i.LIB_EFLASH_UpdateWord) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_UpdateWord_CHIPMODE) refers to lib_eflash.o(.bss) for eflash_ops
    lib_eflash.o(i.LIB_EFLASH_WordProg) refers to lib_eflash.o(i.LIB_EFLASH_BulkProgram) for LIB_EFLASH_BulkProgram
    lib_eflash.o(i.LIB_EFlash_Chip_Mode) refers to lib_eflash.o(i.LIB_EFLASH_UpdateWord_CHIPMODE) for LIB_EFLASH_UpdateWord_CHIPMODE
    event_groups.o(i.vEventGroupClearBitsCallback) refers to event_groups.o(i.xEventGroupClearBits) for xEventGroupClearBits
    event_groups.o(i.vEventGroupDelete) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    event_groups.o(i.vEventGroupDelete) refers to tasks.o(i.vTaskRemoveFromUnorderedEventList) for vTaskRemoveFromUnorderedEventList
    event_groups.o(i.vEventGroupDelete) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    event_groups.o(i.vEventGroupSetBitsCallback) refers to event_groups.o(i.xEventGroupSetBits) for xEventGroupSetBits
    event_groups.o(i.xEventGroupClearBits) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    event_groups.o(i.xEventGroupClearBits) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    event_groups.o(i.xEventGroupCreateStatic) refers to list.o(i.vListInitialise) for vListInitialise
    event_groups.o(i.xEventGroupSetBits) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    event_groups.o(i.xEventGroupSetBits) refers to tasks.o(i.vTaskRemoveFromUnorderedEventList) for vTaskRemoveFromUnorderedEventList
    event_groups.o(i.xEventGroupSetBits) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    event_groups.o(i.xEventGroupSync) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    event_groups.o(i.xEventGroupSync) refers to event_groups.o(i.xEventGroupSetBits) for xEventGroupSetBits
    event_groups.o(i.xEventGroupSync) refers to tasks.o(i.vTaskPlaceOnUnorderedEventList) for vTaskPlaceOnUnorderedEventList
    event_groups.o(i.xEventGroupSync) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    event_groups.o(i.xEventGroupSync) refers to tasks.o(i.uxTaskResetEventItemValue) for uxTaskResetEventItemValue
    event_groups.o(i.xEventGroupSync) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    event_groups.o(i.xEventGroupSync) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    event_groups.o(i.xEventGroupWaitBits) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    event_groups.o(i.xEventGroupWaitBits) refers to event_groups.o(i.prvTestWaitCondition) for prvTestWaitCondition
    event_groups.o(i.xEventGroupWaitBits) refers to tasks.o(i.vTaskPlaceOnUnorderedEventList) for vTaskPlaceOnUnorderedEventList
    event_groups.o(i.xEventGroupWaitBits) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    event_groups.o(i.xEventGroupWaitBits) refers to tasks.o(i.uxTaskResetEventItemValue) for uxTaskResetEventItemValue
    event_groups.o(i.xEventGroupWaitBits) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    event_groups.o(i.xEventGroupWaitBits) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.prvCopyDataFromQueue) refers to memcpya.o(.text) for __aeabi_memcpy
    queue.o(i.prvCopyDataToQueue) refers to tasks.o(i.xTaskPriorityDisinherit) for xTaskPriorityDisinherit
    queue.o(i.prvCopyDataToQueue) refers to memcpya.o(.text) for __aeabi_memcpy
    queue.o(i.prvInitialiseMutex) refers to queue.o(i.xQueueGenericSend) for xQueueGenericSend
    queue.o(i.prvInitialiseNewQueue) refers to queue.o(i.xQueueGenericReset) for xQueueGenericReset
    queue.o(i.prvIsQueueEmpty) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.prvIsQueueEmpty) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.prvIsQueueFull) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.prvIsQueueFull) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.prvUnlockQueue) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.prvUnlockQueue) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.prvUnlockQueue) refers to tasks.o(i.vTaskMissedYield) for vTaskMissedYield
    queue.o(i.prvUnlockQueue) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.uxQueueMessagesWaiting) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.uxQueueMessagesWaiting) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.uxQueueSpacesAvailable) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.uxQueueSpacesAvailable) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueueCreateMutexStatic) refers to queue.o(i.xQueueGenericCreateStatic) for xQueueGenericCreateStatic
    queue.o(i.xQueueCreateMutexStatic) refers to queue.o(i.prvInitialiseMutex) for prvInitialiseMutex
    queue.o(i.xQueueGenericCreateStatic) refers to queue.o(i.prvInitialiseNewQueue) for prvInitialiseNewQueue
    queue.o(i.xQueueGenericReset) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.xQueueGenericReset) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueGenericReset) refers to list.o(i.vListInitialise) for vListInitialise
    queue.o(i.xQueueGenericReset) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueueGenericSend) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.xQueueGenericSend) refers to queue.o(i.prvCopyDataToQueue) for prvCopyDataToQueue
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueGenericSend) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.vTaskInternalSetTimeOutState) for vTaskInternalSetTimeOutState
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.xTaskCheckForTimeOut) for xTaskCheckForTimeOut
    queue.o(i.xQueueGenericSend) refers to queue.o(i.prvIsQueueFull) for prvIsQueueFull
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.vTaskPlaceOnEventList) for vTaskPlaceOnEventList
    queue.o(i.xQueueGenericSend) refers to queue.o(i.prvUnlockQueue) for prvUnlockQueue
    queue.o(i.xQueueGenericSend) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    queue.o(i.xQueueGenericSendFromISR) refers to queue.o(i.prvCopyDataToQueue) for prvCopyDataToQueue
    queue.o(i.xQueueGenericSendFromISR) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueGiveFromISR) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueuePeek) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.xQueuePeek) refers to queue.o(i.prvCopyDataFromQueue) for prvCopyDataFromQueue
    queue.o(i.xQueuePeek) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueuePeek) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueuePeek) refers to tasks.o(i.vTaskInternalSetTimeOutState) for vTaskInternalSetTimeOutState
    queue.o(i.xQueuePeek) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    queue.o(i.xQueuePeek) refers to tasks.o(i.xTaskCheckForTimeOut) for xTaskCheckForTimeOut
    queue.o(i.xQueuePeek) refers to queue.o(i.prvIsQueueEmpty) for prvIsQueueEmpty
    queue.o(i.xQueuePeek) refers to tasks.o(i.vTaskPlaceOnEventList) for vTaskPlaceOnEventList
    queue.o(i.xQueuePeek) refers to queue.o(i.prvUnlockQueue) for prvUnlockQueue
    queue.o(i.xQueuePeek) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    queue.o(i.xQueuePeekFromISR) refers to queue.o(i.prvCopyDataFromQueue) for prvCopyDataFromQueue
    queue.o(i.xQueueReceive) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.xQueueReceive) refers to queue.o(i.prvCopyDataFromQueue) for prvCopyDataFromQueue
    queue.o(i.xQueueReceive) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueReceive) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueueReceive) refers to tasks.o(i.vTaskInternalSetTimeOutState) for vTaskInternalSetTimeOutState
    queue.o(i.xQueueReceive) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    queue.o(i.xQueueReceive) refers to tasks.o(i.xTaskCheckForTimeOut) for xTaskCheckForTimeOut
    queue.o(i.xQueueReceive) refers to queue.o(i.prvIsQueueEmpty) for prvIsQueueEmpty
    queue.o(i.xQueueReceive) refers to tasks.o(i.vTaskPlaceOnEventList) for vTaskPlaceOnEventList
    queue.o(i.xQueueReceive) refers to queue.o(i.prvUnlockQueue) for prvUnlockQueue
    queue.o(i.xQueueReceive) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    queue.o(i.xQueueReceiveFromISR) refers to queue.o(i.prvCopyDataFromQueue) for prvCopyDataFromQueue
    queue.o(i.xQueueReceiveFromISR) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueSemaphoreTake) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.pvTaskIncrementMutexHeldCount) for pvTaskIncrementMutexHeldCount
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.xTaskRemoveFromEventList) for xTaskRemoveFromEventList
    queue.o(i.xQueueSemaphoreTake) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.vTaskInternalSetTimeOutState) for vTaskInternalSetTimeOutState
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.xTaskCheckForTimeOut) for xTaskCheckForTimeOut
    queue.o(i.xQueueSemaphoreTake) refers to queue.o(i.prvIsQueueEmpty) for prvIsQueueEmpty
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.xTaskPriorityInherit) for xTaskPriorityInherit
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.vTaskPlaceOnEventList) for vTaskPlaceOnEventList
    queue.o(i.xQueueSemaphoreTake) refers to queue.o(i.prvUnlockQueue) for prvUnlockQueue
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    queue.o(i.xQueueSemaphoreTake) refers to queue.o(i.prvGetDisinheritPriorityAfterTimeout) for prvGetDisinheritPriorityAfterTimeout
    queue.o(i.xQueueSemaphoreTake) refers to tasks.o(i.vTaskPriorityDisinheritAfterTimeout) for vTaskPriorityDisinheritAfterTimeout
    tasks.o(i.pcTaskGetName) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.prvAddCurrentTaskToDelayedList) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.prvAddCurrentTaskToDelayedList) refers to list.o(i.vListInsert) for vListInsert
    tasks.o(i.prvAddCurrentTaskToDelayedList) refers to tasks.o(.data) for xTickCount
    tasks.o(i.prvAddCurrentTaskToDelayedList) refers to tasks.o(.bss) for xSuspendedTaskList
    tasks.o(i.prvAddNewTaskToReadyList) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.prvAddNewTaskToReadyList) refers to tasks.o(i.prvInitialiseTaskLists) for prvInitialiseTaskLists
    tasks.o(i.prvAddNewTaskToReadyList) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.prvAddNewTaskToReadyList) refers to tasks.o(.data) for uxCurrentNumberOfTasks
    tasks.o(i.prvAddNewTaskToReadyList) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.prvCheckTasksWaitingTermination) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.prvCheckTasksWaitingTermination) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.prvCheckTasksWaitingTermination) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.prvCheckTasksWaitingTermination) refers to tasks.o(i.prvDeleteTCB) for prvDeleteTCB
    tasks.o(i.prvCheckTasksWaitingTermination) refers to tasks.o(.bss) for xTasksWaitingTermination
    tasks.o(i.prvCheckTasksWaitingTermination) refers to tasks.o(.data) for uxCurrentNumberOfTasks
    tasks.o(i.prvIdleTask) refers to tasks.o(i.prvCheckTasksWaitingTermination) for prvCheckTasksWaitingTermination
    tasks.o(i.prvIdleTask) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.prvInitialiseNewTask) refers to list.o(i.vListInitialiseItem) for vListInitialiseItem
    tasks.o(i.prvInitialiseNewTask) refers to port.o(i.pxPortInitialiseStack) for pxPortInitialiseStack
    tasks.o(i.prvInitialiseTaskLists) refers to list.o(i.vListInitialise) for vListInitialise
    tasks.o(i.prvInitialiseTaskLists) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.prvInitialiseTaskLists) refers to tasks.o(.data) for pxDelayedTaskList
    tasks.o(i.prvResetNextTaskUnblockTime) refers to tasks.o(.data) for pxDelayedTaskList
    tasks.o(i.prvTaskIsTaskSuspended) refers to tasks.o(.bss) for xSuspendedTaskList
    tasks.o(i.pvTaskIncrementMutexHeldCount) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.ulTaskGenericNotifyTake) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.ulTaskGenericNotifyTake) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.ulTaskGenericNotifyTake) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.ulTaskGenericNotifyTake) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.ulTaskGenericNotifyValueClear) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.ulTaskGenericNotifyValueClear) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.ulTaskGenericNotifyValueClear) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.uxTaskGetNumberOfTasks) refers to tasks.o(.data) for uxCurrentNumberOfTasks
    tasks.o(i.uxTaskPriorityGet) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.uxTaskPriorityGet) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.uxTaskPriorityGet) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.uxTaskPriorityGetFromISR) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.uxTaskResetEventItemValue) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskDelay) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    tasks.o(i.vTaskDelay) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.vTaskDelay) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    tasks.o(i.vTaskDelete) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.vTaskDelete) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.vTaskDelete) refers to list.o(i.vListInsertEnd) for vListInsertEnd
    tasks.o(i.vTaskDelete) refers to tasks.o(i.prvResetNextTaskUnblockTime) for prvResetNextTaskUnblockTime
    tasks.o(i.vTaskDelete) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.vTaskDelete) refers to tasks.o(i.prvDeleteTCB) for prvDeleteTCB
    tasks.o(i.vTaskDelete) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskDelete) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskEndScheduler) refers to port.o(i.vPortEndScheduler) for vPortEndScheduler
    tasks.o(i.vTaskEndScheduler) refers to tasks.o(.data) for xSchedulerRunning
    tasks.o(i.vTaskGenericNotifyGiveFromISR) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.vTaskGenericNotifyGiveFromISR) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskInternalSetTimeOutState) refers to tasks.o(.data) for xNumOfOverflows
    tasks.o(i.vTaskMissedYield) refers to tasks.o(.data) for xYieldPending
    tasks.o(i.vTaskPlaceOnEventList) refers to list.o(i.vListInsert) for vListInsert
    tasks.o(i.vTaskPlaceOnEventList) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.vTaskPlaceOnEventList) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskPlaceOnUnorderedEventList) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.vTaskPlaceOnUnorderedEventList) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskPriorityDisinheritAfterTimeout) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.vTaskPriorityDisinheritAfterTimeout) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskPriorityDisinheritAfterTimeout) refers to tasks.o(.data) for uxTopReadyPriority
    tasks.o(i.vTaskPrioritySet) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.vTaskPrioritySet) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.vTaskPrioritySet) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.vTaskPrioritySet) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskPrioritySet) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskRemoveFromUnorderedEventList) refers to tasks.o(.data) for uxTopReadyPriority
    tasks.o(i.vTaskRemoveFromUnorderedEventList) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskResume) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.vTaskResume) refers to tasks.o(i.prvTaskIsTaskSuspended) for prvTaskIsTaskSuspended
    tasks.o(i.vTaskResume) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.vTaskResume) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.vTaskResume) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskResume) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskSetTimeOutState) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.vTaskSetTimeOutState) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.vTaskSetTimeOutState) refers to tasks.o(.data) for xNumOfOverflows
    tasks.o(i.vTaskStartScheduler) refers to main.o(i.vApplicationGetIdleTaskMemory) for vApplicationGetIdleTaskMemory
    tasks.o(i.vTaskStartScheduler) refers to tasks.o(i.xTaskCreateStatic) for xTaskCreateStatic
    tasks.o(i.vTaskStartScheduler) refers to port.o(i.xPortStartScheduler) for xPortStartScheduler
    tasks.o(i.vTaskStartScheduler) refers to tasks.o(i.prvIdleTask) for prvIdleTask
    tasks.o(i.vTaskStartScheduler) refers to tasks.o(.data) for xIdleTaskHandle
    tasks.o(i.vTaskSuspend) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.vTaskSuspend) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.vTaskSuspend) refers to list.o(i.vListInsertEnd) for vListInsertEnd
    tasks.o(i.vTaskSuspend) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.vTaskSuspend) refers to tasks.o(i.prvResetNextTaskUnblockTime) for prvResetNextTaskUnblockTime
    tasks.o(i.vTaskSuspend) refers to tasks.o(i.vTaskSwitchContext) for vTaskSwitchContext
    tasks.o(i.vTaskSuspend) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.vTaskSuspend) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.vTaskSuspendAll) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.vTaskSwitchContext) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.vTaskSwitchContext) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskCatchUpTicks) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    tasks.o(i.xTaskCatchUpTicks) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    tasks.o(i.xTaskCatchUpTicks) refers to tasks.o(.data) for xPendedTicks
    tasks.o(i.xTaskCheckForTimeOut) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.xTaskCheckForTimeOut) refers to tasks.o(i.vTaskInternalSetTimeOutState) for vTaskInternalSetTimeOutState
    tasks.o(i.xTaskCheckForTimeOut) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.xTaskCheckForTimeOut) refers to tasks.o(.data) for xTickCount
    tasks.o(i.xTaskCreateStatic) refers to tasks.o(i.prvInitialiseNewTask) for prvInitialiseNewTask
    tasks.o(i.xTaskCreateStatic) refers to tasks.o(i.prvAddNewTaskToReadyList) for prvAddNewTaskToReadyList
    tasks.o(i.xTaskDelayUntil) refers to tasks.o(i.vTaskSuspendAll) for vTaskSuspendAll
    tasks.o(i.xTaskDelayUntil) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.xTaskDelayUntil) refers to tasks.o(i.xTaskResumeAll) for xTaskResumeAll
    tasks.o(i.xTaskDelayUntil) refers to tasks.o(.data) for xTickCount
    tasks.o(i.xTaskGenericNotify) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.xTaskGenericNotify) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.xTaskGenericNotify) refers to tasks.o(.data) for uxTopReadyPriority
    tasks.o(i.xTaskGenericNotify) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskGenericNotifyFromISR) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.xTaskGenericNotifyFromISR) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskGenericNotifyStateClear) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.xTaskGenericNotifyStateClear) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.xTaskGenericNotifyStateClear) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.xTaskGenericNotifyWait) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.xTaskGenericNotifyWait) refers to tasks.o(i.prvAddCurrentTaskToDelayedList) for prvAddCurrentTaskToDelayedList
    tasks.o(i.xTaskGenericNotifyWait) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.xTaskGenericNotifyWait) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.xTaskGetCurrentTaskHandle) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.xTaskGetTickCount) refers to tasks.o(.data) for xTickCount
    tasks.o(i.xTaskGetTickCountFromISR) refers to tasks.o(.data) for xTickCount
    tasks.o(i.xTaskIncrementTick) refers to tasks.o(i.prvResetNextTaskUnblockTime) for prvResetNextTaskUnblockTime
    tasks.o(i.xTaskIncrementTick) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.xTaskIncrementTick) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskPriorityDisinherit) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.xTaskPriorityDisinherit) refers to tasks.o(.data) for uxTopReadyPriority
    tasks.o(i.xTaskPriorityDisinherit) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskPriorityInherit) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.xTaskPriorityInherit) refers to tasks.o(.data) for pxCurrentTCB
    tasks.o(i.xTaskPriorityInherit) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskRemoveFromEventList) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.xTaskRemoveFromEventList) refers to tasks.o(.bss) for pxReadyTasksLists
    tasks.o(i.xTaskResumeAll) refers to port.o(i.vPortEnterCritical) for vPortEnterCritical
    tasks.o(i.xTaskResumeAll) refers to tasks.o(i.prvResetNextTaskUnblockTime) for prvResetNextTaskUnblockTime
    tasks.o(i.xTaskResumeAll) refers to tasks.o(i.xTaskIncrementTick) for xTaskIncrementTick
    tasks.o(i.xTaskResumeAll) refers to port.o(i.vPortExitCritical) for vPortExitCritical
    tasks.o(i.xTaskResumeAll) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.xTaskResumeAll) refers to tasks.o(.bss) for xPendingReadyList
    tasks.o(i.xTaskResumeFromISR) refers to tasks.o(i.prvTaskIsTaskSuspended) for prvTaskIsTaskSuspended
    tasks.o(i.xTaskResumeFromISR) refers to list.o(i.uxListRemove) for uxListRemove
    tasks.o(i.xTaskResumeFromISR) refers to list.o(i.vListInsertEnd) for vListInsertEnd
    tasks.o(i.xTaskResumeFromISR) refers to tasks.o(.data) for uxSchedulerSuspended
    tasks.o(i.xTaskResumeFromISR) refers to tasks.o(.bss) for pxReadyTasksLists
    port.o(.emb_text) refers to tasks.o(i.vTaskSwitchContext) for vTaskSwitchContext
    port.o(.emb_text) refers to tasks.o(.data) for pxCurrentTCB
    port.o(i.SysTick_Handler) refers to tasks.o(i.xTaskIncrementTick) for xTaskIncrementTick
    port.o(i.pxPortInitialiseStack) refers to port.o(i.prvTaskExitError) for prvTaskExitError
    port.o(i.vPortEnterCritical) refers to port.o(.data) for uxCriticalNesting
    port.o(i.vPortExitCritical) refers to port.o(.data) for uxCriticalNesting
    port.o(i.xPortStartScheduler) refers to port.o(i.vPortSetupTimerInterrupt) for vPortSetupTimerInterrupt
    port.o(i.xPortStartScheduler) refers to port.o(.emb_text) for __asm___6_port_c_39a90d8d__prvEnableVFP
    port.o(i.xPortStartScheduler) refers to port.o(.data) for uxCriticalNesting
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to debug.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to debug.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to debug.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to debug.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to debug.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to debug.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to debug.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to debug.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to debug.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to debug.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to debug.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to debug.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to debug.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to debug.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to debug.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to debug.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to debug.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to debug.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to debug.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to debug.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to debug.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to debug.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to debug.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to debug.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to debug.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to debug.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to debug.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to debug.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to debug.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to debug.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to debug.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to debug.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to debug.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to debug.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to debug.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to debug.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to debug.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to debug.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to debug.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to debug.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to debug.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to debug.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to debug.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to debug.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to debug.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to debug.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to debug.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to debug.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to debug.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to debug.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to debug.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to debug.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to debug.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to debug.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to debug.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to debug.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to debug.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to debug.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to debug.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to debug.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to debug.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to debug.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to debug.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to debug.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to debug.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to debug.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_armcm4.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_armcm4.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing main.o(i.HAL_IncTick), (16 bytes).
    Removing main.o(.data), (40 bytes).
    Removing bsp.o(.rev16_text), (4 bytes).
    Removing bsp.o(.revsh_text), (4 bytes).
    Removing bsp.o(.rrx_text), (6 bytes).
    Removing bsp.o(i.Active_Window_WH), (2 bytes).
    Removing bsp.o(i.Active_Window_XY), (2 bytes).
    Removing bsp.o(i.Canvas_Image_Start_address), (12 bytes).
    Removing bsp.o(i.DMAC_M2MTest2), (48 bytes).
    Removing bsp.o(i.DMAC_M2MTest3), (36 bytes).
    Removing bsp.o(i.LT768_BTE_Init), (68 bytes).
    Removing bsp.o(i.LT_ReadFlash), (20 bytes).
    Removing bsp.o(i.Main_Image_Start_Address), (2 bytes).
    Removing bsp.o(i.Main_Image_Width), (2 bytes).
    Removing bsp.o(i.Main_Window_Start_XY), (2 bytes).
    Removing bsp.o(i.Rx_CRC_CCITT), (56 bytes).
    Removing bsp.o(.bss), (72 bytes).
    Removing bsp.o(.data), (1 bytes).
    Removing bsp.o(.data), (1 bytes).
    Removing adc_drv.o(.rev16_text), (4 bytes).
    Removing adc_drv.o(.revsh_text), (4 bytes).
    Removing adc_drv.o(.rrx_text), (6 bytes).
    Removing adc_drv.o(i.DRV_ADC_ChannelSel), (12 bytes).
    Removing adc_drv.o(i.DRV_ADC_ConvStart), (16 bytes).
    Removing adc_drv.o(i.DRV_ADC_ConvStop), (28 bytes).
    Removing adc_drv.o(i.DRV_ADC_IRQHandler), (16 bytes).
    Removing adc_drv.o(i.DRV_ADC_ModuleDis), (24 bytes).
    Removing adc_drv.o(i.DRV_ADC_ModuleEn), (24 bytes).
    Removing cache_drv.o(.rev16_text), (4 bytes).
    Removing cache_drv.o(.revsh_text), (4 bytes).
    Removing cache_drv.o(.rrx_text), (6 bytes).
    Removing cache_drv.o(i.DRV_DCACHE_Syn), (24 bytes).
    Removing cache_drv.o(i.DRV_ICACHE_Syn), (24 bytes).
    Removing can_drv.o(.rev16_text), (4 bytes).
    Removing can_drv.o(.revsh_text), (4 bytes).
    Removing can_drv.o(.rrx_text), (6 bytes).
    Removing can_drv.o(i.CanRecieved), (24 bytes).
    Removing can_drv.o(i.CanRecvByte), (44 bytes).
    Removing can_drv.o(i.DRV_CAN0_3_Handler), (104 bytes).
    Removing can_drv.o(i.DRV_CAN12_15_Handler), (104 bytes).
    Removing can_drv.o(i.DRV_CAN16_31_Handler), (104 bytes).
    Removing can_drv.o(i.DRV_CAN32_63_Handler), (100 bytes).
    Removing can_drv.o(i.DRV_CAN8_11_Handler), (104 bytes).
    Removing can_drv.o(i.DRV_CAN_DeInit), (84 bytes).
    Removing can_drv.o(i.DRV_CAN_FIFO_ReceiveBytes), (200 bytes).
    Removing can_drv.o(i.DRV_CAN_FIFO_ReceiveBytesIT), (132 bytes).
    Removing can_drv.o(i.DRV_CAN_FuncSwap), (32 bytes).
    Removing can_drv.o(i.DRV_CAN_Init), (320 bytes).
    Removing can_drv.o(i.DRV_CAN_ReceiveBytes), (236 bytes).
    Removing can_drv.o(i.DRV_CAN_ReceiveBytesIT), (268 bytes).
    Removing can_drv.o(i.DRV_CAN_SoftReset), (18 bytes).
    Removing can_drv.o(i.DRV_CAN_TransmitBytes), (174 bytes).
    Removing can_drv.o(i.DRV_CAN_TransmitBytesIT), (188 bytes).
    Removing can_drv.o(.bss), (372 bytes).
    Removing can_drv.o(.data), (4 bytes).
    Removing cpm_drv.o(.rev16_text), (4 bytes).
    Removing cpm_drv.o(.revsh_text), (4 bytes).
    Removing cpm_drv.o(.rrx_text), (6 bytes).
    Removing cpm_drv.o(i.DRV_CPM_GetEFMClHz), (12 bytes).
    Removing cpm_drv.o(i.DRV_CPM_ModuleClkOff), (90 bytes).
    Removing cpm_drv.o(i.DRV_CPM_ModuleClkOn), (90 bytes).
    Removing cpm_drv.o(i.DRV_CPM_PorReset), (20 bytes).
    Removing cpm_drv.o(i.DRV_CPM_SetSDHostClkDiv), (34 bytes).
    Removing cpm_drv.o(i.DRV_CPM_SystemClkVrefTrim), (48 bytes).
    Removing cpm_drv.o(i.DRV_CPM_UsbPhyInit), (168 bytes).
    Removing cpm_drv.o(i.DRV_CPM_VccCoreTestModeKeySet), (32 bytes).
    Removing cpm_drv.o(i.DRV_CPM_VccCoreTestModeSet), (28 bytes).
    Removing cpm_drv.o(.data), (4 bytes).
    Removing cpm_drv.o(.data), (4 bytes).
    Removing dac_drv.o(.rev16_text), (4 bytes).
    Removing dac_drv.o(.revsh_text), (4 bytes).
    Removing dac_drv.o(.rrx_text), (6 bytes).
    Removing dac_drv.o(i.DRV_DAC_Deinit), (24 bytes).
    Removing dac_drv.o(i.DRV_DAC_GetData), (20 bytes).
    Removing dac_drv.o(i.DRV_DAC_Init), (104 bytes).
    Removing dac_drv.o(i.DRV_DAC_SW_Trig), (24 bytes).
    Removing dac_drv.o(i.DRV_DAC_SendData), (12 bytes).
    Removing dma_drv.o(.rev16_text), (4 bytes).
    Removing dma_drv.o(.revsh_text), (4 bytes).
    Removing dma_drv.o(.rrx_text), (6 bytes).
    Removing dma_drv.o(i.DMA_REG_Init), (20 bytes).
    Removing dma_drv.o(i.DRV_DMAC_ClearRawStatus), (10 bytes).
    Removing dma_drv.o(i.DRV_DMAC_ClrTrfFlag), (10 bytes).
    Removing dma_drv.o(i.DRV_DMAC_CtrlRegConfig), (98 bytes).
    Removing dma_drv.o(i.DRV_DMAC_DisTfrIt), (20 bytes).
    Removing dma_drv.o(i.DRV_DMAC_GetRawStatus), (16 bytes).
    Removing dma_drv.o(i.DRV_DMAC_LliRegInit), (36 bytes).
    Removing dma_drv.o(i.clear_dma_flag), (48 bytes).
    Removing dma_drv.o(i.dma_ssi_m2p_start), (232 bytes).
    Removing dma_drv.o(i.dma_ssi_p2m_lli_start), (348 bytes).
    Removing dma_drv.o(i.dma_ssi_wait), (64 bytes).
    Removing dma_drv.o(i.get_dma_flag), (44 bytes).
    Removing dma_drv.o(.bss), (476 bytes).
    Removing dma2d_drv.o(.rev16_text), (4 bytes).
    Removing dma2d_drv.o(.revsh_text), (4 bytes).
    Removing dma2d_drv.o(.rrx_text), (6 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_BgClutLoad), (44 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_BlendHard), (192 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_ClutInit), (28 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_FgClutLoad), (42 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_Mem2Mem), (164 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_PfcHard), (168 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_Reg2Mem), (160 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_SetAlphaCmp), (18 bytes).
    Removing dma2d_drv.o(i.DRV_DMA2D_SoftReset), (24 bytes).
    Removing edma_drv.o(.rev16_text), (4 bytes).
    Removing edma_drv.o(.revsh_text), (4 bytes).
    Removing edma_drv.o(.rrx_text), (6 bytes).
    Removing edma_drv.o(i.DRV_EDMAC_CtrlRegConfig), (46 bytes).
    Removing edma_drv.o(i.DRV_EDMAC_ResetReg), (14 bytes).
    Removing edma_drv.o(i.DRV_EDMAC_WriteAndReadBufferAdderAddConfig), (34 bytes).
    Removing eflash_drv.o(.rev16_text), (4 bytes).
    Removing eflash_drv.o(.revsh_text), (4 bytes).
    Removing eflash_drv.o(.rrx_text), (6 bytes).
    Removing eflash_drv.o(i.DRV_EFLASH_SetWritePermission), (4 bytes).
    Removing eflash_drv.o(i.DRV_EFM_EreasePage), (4 bytes).
    Removing eflash_drv.o(i.DRV_EFM_MainCmd), (20 bytes).
    Removing eflash_drv.o(i.DRV_EFM_ProgramBulk), (10 bytes).
    Removing eflash_drv.o(i.DRV_EFM_ProgramWord), (12 bytes).
    Removing eflash_drv.o(i.DRV_EFM_Read), (18 bytes).
    Removing eflash_drv.o(i.DRV_EFM_ReadCmd), (24 bytes).
    Removing eflash_drv.o(i.DRV_EFM_WriteCmd), (24 bytes).
    Removing eport_drv.o(.rev16_text), (4 bytes).
    Removing eport_drv.o(.revsh_text), (4 bytes).
    Removing eport_drv.o(.rrx_text), (6 bytes).
    Removing eport_drv.o(i.DRV_EPORT_IRQHandler), (1324 bytes).
    Removing eport_drv.o(i.DRV_EPORT_ReadITFlag), (6 bytes).
    Removing eport_drv.o(i.DRV_EPORT_ReadPinsLevel), (6 bytes).
    Removing eport_drv.o(i.DRV_EPORT_SetDirection), (20 bytes).
    Removing eport_drv.o(i.DRV_EPORT_SetOpenDrain), (20 bytes).
    Removing eport_drv.o(i.DRV_EPORT_SetPullUp), (20 bytes).
    Removing eport_drv.o(i.DRV_EPORT_WritePinsLevel), (20 bytes).
    Removing i2c_drv.o(.rev16_text), (4 bytes).
    Removing i2c_drv.o(.revsh_text), (4 bytes).
    Removing i2c_drv.o(.rrx_text), (6 bytes).
    Removing i2c_drv.o(i.DRV_I2C_Cmd), (20 bytes).
    Removing i2c_drv.o(i.DRV_I2C_DeInit), (8 bytes).
    Removing i2c_drv.o(i.DRV_I2C_GetDR), (6 bytes).
    Removing i2c_drv.o(i.DRV_I2C_GetFlag), (18 bytes).
    Removing i2c_drv.o(i.DRV_I2C_GetItFlags), (12 bytes).
    Removing i2c_drv.o(i.DRV_I2C_GetItSource), (46 bytes).
    Removing i2c_drv.o(i.DRV_I2C_GpioDeInit), (30 bytes).
    Removing i2c_drv.o(i.DRV_I2C_Init), (92 bytes).
    Removing i2c_drv.o(i.DRV_I2C_ItCmd), (16 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterGenerateStop), (34 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterGenerateStopV1), (120 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterGenerateStopV2), (124 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterHighspeedWriteRequest), (118 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterReadRequest), (54 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterRestartReadRequest), (32 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MasterWriteRequest), (54 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MemRead), (264 bytes).
    Removing i2c_drv.o(i.DRV_I2C_MemWrite), (162 bytes).
    Removing i2c_drv.o(i.DRV_I2C_Receive), (148 bytes).
    Removing i2c_drv.o(i.DRV_I2C_ReceiveByte), (26 bytes).
    Removing i2c_drv.o(i.DRV_I2C_ReceiveIT), (50 bytes).
    Removing i2c_drv.o(i.DRV_I2C_SetDR), (4 bytes).
    Removing i2c_drv.o(i.DRV_I2C_SlaveReceive), (88 bytes).
    Removing i2c_drv.o(i.DRV_I2C_SlaveTransmit), (78 bytes).
    Removing i2c_drv.o(i.DRV_I2C_SlaveTransmitReceive), (78 bytes).
    Removing i2c_drv.o(i.DRV_I2C_Stop), (26 bytes).
    Removing i2c_drv.o(i.DRV_I2C_TogglePin), (12 bytes).
    Removing i2c_drv.o(i.DRV_I2C_Transmit), (74 bytes).
    Removing i2c_drv.o(i.DRV_I2C_TransmitByte), (12 bytes).
    Removing i2c_drv.o(i.DRV_I2C_TransmitIT), (46 bytes).
    Removing i2c_drv.o(i.DRV_I2C_WaitonFlagTimeout), (152 bytes).
    Removing i2c_drv.o(i.DRV_I2C_WaitonSlvHsFlagTimeout), (48 bytes).
    Removing i2c_drv.o(i.DRV_I2C_WritePin), (18 bytes).
    Removing interrupt.o(.rev16_text), (4 bytes).
    Removing interrupt.o(.revsh_text), (4 bytes).
    Removing interrupt.o(.rrx_text), (6 bytes).
    Removing interrupt.o(i.Access_Error), (60 bytes).
    Removing interrupt.o(i.Breakpoint_Exception), (60 bytes).
    Removing interrupt.o(i.CLCD_IRQHandler), (2 bytes).
    Removing interrupt.o(i.DummyHandler), (60 bytes).
    Removing interrupt.o(i.Illegal_Instrn), (64 bytes).
    Removing interrupt.o(i.Misaligned_Access), (64 bytes).
    Removing interrupt.o(i.OperationalLogic_Error), (72 bytes).
    Removing interrupt.o(i.SysTick_Handler3), (16 bytes).
    Removing interrupt.o(i.USI1_IRQHandler), (2 bytes).
    Removing interrupt.o(i.Unrecoverable_Error), (68 bytes).
    Removing interrupt.o(.data), (4 bytes).
    Removing ioctrl_drv.o(.rev16_text), (4 bytes).
    Removing ioctrl_drv.o(.revsh_text), (4 bytes).
    Removing ioctrl_drv.o(.rrx_text), (6 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SPIMSwapDisable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SPIMSwapEn), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SdramswapDisable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SdramswapEn), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDDATAIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDDATAPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetCLCDSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMIDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMIIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMIIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMIPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMIPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetDCMISR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTHSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetGINTLSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C1IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C1PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C2IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C2PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C3IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2C3PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2CDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2CIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2CSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SPS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetI2SSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMADDRIE), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMADDRPDE), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMADDRPUE), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATADC), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATAHX), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATAIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATAODE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATAPDE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRAMDATAPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRDC), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRHX), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRODE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRPDE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSDRPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMDC), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMHX), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMIE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMODE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMPDE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSMPUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI1IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI1PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI2IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI2PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI3IE), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPI3PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPIDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPIIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSPISR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1DS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1IE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1IS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1ODE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1PS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1PUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI1SR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2DS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2IE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2IS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2ODE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2PS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2PUE), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetSSI2SR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUART1PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUART2PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUARTDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUARTIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUARTSR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI1PS), (34 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2DIEN), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2DREN), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2SWAPDis), (14 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI2SWAPEn), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3DIEN), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3DREN), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSI3PUEN), (28 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSIDS), (58 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSIIS), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SetUSISR), (30 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap2Disable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap2En), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap3Disable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap3En), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap4Disable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap4En), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap5Disable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_Swap5En), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SwaphDisable), (16 bytes).
    Removing ioctrl_drv.o(i.DRV_IOCTRL_SwaphEn), (16 bytes).
    Removing pit32_drv.o(.rev16_text), (4 bytes).
    Removing pit32_drv.o(.revsh_text), (4 bytes).
    Removing pit32_drv.o(.rrx_text), (6 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_Cmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_DebugCmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_DozeCmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_GetCounter), (4 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_ImmediatelyUpdateCNTCmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_InterruptCmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_ReloadCmd), (20 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_SetCounter), (4 bytes).
    Removing pit32_drv.o(i.DRV_PIT32_SetPrescaler), (14 bytes).
    Removing pwm_drv.o(.rev16_text), (4 bytes).
    Removing pwm_drv.o(.revsh_text), (4 bytes).
    Removing pwm_drv.o(.rrx_text), (6 bytes).
    Removing pwm_drv.o(i.DRV_PWM_CHxCaptureCmd), (178 bytes).
    Removing pwm_drv.o(i.DRV_PWM_CHxFallinginterruptCmd), (178 bytes).
    Removing pwm_drv.o(i.DRV_PWM_CHxRisingInterruptCmd), (178 bytes).
    Removing pwm_drv.o(i.DRV_PWM_GetCHxLevel), (76 bytes).
    Removing pwm_drv.o(i.DRV_PWM_GetCHxPeriod), (56 bytes).
    Removing pwm_drv.o(i.DRV_PWM_GetCHxTimerCounter), (56 bytes).
    Removing pwm_drv.o(i.DRV_PWM_GetCHxTimerInterrupt), (76 bytes).
    Removing pwm_drv.o(i.DRV_PWM_GetCHxWidth), (56 bytes).
    Removing reset_drv.o(.rev16_text), (4 bytes).
    Removing reset_drv.o(.revsh_text), (4 bytes).
    Removing reset_drv.o(.rrx_text), (6 bytes).
    Removing reset_drv.o(i.DRV_RESET_GetStatus), (32 bytes).
    Removing reset_drv.o(i.DRV_RESET_SoftReset), (16 bytes).
    Removing rtc_drv.o(.rev16_text), (4 bytes).
    Removing rtc_drv.o(.revsh_text), (4 bytes).
    Removing rtc_drv.o(.rrx_text), (6 bytes).
    Removing rtc_drv.o(i.DRV_RTC_IRQHandler), (308 bytes).
    Removing rtc_drv.o(i.DRV_RTC_SetAlarmTimeCounter), (60 bytes).
    Removing sdio_drv.o(i.ACMD41_SD_tsk), (36 bytes).
    Removing sdio_drv.o(i.ACMD42_SD_tsk), (36 bytes).
    Removing sdio_drv.o(i.ACMD51_SD_tsk), (40 bytes).
    Removing sdio_drv.o(i.ACMD6_SD_tsk), (36 bytes).
    Removing sdio_drv.o(i.CMD0_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD11_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD12_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD13_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD16_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD17_SD_tsk), (40 bytes).
    Removing sdio_drv.o(i.CMD18_SD_tsk), (40 bytes).
    Removing sdio_drv.o(i.CMD1_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD24_SD_tsk), (40 bytes).
    Removing sdio_drv.o(i.CMD25_SD_tsk), (40 bytes).
    Removing sdio_drv.o(i.CMD2_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD3_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD52_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD55_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD5_SD_tsk), (36 bytes).
    Removing sdio_drv.o(i.CMD6_SD_tsk), (28 bytes).
    Removing sdio_drv.o(i.CMD7_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD8_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.CMD9_SD_tsk), (24 bytes).
    Removing sdio_drv.o(i.SDIO_CardDetect), (48 bytes).
    Removing sdio_drv.o(i.SDIO_Card_Volt), (20 bytes).
    Removing sdio_drv.o(i.SDIO_ConfigDesc), (84 bytes).
    Removing sdio_drv.o(i.SDIO_GetPowerState), (20 bytes).
    Removing sdio_drv.o(i.SDIO_HCON), (24 bytes).
    Removing sdio_drv.o(i.SDIO_Init_NOINT), (44 bytes).
    Removing sdio_drv.o(i.SDIO_Internal_Dmac_Ctrl), (40 bytes).
    Removing sdio_drv.o(i.SDIO_PollStatus), (48 bytes).
    Removing sdio_drv.o(i.SDIO_PowerUp), (20 bytes).
    Removing sdio_drv.o(i.SDIO_Reset), (32 bytes).
    Removing sdio_drv.o(i.SDIO_SetClk), (56 bytes).
    Removing sdio_drv.o(i.SDIO_Start_CMD), (16 bytes).
    Removing sdio_drv.o(i.SDIO_SwitchClk), (24 bytes).
    Removing sdio_drv.o(.bss), (4096 bytes).
    Removing sdio_drv.o(.data), (4 bytes).
    Removing sdram_drv.o(.rev16_text), (4 bytes).
    Removing sdram_drv.o(.revsh_text), (4 bytes).
    Removing sdram_drv.o(.rrx_text), (6 bytes).
    Removing sdram2lcd_drv.o(.rev16_text), (4 bytes).
    Removing sdram2lcd_drv.o(.revsh_text), (4 bytes).
    Removing sdram2lcd_drv.o(.rrx_text), (6 bytes).
    Removing sdram2lcd_drv.o(i.DRV_SDRAM2LCD_Init), (36 bytes).
    Removing spi_drv.o(.rev16_text), (4 bytes).
    Removing spi_drv.o(.revsh_text), (4 bytes).
    Removing spi_drv.o(.rrx_text), (6 bytes).
    Removing spi_drv.o(i.DRV_SPI_ClrFlag), (66 bytes).
    Removing spi_drv.o(i.DRV_SPI_Cmd), (20 bytes).
    Removing spi_drv.o(i.DRV_SPI_DeInit), (20 bytes).
    Removing spi_drv.o(i.DRV_SPI_Dis), (10 bytes).
    Removing spi_drv.o(i.DRV_SPI_En), (10 bytes).
    Removing spi_drv.o(i.DRV_SPI_GPIODeInit), (2 bytes).
    Removing spi_drv.o(i.DRV_SPI_GPIOInit), (40 bytes).
    Removing spi_drv.o(i.DRV_SPI_GetDR), (6 bytes).
    Removing spi_drv.o(i.DRV_SPI_GetFlag), (44 bytes).
    Removing spi_drv.o(i.DRV_SPI_Init), (374 bytes).
    Removing spi_drv.o(i.DRV_SPI_ItEn), (2 bytes).
    Removing spi_drv.o(i.DRV_SPI_ReadPin), (14 bytes).
    Removing spi_drv.o(i.DRV_SPI_ReceiveByte), (54 bytes).
    Removing spi_drv.o(i.DRV_SPI_ReceiveBytes), (66 bytes).
    Removing spi_drv.o(i.DRV_SPI_SetDR), (4 bytes).
    Removing spi_drv.o(i.DRV_SPI_SlaveReceiveByte), (44 bytes).
    Removing spi_drv.o(i.DRV_SPI_SlaveReceiveBytes), (66 bytes).
    Removing spi_drv.o(i.DRV_SPI_SlaveTransmitByte), (52 bytes).
    Removing spi_drv.o(i.DRV_SPI_SlaveTransmitBytes), (56 bytes).
    Removing spi_drv.o(i.DRV_SPI_TogglePin), (12 bytes).
    Removing spi_drv.o(i.DRV_SPI_TransmitByte), (26 bytes).
    Removing spi_drv.o(i.DRV_SPI_TransmitBytes), (48 bytes).
    Removing spi_drv.o(i.DRV_SPI_WaitonFlagTimeout), (108 bytes).
    Removing spi_drv.o(i.DRV_SPI_WritePin), (18 bytes).
    Removing ssi_drv.o(.rev16_text), (4 bytes).
    Removing ssi_drv.o(.revsh_text), (4 bytes).
    Removing ssi_drv.o(.rrx_text), (6 bytes).
    Removing ssi_drv.o(i.DRV_EFlash_Set_Read_Para), (100 bytes).
    Removing ssi_drv.o(i.DRV_Get_SSI_baund), (6 bytes).
    Removing ssi_drv.o(i.DRV_PsramInit), (108 bytes).
    Removing ssi_drv.o(i.DRV_SSI_CS_HIGH), (36 bytes).
    Removing ssi_drv.o(i.DRV_SSI_CS_LOW), (36 bytes).
    Removing ssi_drv.o(i.DRV_SSI_DMA_Receive_level), (4 bytes).
    Removing ssi_drv.o(i.DRV_SSI_DMA_Transmit_level), (4 bytes).
    Removing ssi_drv.o(i.DRV_SSI_DUAL_DMA_Trig), (8 bytes).
    Removing ssi_drv.o(i.DRV_SSI_DUAL_Init), (146 bytes).
    Removing ssi_drv.o(i.DRV_SSI_DeInit), (44 bytes).
    Removing ssi_drv.o(i.DRV_SSI_Dis), (10 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_DUAL_Read), (104 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_Get_Status1), (122 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_Get_Status2), (122 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status12), (80 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_Prog_Status2), (86 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_EXIT), (72 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Enter), (74 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Get_Status1), (106 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Program), (114 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Read), (122 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Sector_Erase), (142 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_WAIT_Status1), (50 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QPI_Write_Enable), (104 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Program), (180 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_QUAD_Read), (104 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_STD_Block_Erase), (112 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_STD_Program), (146 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_STD_Read), (144 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_STD_Sector_Erase), (120 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_WAIT_Status1), (48 bytes).
    Removing ssi_drv.o(i.DRV_SSI_EFlash_Write_Enable), (112 bytes).
    Removing ssi_drv.o(i.DRV_SSI_En), (10 bytes).
    Removing ssi_drv.o(i.DRV_SSI_ItEn), (2 bytes).
    Removing ssi_drv.o(i.DRV_SSI_QPI_DMA_Trig), (8 bytes).
    Removing ssi_drv.o(i.DRV_SSI_QPI_Init), (252 bytes).
    Removing ssi_drv.o(i.DRV_SSI_QUAD_DMA_Trig), (8 bytes).
    Removing ssi_drv.o(i.DRV_SSI_QUAD_Init), (140 bytes).
    Removing ssi_drv.o(i.DRV_SSI_STD_DMA_Trig), (22 bytes).
    Removing ssi_drv.o(i.DRV_SSI_STD_Init), (68 bytes).
    Removing ssi_drv.o(i.DRV_SSI_STD_Read_ID), (114 bytes).
    Removing ssi_drv.o(i.DRV_SSI_STD_Reset), (76 bytes).
    Removing ssi_drv.o(i.DRV_SSI_STD_Reset_Enable), (62 bytes).
    Removing ssi_drv.o(i.DRV_SSI_StructInit), (60 bytes).
    Removing ssi_drv.o(i.DRV_SSI_WAIT_IDLE), (10 bytes).
    Removing ssi_drv.o(i.DRV_SSI_XIP_SET), (152 bytes).
    Removing ssi_drv.o(i.DRV_SSI_clear_fifo), (82 bytes).
    Removing ssi_drv.o(i.DRV_XIP_EXIT), (50 bytes).
    Removing ssi_drv.o(i.DRV_XIP_Enter), (146 bytes).
    Removing ssi_drv.o(i.SSI_EFlash_Get_Status), (68 bytes).
    Removing ssi_drv.o(i.SSI_EFlash_Write_Enable), (92 bytes).
    Removing ssi_drv.o(i.SSI_QUAD_Burst_Init), (120 bytes).
    Removing ssi_drv.o(i.SSI_STD_DMA_Program), (112 bytes).
    Removing ssi_drv.o(i.SSI_STD_DMA_Read), (120 bytes).
    Removing ssi_drv.o(i.SSI_Standard_Init), (64 bytes).
    Removing ssi_drv.o(i.SSI_Wait_SPIFlash_Idle), (38 bytes).
    Removing tc_drv.o(.rev16_text), (4 bytes).
    Removing tc_drv.o(.revsh_text), (4 bytes).
    Removing tc_drv.o(.rrx_text), (6 bytes).
    Removing tc_drv.o(i.DRV_TC_DebugCmd), (6 bytes).
    Removing tc_drv.o(i.DRV_TC_DozeCmd), (6 bytes).
    Removing tc_drv.o(i.DRV_TC_InterruptCmd), (20 bytes).
    Removing tc_drv.o(i.DRV_TC_ResetCmd), (20 bytes).
    Removing tc_drv.o(i.DRV_TC_StopCmd), (6 bytes).
    Removing tc_drv.o(i.DRV_TC_WaitCmd), (14 bytes).
    Removing tc_drv.o(.data), (1 bytes).
    Removing uart_drv.o(.rev16_text), (4 bytes).
    Removing uart_drv.o(.revsh_text), (4 bytes).
    Removing uart_drv.o(.rrx_text), (6 bytes).
    Removing uart_drv.o(i.DRV_UART_ClearFlag), (32 bytes).
    Removing uart_drv.o(i.DRV_UART_Deinit), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_Dis), (18 bytes).
    Removing uart_drv.o(i.DRV_UART_DisIt), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_DisItRe), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_DisItTcie), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_DisItTie), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_DisPullup), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_DisRx), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_DisTx), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_En), (18 bytes).
    Removing uart_drv.o(i.DRV_UART_EnIt), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_EnPullup), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_EnRx), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_EnTx), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_GetData), (34 bytes).
    Removing uart_drv.o(i.DRV_UART_GetFlag), (34 bytes).
    Removing uart_drv.o(i.DRV_UART_GetItSource), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_GetPinBit), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_GetRxdPinBit), (6 bytes).
    Removing uart_drv.o(i.DRV_UART_GetStatus), (12 bytes).
    Removing uart_drv.o(i.DRV_UART_GetTxdPinBit), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_Init), (84 bytes).
    Removing uart_drv.o(i.DRV_UART_PutcDev), (36 bytes).
    Removing uart_drv.o(i.DRV_UART_PutsDev), (22 bytes).
    Removing uart_drv.o(i.DRV_UART_ResetPinBit), (12 bytes).
    Removing uart_drv.o(i.DRV_UART_ResetRxdPinBit), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_ResetTxdPinBit), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_RxdPinToggle), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_SendByte), (16 bytes).
    Removing uart_drv.o(i.DRV_UART_SendByteHex), (28 bytes).
    Removing uart_drv.o(i.DRV_UART_SendBytes), (30 bytes).
    Removing uart_drv.o(i.DRV_UART_SendData), (8 bytes).
    Removing uart_drv.o(i.DRV_UART_SendOne), (26 bytes).
    Removing uart_drv.o(i.DRV_UART_SendString), (24 bytes).
    Removing uart_drv.o(i.DRV_UART_SetOutputCmos), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetOutputOpendrain), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetPinBit), (12 bytes).
    Removing uart_drv.o(i.DRV_UART_SetRxdDirInput), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetRxdDirOutput), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetRxdPinBit), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetTxdDirInput), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetTxdDirOutput), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_SetTxdPinBit), (10 bytes).
    Removing uart_drv.o(i.DRV_UART_TxdPinToggle), (22 bytes).
    Removing uart_drv.o(i.DRV_UART_WaitonFlagTimeout), (108 bytes).
    Removing uart_drv.o(i.UART_ISR), (44 bytes).
    Removing uart_drv.o(i.UART_RecvByte), (108 bytes).
    Removing uart_drv.o(i.UART_SendByte), (32 bytes).
    Removing uart_drv.o(.bss), (2064 bytes).
    Removing uart_drv.o(.data), (4 bytes).
    Removing wdt_drv.o(.rev16_text), (4 bytes).
    Removing wdt_drv.o(.revsh_text), (4 bytes).
    Removing wdt_drv.o(.rrx_text), (6 bytes).
    Removing wdt_drv.o(i.DRV_WDT_Close), (16 bytes).
    Removing wdt_drv.o(i.DRV_WDT_FeedDog), (20 bytes).
    Removing wdt_drv.o(i.DRV_WDT_GetCount), (12 bytes).
    Removing wdt_drv.o(i.DRV_WDT_Init), (16 bytes).
    Removing wdt_drv.o(i.DRV_WDT_Open), (16 bytes).
    Removing cache_hal.o(.rev16_text), (4 bytes).
    Removing cache_hal.o(.revsh_text), (4 bytes).
    Removing cache_hal.o(.rrx_text), (6 bytes).
    Removing cache_hal.o(i.HAL_CACHE_Syn), (14 bytes).
    Removing can_hal.o(.rev16_text), (4 bytes).
    Removing can_hal.o(.revsh_text), (4 bytes).
    Removing can_hal.o(.rrx_text), (6 bytes).
    Removing can_hal.o(i.DrvStatusToHalStatus), (2 bytes).
    Removing can_hal.o(i.HAL_CAN_DeInit), (80 bytes).
    Removing can_hal.o(i.HAL_CAN_IRQHandler), (184 bytes).
    Removing can_hal.o(i.HAL_CAN_Init), (164 bytes).
    Removing can_hal.o(i.HAL_CAN_MspInit), (2 bytes).
    Removing can_hal.o(i.HAL_CAN_Receive), (70 bytes).
    Removing can_hal.o(i.HAL_CAN_ReceiveIT), (70 bytes).
    Removing can_hal.o(i.HAL_CAN_Transmit), (54 bytes).
    Removing can_hal.o(i.HAL_CAN_TransmitIT), (54 bytes).
    Removing can_hal.o(i.NVIC_DisableIRQ), (22 bytes).
    Removing can_hal.o(.data), (4 bytes).
    Removing clcd_hal.o(.rev16_text), (4 bytes).
    Removing clcd_hal.o(.revsh_text), (4 bytes).
    Removing clcd_hal.o(.rrx_text), (6 bytes).
    Removing clcd_hal.o(i.HAL_CLCD_CheckState), (36 bytes).
    Removing clcd_hal.o(i.HAL_CLCD_DeInit), (12 bytes).
    Removing clcd_hal.o(.data), (4 bytes).
    Removing cpm_hal.o(.rev16_text), (4 bytes).
    Removing cpm_hal.o(.revsh_text), (4 bytes).
    Removing cpm_hal.o(.rrx_text), (6 bytes).
    Removing cpm_hal.o(i.HAL_CPM_CardPowerOff), (26 bytes).
    Removing cpm_hal.o(i.HAL_CPM_CardPowerOn), (116 bytes).
    Removing cpm_hal.o(i.HAL_CPM_GetClocksFreq), (22 bytes).
    Removing cpm_hal.o(i.HAL_CPM_ModuleClkCmd), (10 bytes).
    Removing cpm_hal.o(i.HAL_CPM_PorReset), (4 bytes).
    Removing cpm_hal.o(i.HAL_CPM_TrimCardVoltage), (46 bytes).
    Removing cpm_hal.o(i.HAL_CPM_VCC5VByPass), (28 bytes).
    Removing cpm_hal.o(i.HAL_CPM_WakeupDeInit), (12 bytes).
    Removing cpm_hal.o(i.HAL_CPM_WakeupFlagDet), (78 bytes).
    Removing cpm_hal.o(i.HAL_CPM_WakeupInit), (262 bytes).
    Removing cpm_hal.o(.constdata), (4 bytes).
    Removing dcmi_hal.o(.rev16_text), (4 bytes).
    Removing dcmi_hal.o(.revsh_text), (4 bytes).
    Removing dcmi_hal.o(.rrx_text), (6 bytes).
    Removing dcmi_hal.o(i.HAL_DCMI_Callback), (144 bytes).
    Removing dcmi_hal.o(i.HAL_DCMI_Getgray), (16 bytes).
    Removing dcmi_hal.o(i.HAL_DCMI_IRQHandler), (20 bytes).
    Removing dcmi_hal.o(i.HAL_DCMI_Init), (52 bytes).
    Removing dcmi_hal.o(.data), (4 bytes).
    Removing dma_hal.o(.rev16_text), (4 bytes).
    Removing dma_hal.o(.revsh_text), (4 bytes).
    Removing dma_hal.o(.rrx_text), (6 bytes).
    Removing dma_hal.o(i.DMAC_SetConfig), (280 bytes).
    Removing dma_hal.o(i.HAL_DMAC_Abort), (102 bytes).
    Removing dma_hal.o(i.HAL_DMAC_ClearRawStatus), (6 bytes).
    Removing dma_hal.o(i.HAL_DMAC_ConfigLLi), (12 bytes).
    Removing dma_hal.o(i.HAL_DMAC_Deinit), (90 bytes).
    Removing dma_hal.o(i.HAL_DMAC_GetFreeChannel), (36 bytes).
    Removing dma_hal.o(i.HAL_DMAC_IRQHandler), (116 bytes).
    Removing dma_hal.o(i.HAL_DMAC_Init), (114 bytes).
    Removing dma_hal.o(i.HAL_DMAC_PollForTransfer), (92 bytes).
    Removing dma_hal.o(i.HAL_DMAC_PollForTransfer_IT), (108 bytes).
    Removing dma_hal.o(i.HAL_DMAC_PollForTransfer_test), (48 bytes).
    Removing dma_hal.o(i.HAL_DMAC_Resume), (4 bytes).
    Removing dma_hal.o(i.HAL_DMAC_StartIT), (116 bytes).
    Removing dma_hal.o(i.HAL_DMAC_StartPolling), (62 bytes).
    Removing dma_hal.o(i.HAL_DMAC_StartPolling_test), (62 bytes).
    Removing dma_hal.o(i.HAL_DMAC_Suspend), (4 bytes).
    Removing dma_hal.o(i.HAL_DMA_Getstate), (6 bytes).
    Removing dma_hal.o(.data), (4 bytes).
    Removing dma2d_hal.o(.rev16_text), (4 bytes).
    Removing dma2d_hal.o(.revsh_text), (4 bytes).
    Removing dma2d_hal.o(.rrx_text), (6 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_BlendHard), (40 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_Callback), (32 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_ClutInit), (4 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_FgClutLoad), (10 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_IRQHandler), (20 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_Mem2Mem), (40 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_PfcHard), (40 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_Reg2Mem), (40 bytes).
    Removing dma2d_hal.o(i.HAL_DMA2D_SoftReset), (4 bytes).
    Removing dma2d_hal.o(.data), (4 bytes).
    Removing eflash_hal.o(.rev16_text), (4 bytes).
    Removing eflash_hal.o(.revsh_text), (4 bytes).
    Removing eflash_hal.o(.rrx_text), (6 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_Lock), (8 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_PageErase), (12 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_ProgramBulk), (12 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_ProgramWord), (12 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_Read), (4 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_SetWritePermission), (4 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_Unlock), (8 bytes).
    Removing eflash_hal.o(i.HAL_EFLASH_Write), (220 bytes).
    Removing eflash_hal.o(.bss), (512 bytes).
    Removing eport_hal.o(.rev16_text), (4 bytes).
    Removing eport_hal.o(.revsh_text), (4 bytes).
    Removing eport_hal.o(.rrx_text), (6 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT0_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT10_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT11_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT12_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT13_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT14_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_0_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_1_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_2_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_3_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_4_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_5_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_6_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT15_7_IRQHandler), (32 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT1_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT2_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT3_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT4_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT5_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT6_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT7_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT8_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_0_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_1_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_2_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_3_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_4_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_5_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_6_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT9_7_IRQHandler), (12 bytes).
    Removing eport_hal.o(i.HAL_EPORT_GintSwitch), (1304 bytes).
    Removing eport_hal.o(i.HAL_EPORT_Init), (904 bytes).
    Removing eport_hal.o(i.HAL_EPORT_ReadPinLevel), (10 bytes).
    Removing eport_hal.o(i.HAL_EPORT_ReadPinsLevel), (6 bytes).
    Removing eport_hal.o(i.HAL_EPORT_WritePinsLevel), (4 bytes).
    Removing hal.o(.rev16_text), (4 bytes).
    Removing hal.o(.revsh_text), (4 bytes).
    Removing hal.o(.rrx_text), (6 bytes).
    Removing hal.o(i.HAL_DeInit), (4 bytes).
    Removing hal.o(i.HAL_Delay), (2 bytes).
    Removing hal.o(i.HAL_DisBoot), (6 bytes).
    Removing hal.o(i.HAL_GetSN), (10 bytes).
    Removing hal.o(i.HAL_GetTick), (4 bytes).
    Removing hal.o(i.HAL_IncTick1), (32 bytes).
    Removing hal.o(i.HAL_InitTick), (4 bytes).
    Removing hal.o(i.HAL_LockDisJtag), (2 bytes).
    Removing hal.o(i.HAL_PrintfVersion), (424 bytes).
    Removing hal.o(i.HAL_RebackBoot), (14 bytes).
    Removing hal.o(i.HAL_ResumeTick), (4 bytes).
    Removing hal.o(i.HAL_SuspendTick), (4 bytes).
    Removing hal.o(i.SysClk_SoftRstReconfig), (52 bytes).
    Removing hal.o(.data), (4 bytes).
    Removing hal.o(.data), (4 bytes).
    Removing i2c_hal.o(.rev16_text), (4 bytes).
    Removing i2c_hal.o(.revsh_text), (4 bytes).
    Removing i2c_hal.o(.rrx_text), (6 bytes).
    Removing i2c_hal.o(i.DrvStatusToHalStatus), (2 bytes).
    Removing i2c_hal.o(i.HAL_I2C_DeInit), (32 bytes).
    Removing i2c_hal.o(i.HAL_I2C_GPIODeInit), (6 bytes).
    Removing i2c_hal.o(i.HAL_I2C_GPIOTogglePin), (6 bytes).
    Removing i2c_hal.o(i.HAL_I2C_GPIOWritePin), (6 bytes).
    Removing i2c_hal.o(i.HAL_I2C_GetError), (4 bytes).
    Removing i2c_hal.o(i.HAL_I2C_GetState), (6 bytes).
    Removing i2c_hal.o(i.HAL_I2C_IRQ), (46 bytes).
    Removing i2c_hal.o(i.HAL_I2C_Init), (48 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterIRQHandler), (196 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterMemIRQHandler), (328 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterRecceive), (80 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterReceiveIT), (100 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterTransmit), (80 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MasterTransmitIT), (96 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MemRead), (94 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MemReadIT), (104 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MemWrite), (94 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MemWriteIT), (96 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MspDeInit), (2 bytes).
    Removing i2c_hal.o(i.HAL_I2C_MspInit), (2 bytes).
    Removing i2c_hal.o(i.HAL_I2C_SlaveIRQHandler), (146 bytes).
    Removing i2c_hal.o(i.HAL_I2C_SlaveReceive), (68 bytes).
    Removing i2c_hal.o(i.HAL_I2C_SlaveReceiveIT), (64 bytes).
    Removing i2c_hal.o(i.HAL_I2C_SlaveTransmit), (64 bytes).
    Removing i2c_hal.o(i.HAL_I2C_SlaveTransmitIT), (64 bytes).
    Removing ioctrl_hal.o(.rev16_text), (4 bytes).
    Removing ioctrl_hal.o(.revsh_text), (4 bytes).
    Removing ioctrl_hal.o(.rrx_text), (6 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_GINTIint), (88 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_I2CInit), (92 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_SPIInit), (92 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_SSIIint), (112 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_SwapintDIS), (18 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_UARTInit), (54 bytes).
    Removing ioctrl_hal.o(i.HAL_IOCTRL_USIInit), (88 bytes).
    Removing lowpower_hal.o(.rev16_text), (4 bytes).
    Removing lowpower_hal.o(.revsh_text), (4 bytes).
    Removing lowpower_hal.o(.rrx_text), (6 bytes).
    Removing lowpower_hal.o(i.LOWPOWER_DeepSleep), (204 bytes).
    Removing lowpower_hal.o(i.LOWPOWER_Hiber), (168 bytes).
    Removing lowpower_hal.o(i.LOWPOWER_Lowpower), (172 bytes).
    Removing lowpower_hal.o(i.LOWPOWER_Retention), (208 bytes).
    Removing pit32_hal.o(.rev16_text), (4 bytes).
    Removing pit32_hal.o(.revsh_text), (4 bytes).
    Removing pit32_hal.o(.rrx_text), (6 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_CMD), (6 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_Callback), (2 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_CleanITStatus), (12 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_GetCounter), (12 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_GetITStatus), (16 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_GetPrescaler), (10 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_ITConfig), (6 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_Init), (180 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_SetCounter), (6 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_SetPrescaler), (6 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_Start), (8 bytes).
    Removing pit32_hal.o(i.HAL_PIT32_Stop), (8 bytes).
    Removing psram_hal.o(.rev16_text), (4 bytes).
    Removing psram_hal.o(.revsh_text), (4 bytes).
    Removing psram_hal.o(.rrx_text), (6 bytes).
    Removing psram_hal.o(i.HAL_PSRAM_Init), (24 bytes).
    Removing psram_hal.o(i.HAL_PSRAM_Read), (38 bytes).
    Removing psram_hal.o(i.HAL_PSRAM_Write), (38 bytes).
    Removing psram_hal.o(i.get_psram_baseaddress), (28 bytes).
    Removing psram_hal.o(.data), (4 bytes).
    Removing pwm_hal.o(.rev16_text), (4 bytes).
    Removing pwm_hal.o(.revsh_text), (4 bytes).
    Removing pwm_hal.o(.rrx_text), (6 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxAutoLoadMode), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxCaptureCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxDeadZoneCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxFallinginterruptCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxInverteCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxPullupCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxRisingInterruptCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_CHxTimerInverteCmd), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ClrCaptureInterruptFlag), (114 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ClrFallingInterruptFlag), (114 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ClrRisingInterruptFlag), (114 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxClkDiv), (16 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxDeadZone), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxEdgeinterrupt), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxPeriod), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxPerscaler), (16 bytes).
    Removing pwm_hal.o(i.HAL_PWM_ConfigCHxWidth), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetCHxLevel), (8 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetCHxPeriod), (8 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetCHxTimerCounter), (8 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetCHxWidth), (8 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetCaptureInterruptFlag), (82 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetFallingInterruptFlag), (82 bytes).
    Removing pwm_hal.o(i.HAL_PWM_GetRisingInterruptFlag), (82 bytes).
    Removing pwm_hal.o(i.HAL_PWM_IRQHandler), (124 bytes).
    Removing pwm_hal.o(i.HAL_PWM_SetCHxDirection), (10 bytes).
    Removing pwm_hal.o(i.HAL_PWM_SetCHxLevel), (10 bytes).
    Removing reset_hal.o(.rev16_text), (4 bytes).
    Removing reset_hal.o(.revsh_text), (4 bytes).
    Removing reset_hal.o(.rrx_text), (6 bytes).
    Removing reset_hal.o(i.HAL_RESET_Disable), (68 bytes).
    Removing reset_hal.o(i.HAL_RESET_GetStatus), (12 bytes).
    Removing reset_hal.o(i.HAL_RESET_SoftReset), (4 bytes).
    Removing rtc_hal.o(.rev16_text), (4 bytes).
    Removing rtc_hal.o(.revsh_text), (4 bytes).
    Removing rtc_hal.o(.rrx_text), (6 bytes).
    Removing rtc_hal.o(i.HAL_RTC_AralmConfig), (188 bytes).
    Removing rtc_hal.o(i.HAL_RTC_GetTime), (4 bytes).
    Removing rtc_hal.o(i.HAL_RTC_IRQHandler), (4 bytes).
    Removing rtc_hal.o(i.HAL_RTC_Init), (88 bytes).
    Removing rtc_hal.o(i.HAL_RTC_SetTime), (4 bytes).
    Removing sdcard_hal.o(i.HAL_SD_EnWideBus), (68 bytes).
    Removing sdcard_hal.o(i.HAL_SD_EnumCard), (308 bytes).
    Removing sdcard_hal.o(i.HAL_SD_GetCardInfo), (580 bytes).
    Removing sdcard_hal.o(i.HAL_SD_Init), (184 bytes).
    Removing sdcard_hal.o(i.HAL_SD_InitializeCards), (372 bytes).
    Removing sdcard_hal.o(i.HAL_SD_PowerON), (132 bytes).
    Removing sdcard_hal.o(i.HAL_SD_ReadBlock), (156 bytes).
    Removing sdcard_hal.o(i.HAL_SD_SelectDeselect), (68 bytes).
    Removing sdcard_hal.o(i.HAL_SD_SendSCR), (68 bytes).
    Removing sdcard_hal.o(i.HAL_SD_StopTransfer), (40 bytes).
    Removing sdcard_hal.o(i.HAL_SD_WriteBlock), (180 bytes).
    Removing sdcard_hal.o(i.SDIO_CMD53_Xfer), (172 bytes).
    Removing sdcard_hal.o(i.SDIO_EnableAsyncInterrupt), (114 bytes).
    Removing sdcard_hal.o(i.SDIO_GetCardCapability), (300 bytes).
    Removing sdcard_hal.o(i.SDIO_IO_RW_Direct), (72 bytes).
    Removing sdcard_hal.o(i.SDIO_SetDriverStrength), (92 bytes).
    Removing sdcard_hal.o(i.SDIO_SwitchToHighSpeed), (126 bytes).
    Removing sdcard_hal.o(i.SD_CmdResp1Error), (172 bytes).
    Removing sdcard_hal.o(i.SD_ReadBlock_Start), (72 bytes).
    Removing sdcard_hal.o(i.SD_ReadBlock_Stop), (48 bytes).
    Removing sdcard_hal.o(i.SD_SwitchFunc_V2_0), (120 bytes).
    Removing sdcard_hal.o(i.SD_SwitchFunc_V3_0), (244 bytes).
    Removing sdcard_hal.o(i.SD_WriteBlock_Start), (84 bytes).
    Removing sdcard_hal.o(i.SD_WriteBlock_Stop), (116 bytes).
    Removing sdcard_hal.o(i.core_sdio_xfer), (276 bytes).
    Removing sdcard_hal.o(.bss), (688 bytes).
    Removing sdcard_hal.o(.data), (20 bytes).
    Removing sdram_hal.o(.rev16_text), (4 bytes).
    Removing sdram_hal.o(.revsh_text), (4 bytes).
    Removing sdram_hal.o(.rrx_text), (6 bytes).
    Removing sdram2lcd_hal.o(.rev16_text), (4 bytes).
    Removing sdram2lcd_hal.o(.revsh_text), (4 bytes).
    Removing sdram2lcd_hal.o(.rrx_text), (6 bytes).
    Removing sdram2lcd_hal.o(i.HAL_SDRAM2LCD_Init), (16 bytes).
    Removing spi_hal.o(.rev16_text), (4 bytes).
    Removing spi_hal.o(.revsh_text), (4 bytes).
    Removing spi_hal.o(.rrx_text), (6 bytes).
    Removing spi_hal.o(i.DrvStatusToHalStatus), (2 bytes).
    Removing spi_hal.o(i.HAL_SPI_ClrFlag), (22 bytes).
    Removing spi_hal.o(i.HAL_SPI_ClrRxFifo), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_ClrTxFifo), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_DeInit), (42 bytes).
    Removing spi_hal.o(i.HAL_SPI_Dis), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_DisIt), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_DisRxDma), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_DisTxDma), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_Disable), (10 bytes).
    Removing spi_hal.o(i.HAL_SPI_En), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_EnIt), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_EnRxDma), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_EnTxDma), (12 bytes).
    Removing spi_hal.o(i.HAL_SPI_GPIODeInit), (6 bytes).
    Removing spi_hal.o(i.HAL_SPI_GPIOInit), (10 bytes).
    Removing spi_hal.o(i.HAL_SPI_GPIOReadPin), (6 bytes).
    Removing spi_hal.o(i.HAL_SPI_GPIOTogglePin), (6 bytes).
    Removing spi_hal.o(i.HAL_SPI_GPIOWritePin), (6 bytes).
    Removing spi_hal.o(i.HAL_SPI_GetError), (4 bytes).
    Removing spi_hal.o(i.HAL_SPI_GetFlag), (22 bytes).
    Removing spi_hal.o(i.HAL_SPI_GetState), (6 bytes).
    Removing spi_hal.o(i.HAL_SPI_IRQ), (76 bytes).
    Removing spi_hal.o(i.HAL_SPI_Init), (52 bytes).
    Removing spi_hal.o(i.HAL_SPI_MspDeInit), (2 bytes).
    Removing spi_hal.o(i.HAL_SPI_MspInit), (2 bytes).
    Removing spi_hal.o(i.HAL_SPI_Receive), (110 bytes).
    Removing spi_hal.o(i.HAL_SPI_ReceiveEDMAC), (4 bytes).
    Removing spi_hal.o(i.HAL_SPI_ReceiveIT), (64 bytes).
    Removing spi_hal.o(i.HAL_SPI_RegisterCallback), (20 bytes).
    Removing spi_hal.o(i.HAL_SPI_Transmit), (100 bytes).
    Removing spi_hal.o(i.HAL_SPI_TransmitEDMAC), (4 bytes).
    Removing spi_hal.o(i.HAL_SPI_TransmitIT), (76 bytes).
    Removing spi_hal.o(i.HAL_SPI_TransmitReceive), (44 bytes).
    Removing spi_hal.o(i.HAL_SPI_WaitonFlagTimeout), (22 bytes).
    Removing ssi_hal.o(.rev16_text), (4 bytes).
    Removing ssi_hal.o(.revsh_text), (4 bytes).
    Removing ssi_hal.o(.rrx_text), (6 bytes).
    Removing ssi_hal.o(i.DrvSSIStatusToHalStatus), (2 bytes).
    Removing ssi_hal.o(i.HAL_SSI_DMA_Receive_level), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_DMA_Transmit_level), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_DUAL_DMA_Trig), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_DeInit), (24 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_Program), (66 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_EXIT), (28 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_Enter), (60 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_Program), (40 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_Read), (36 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_Sector_Erase), (30 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_QPI_Write_Enable), (22 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_Read), (92 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_Sector_Erase), (32 bytes).
    Removing ssi_hal.o(i.HAL_SSI_EFlash_Write_Enable), (16 bytes).
    Removing ssi_hal.o(i.HAL_SSI_FLASH_Reset), (36 bytes).
    Removing ssi_hal.o(i.HAL_SSI_Init), (66 bytes).
    Removing ssi_hal.o(i.HAL_SSI_MspInit), (2 bytes).
    Removing ssi_hal.o(i.HAL_SSI_QPI_DMA_Trig), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_QUAD_DMA_Trig), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_Read_ID), (38 bytes).
    Removing ssi_hal.o(i.HAL_SSI_STD_DMA_Program), (12 bytes).
    Removing ssi_hal.o(i.HAL_SSI_STD_DMA_Read), (12 bytes).
    Removing ssi_hal.o(i.HAL_SSI_STD_DMA_Trig), (6 bytes).
    Removing ssi_hal.o(i.HAL_SSI_Standard_Init), (4 bytes).
    Removing ssi_hal.o(i.HAL_SSI_WAIT_IDLE), (22 bytes).
    Removing ssi_hal.o(i.HAL_XIP_EXIT), (28 bytes).
    Removing ssi_hal.o(i.HAL_XIP_Enter), (28 bytes).
    Removing systick_hal.o(.rev16_text), (4 bytes).
    Removing systick_hal.o(.revsh_text), (4 bytes).
    Removing systick_hal.o(.rrx_text), (6 bytes).
    Removing systick_hal.o(i.HAL_Delay_ms), (32 bytes).
    Removing systick_hal.o(i.HAL_SYSTICK_Init), (56 bytes).
    Removing systick_hal.o(i.HAL_TimingDelay_Decrement), (20 bytes).
    Removing systick_hal.o(.data), (4 bytes).
    Removing tc_hal.o(.rev16_text), (4 bytes).
    Removing tc_hal.o(.revsh_text), (4 bytes).
    Removing tc_hal.o(.rrx_text), (6 bytes).
    Removing tc_hal.o(i.HAL_TC_Callback), (28 bytes).
    Removing tc_hal.o(i.HAL_TC_FeedWatchdog), (16 bytes).
    Removing tc_hal.o(i.HAL_TC_GetCounter), (6 bytes).
    Removing tc_hal.o(i.HAL_TC_GetMs), (2 bytes).
    Removing tc_hal.o(i.HAL_TC_IRQHandler), (36 bytes).
    Removing tc_hal.o(i.HAL_TC_Init), (120 bytes).
    Removing tc_hal.o(.data), (8 bytes).
    Removing uart_hal.o(.rev16_text), (4 bytes).
    Removing uart_hal.o(.revsh_text), (4 bytes).
    Removing uart_hal.o(.rrx_text), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_DeInit), (32 bytes).
    Removing uart_hal.o(i.HAL_UART_DisItRe), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_DisItTcie), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_DisItTie), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_DisRxDma), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_DisRxFifo), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_DisTxDma), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_DisTxFifo), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_EnIt), (14 bytes).
    Removing uart_hal.o(i.HAL_UART_EnRxDma), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_EnRxFifo), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_EnTxDma), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_EnTxFifo), (12 bytes).
    Removing uart_hal.o(i.HAL_UART_GPIODeInit), (2 bytes).
    Removing uart_hal.o(i.HAL_UART_GPIOInit), (76 bytes).
    Removing uart_hal.o(i.HAL_UART_GPIOReadPin), (18 bytes).
    Removing uart_hal.o(i.HAL_UART_GPIOTogglePin), (10 bytes).
    Removing uart_hal.o(i.HAL_UART_GPIOWritePin), (32 bytes).
    Removing uart_hal.o(i.HAL_UART_GetData), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_GetError), (4 bytes).
    Removing uart_hal.o(i.HAL_UART_GetRxItFlag), (10 bytes).
    Removing uart_hal.o(i.HAL_UART_GetState), (6 bytes).
    Removing uart_hal.o(i.HAL_UART_IRQHandler), (248 bytes).
    Removing uart_hal.o(i.HAL_UART_ISR_IRQHandler), (4 bytes).
    Removing uart_hal.o(i.HAL_UART_Init), (70 bytes).
    Removing uart_hal.o(i.HAL_UART_MspDeInit), (2 bytes).
    Removing uart_hal.o(i.HAL_UART_MspInit), (2 bytes).
    Removing uart_hal.o(i.HAL_UART_Receive), (76 bytes).
    Removing uart_hal.o(i.HAL_UART_ReceiveIT), (28 bytes).
    Removing uart_hal.o(i.HAL_UART_RecvByteIT), (14 bytes).
    Removing uart_hal.o(i.HAL_UART_RxCpltCallback), (2 bytes).
    Removing uart_hal.o(i.HAL_UART_SendByteIT), (4 bytes).
    Removing uart_hal.o(i.HAL_UART_SendData), (68 bytes).
    Removing uart_hal.o(i.HAL_UART_Transmit), (106 bytes).
    Removing uart_hal.o(i.HAL_UART_TransmitIT), (52 bytes).
    Removing uart_hal.o(i.HAL_UART_TxCpltCallback), (2 bytes).
    Removing wdt_hal.o(.rev16_text), (4 bytes).
    Removing wdt_hal.o(.revsh_text), (4 bytes).
    Removing wdt_hal.o(.rrx_text), (6 bytes).
    Removing wdt_hal.o(i.HAL_WDT_CMD), (12 bytes).
    Removing wdt_hal.o(i.HAL_WDT_FeedWatchdog), (4 bytes).
    Removing wdt_hal.o(i.HAL_WDT_GetCounter), (4 bytes).
    Removing wdt_hal.o(i.HAL_WDT_Init), (4 bytes).
    Removing common.o(i.Read_VEC), (12 bytes).
    Removing common.o(i.enter_critical_sr_save), (6 bytes).
    Removing common.o(i.exit_critical_sr_restore), (6 bytes).
    Removing sys.o(.rev16_text), (4 bytes).
    Removing sys.o(.revsh_text), (4 bytes).
    Removing sys.o(.rrx_text), (6 bytes).
    Removing sys.o(.emb_text), (6 bytes).
    Removing sys.o(i.INTX_DISABLE), (4 bytes).
    Removing sys.o(i.NVIC_SetVectorTable), (16 bytes).
    Removing sys.o(i.Sys_Soft_Reset), (16 bytes).
    Removing sys.o(i.Sys_Standby), (20 bytes).
    Removing sys.o(i.WFI_SET), (4 bytes).
    Removing system_armcm4.o(.rev16_text), (4 bytes).
    Removing system_armcm4.o(.revsh_text), (4 bytes).
    Removing system_armcm4.o(.rrx_text), (6 bytes).
    Removing startup_armcm4.o(HEAP), (8192 bytes).
    Removing misc_c.o(i.ByteToHexAscii), (24 bytes).
    Removing misc_c.o(i.Show16BitValue), (88 bytes).
    Removing misc_c.o(i.Show32BitDecimal), (100 bytes).
    Removing misc_c.o(i.Show32BitValue), (150 bytes).
    Removing misc_c.o(i.Show8BitValue), (46 bytes).
    Removing data.o(.bss), (2048 bytes).
    Removing data.o(.bss), (2048 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (2 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (2 bytes).
    Removing data.o(.data), (2 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (2 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (1 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (4 bytes).
    Removing data.o(.data), (2 bytes).
    Removing font_data.o(.constdata), (95 bytes).
    Removing font_data.o(.constdata), (95 bytes).
    Removing font_data.o(.constdata), (95 bytes).
    Removing font_data.o(.constdata), (95 bytes).
    Removing font_data.o(.constdata), (95 bytes).
    Removing ft5216.o(.rev16_text), (4 bytes).
    Removing ft5216.o(.revsh_text), (4 bytes).
    Removing ft5216.o(.rrx_text), (6 bytes).
    Removing ft5216.o(i.Checksum), (40 bytes).
    Removing ft5216.o(i.I2C_ReadBytes), (28 bytes).
    Removing ft5216.o(i.I2C_WriteBytes), (28 bytes).
    Removing ft5216.o(.bss), (20 bytes).
    Removing ft5216.o(.data), (1 bytes).
    Removing ft5216.o(.data), (186 bytes).
    Removing inputhz.o(.rev16_text), (4 bytes).
    Removing inputhz.o(.revsh_text), (4 bytes).
    Removing inputhz.o(.rrx_text), (6 bytes).
    Removing inputhz.o(i.Init_PY), (40 bytes).
    Removing inputhz.o(i.Search_py), (172 bytes).
    Removing inputhz.o(.bss), (276 bytes).
    Removing inputhz.o(.constdata), (1 bytes).
    Removing inputhz.o(.constdata), (1 bytes).
    Removing inputhz.o(.conststring), (312 bytes).
    Removing inputhz.o(.conststring), (168 bytes).
    Removing inputhz.o(.conststring), (200 bytes).
    Removing inputhz.o(.conststring), (308 bytes).
    Removing inputhz.o(.conststring), (228 bytes).
    Removing inputhz.o(.conststring), (448 bytes).
    Removing inputhz.o(.conststring), (104 bytes).
    Removing inputhz.o(.conststring), (420 bytes).
    Removing inputhz.o(.data), (880 bytes).
    Removing inputhz.o(.data), (528 bytes).
    Removing inputhz.o(.data), (608 bytes).
    Removing inputhz.o(.data), (912 bytes).
    Removing inputhz.o(.data), (704 bytes).
    Removing inputhz.o(.data), (1264 bytes).
    Removing inputhz.o(.data), (304 bytes).
    Removing inputhz.o(.data), (1184 bytes).
    Removing inputhz.o(.data), (80 bytes).
    Removing lcd.o(.rev16_text), (4 bytes).
    Removing lcd.o(.revsh_text), (4 bytes).
    Removing lcd.o(.rrx_text), (6 bytes).
    Removing pwm.o(.rev16_text), (4 bytes).
    Removing pwm.o(.revsh_text), (4 bytes).
    Removing pwm.o(.rrx_text), (6 bytes).
    Removing pwm.o(i.InitPort), (88 bytes).
    Removing tp.o(.rev16_text), (4 bytes).
    Removing tp.o(.revsh_text), (4 bytes).
    Removing tp.o(.rrx_text), (6 bytes).
    Removing tp.o(i.CtpX), (20 bytes).
    Removing tp.o(i.CtpY), (18 bytes).
    Removing tp.o(i.InitTouch), (128 bytes).
    Removing tp.o(i.IsTouchPressed), (16 bytes).
    Removing tp.o(i.ReadBytes), (28 bytes).
    Removing tp.o(i.ReadTouchData), (66 bytes).
    Removing tp.o(i.ReadTouchData2), (120 bytes).
    Removing tp.o(.bss), (56 bytes).
    Removing tp.o(.data), (7 bytes).
    Removing winbond.o(.rev16_text), (4 bytes).
    Removing winbond.o(.revsh_text), (4 bytes).
    Removing winbond.o(.rrx_text), (6 bytes).
    Removing winbond.o(i.CS_FLash_RESET), (36 bytes).
    Removing winbond.o(i.CS_FLash_SET), (36 bytes).
    Removing winbond.o(i.Check_SSI2_Busy), (20 bytes).
    Removing winbond.o(i.Flash_Enter_QPI), (18 bytes).
    Removing winbond.o(i.SPI5_Dual_Read_Init), (76 bytes).
    Removing winbond.o(i.SPI5_Dual_Read_Init_test), (68 bytes).
    Removing winbond.o(i.SPI5_QPI_Set_DataNum), (30 bytes).
    Removing winbond.o(i.SPI5_Quad_Read_Init), (60 bytes).
    Removing winbond.o(i.SPI5_Quad_Write_Init), (72 bytes).
    Removing winbond.o(i.SPI5_Set_DataNum), (32 bytes).
    Removing winbond.o(i.SSI2_DMA_RX), (212 bytes).
    Removing winbond.o(i.SSI2_DMA_RX_Continue), (224 bytes).
    Removing winbond.o(i.SSI2_DMA_TX), (216 bytes).
    Removing winbond.o(i.SSI2_ReadWriteByte), (24 bytes).
    Removing winbond.o(i.W25N01GV_PageRead_Mode), (22 bytes).
    Removing winbond.o(i.W25NXX_ContinuousRead_Mode), (22 bytes).
    Removing winbond.o(i.W25NXX_EraseFlash), (68 bytes).
    Removing winbond.o(i.W25NXX_Erase_Block), (70 bytes).
    Removing winbond.o(i.W25NXX_ReadID), (56 bytes).
    Removing winbond.o(i.W25NXX_ReadPageAddr_Data_QUAD), (144 bytes).
    Removing winbond.o(i.W25NXX_ReadPageAddr_Data_STD), (112 bytes).
    Removing winbond.o(i.W25NXX_ReadSR), (36 bytes).
    Removing winbond.o(i.W25NXX_Read_NoCheck), (92 bytes).
    Removing winbond.o(i.W25NXX_Wait_Busy), (14 bytes).
    Removing winbond.o(i.W25NXX_WritePageAddr_Data_QUAD), (176 bytes).
    Removing winbond.o(i.W25NXX_WritePageAddr_Data_STD), (124 bytes).
    Removing winbond.o(i.W25NXX_Write_Disable), (20 bytes).
    Removing winbond.o(i.W25NXX_Write_Enable), (20 bytes).
    Removing winbond.o(i.W25NXX_Write_NoCheck), (92 bytes).
    Removing winbond.o(i.W25NXX_Write_SR), (44 bytes).
    Removing winbond.o(i.W25QXX_BlockErase64KB_STD), (72 bytes).
    Removing winbond.o(i.W25QXX_Enter_4Byte_AddressMode_STD), (20 bytes).
    Removing winbond.o(i.W25QXX_Enter_QPI_STD), (20 bytes).
    Removing winbond.o(i.W25QXX_Erase_Chip_STD), (32 bytes).
    Removing winbond.o(i.W25QXX_Open_QUAD), (58 bytes).
    Removing winbond.o(i.W25QXX_ReadID_STD), (62 bytes).
    Removing winbond.o(i.W25QXX_ReadID_STD_9F), (52 bytes).
    Removing winbond.o(i.W25QXX_ReadSR_1_STD), (28 bytes).
    Removing winbond.o(i.W25QXX_Read_DUAL), (84 bytes).
    Removing winbond.o(i.W25QXX_Read_QUAD), (136 bytes).
    Removing winbond.o(i.W25QXX_Read_QUAD_DMA), (88 bytes).
    Removing winbond.o(i.W25QXX_Read_STD), (84 bytes).
    Removing winbond.o(i.W25QXX_SectorErase4KB_STD), (72 bytes).
    Removing winbond.o(i.W25QXX_Wait_Busy_STD), (26 bytes).
    Removing winbond.o(i.W25QXX_Write_Disable_STD), (20 bytes).
    Removing winbond.o(i.W25QXX_Write_Enable_STD), (20 bytes).
    Removing winbond.o(i.W25QXX_Write_NoCheck_QUAD), (62 bytes).
    Removing winbond.o(i.W25QXX_Write_NoCheck_STD), (62 bytes).
    Removing winbond.o(i.W25QXX_Write_Page_QUAD), (144 bytes).
    Removing winbond.o(i.W25QXX_Write_Page_STD), (92 bytes).
    Removing winbond.o(i.Write_Page), (48 bytes).
    Removing winbond.o(.data), (1 bytes).
    Removing rtc.o(.rev16_text), (4 bytes).
    Removing rtc.o(.revsh_text), (4 bytes).
    Removing rtc.o(.rrx_text), (6 bytes).
    Removing dac.o(.rev16_text), (4 bytes).
    Removing dac.o(.revsh_text), (4 bytes).
    Removing dac.o(.rrx_text), (6 bytes).
    Removing dac.o(i.DAC_SetData), (24 bytes).
    Removing dac.o(i.DAC_Wait_Load_Done), (16 bytes).
    Removing dac.o(i.DAC_Write_Data), (12 bytes).
    Removing dac.o(i.LT_PlayWav), (260 bytes).
    Removing dac.o(i.WAV_amplifier_DIS), (24 bytes).
    Removing dac.o(i.WAV_amplifier_EN), (24 bytes).
    Removing dac.o(i.close_wav), (60 bytes).
    Removing dac.o(i.etARRValue), (102 bytes).
    Removing dac_wav.o(.rev16_text), (4 bytes).
    Removing dac_wav.o(.revsh_text), (4 bytes).
    Removing dac_wav.o(.rrx_text), (6 bytes).
    Removing dac_wav.o(i.DMA_REG_Init_my), (48 bytes).
    Removing dac_wav.o(i.DMA_dis), (76 bytes).
    Removing dac_wav.o(i.LT_PlayWav_DAC), (368 bytes).
    Removing dac_wav.o(i.close_wav_dac), (32 bytes).
    Removing debug.o(.rev16_text), (4 bytes).
    Removing debug.o(.revsh_text), (4 bytes).
    Removing debug.o(.rrx_text), (6 bytes).
    Removing debug.o(i.GETCHAR), (40 bytes).
    Removing debug.o(i.HandleUartEvent), (212 bytes).
    Removing debug.o(i.LT_ClearRxBuf), (32 bytes).
    Removing debug.o(i.LT_DataToPc), (120 bytes).
    Removing debug.o(i.LT_DataToPc_NoFrame), (88 bytes).
    Removing debug.o(i.PUTCHAR), (40 bytes).
    Removing debug.o(i.PrintfBuf), (60 bytes).
    Removing debug.o(i.UART1_Init), (80 bytes).
    Removing debug.o(i.UARTRecieved), (24 bytes).
    Removing debug.o(i.UARTRecvByte), (48 bytes).
    Removing debug.o(i._sys_exit), (2 bytes).
    Removing debug.o(i._ttywrch), (2 bytes).
    Removing debug.o(i.assert_failed), (60 bytes).
    Removing debug.o(i.configRtc), (72 bytes).
    Removing debug.o(.data), (2 bytes).
    Removing debug.o(.data), (2 bytes).
    Removing debug.o(.data), (2 bytes).
    Removing debug.o(.data), (1 bytes).
    Removing delay.o(.rev16_text), (4 bytes).
    Removing delay.o(.revsh_text), (4 bytes).
    Removing delay.o(.rrx_text), (6 bytes).
    Removing delay.o(i.Delay_ms), (36 bytes).
    Removing delay.o(i.Delay_us), (32 bytes).
    Removing delay.o(i.GetTickTime), (12 bytes).
    Removing delay.o(i.InitSysTick), (56 bytes).
    Removing delay.o(i.InitTickTime), (16 bytes).
    Removing delay.o(i.SysTick_Handler1), (64 bytes).
    Removing delay.o(i.delay), (12 bytes).
    Removing delay.o(.data), (12 bytes).
    Removing i2c.o(.rev16_text), (4 bytes).
    Removing i2c.o(.revsh_text), (4 bytes).
    Removing i2c.o(.rrx_text), (6 bytes).
    Removing pit.o(.rev16_text), (4 bytes).
    Removing pit.o(.revsh_text), (4 bytes).
    Removing pit.o(.rrx_text), (6 bytes).
    Removing pit.o(i.PIT1_Init), (52 bytes).
    Removing pit.o(i.PIT1_Init_1), (52 bytes).
    Removing clcd_drv.o(.rev16_text), (4 bytes).
    Removing clcd_drv.o(.revsh_text), (4 bytes).
    Removing clcd_drv.o(.rrx_text), (6 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_Deinit), (26 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_Dis), (12 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_En), (12 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_GammaConfig), (28 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_InterruptCmd), (20 bytes).
    Removing clcd_drv.o(i.DRV_CLCD_PaletteConfig), (30 bytes).
    Removing dcmi_drv.o(.rev16_text), (4 bytes).
    Removing dcmi_drv.o(.revsh_text), (4 bytes).
    Removing dcmi_drv.o(.rrx_text), (6 bytes).
    Removing dcmi_drv.o(i.DRV_DCMI_Getgray), (32 bytes).
    Removing dcmi_drv.o(i.DRV_DCMI_Getgray_Edma), (92 bytes).
    Removing dcmi_drv.o(i.DRV_DCMI_Getgray_Idma), (48 bytes).
    Removing dcmi_drv.o(i.DRV_DCMI_Init), (256 bytes).
    Removing dcmi_drv.o(i.dma_dcmi_xfer), (452 bytes).
    Removing dcmi_drv.o(i.dma_dcmi_xfer_mcu_lcd), (176 bytes).
    Removing dcmi_drv.o(i.dma_register_init), (60 bytes).
    Removing dcmi_drv.o(i.dma_wait_for_done), (36 bytes).
    Removing dcmi_drv.o(.bss), (1296 bytes).
    Removing dcmi_drv.o(.data), (4 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_BulkProgram), (32 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_ClrInfoRwAuth), (16 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_ClrUserWriteAuth), (16 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_ClrWritePermission), (12 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_Disboot), (20 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_PageErase), (76 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_RecoveryToBoot), (124 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_SetInfoRwAuth), (16 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_SetTPWS), (28 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_SetUserWriteAuth), (16 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_SetWritePermission), (12 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_UpdateWord), (88 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_UpdateWord_CHIPMODE), (96 bytes).
    Removing lib_eflash.o(i.LIB_EFLASH_WordProg), (16 bytes).
    Removing lib_eflash.o(i.LIB_EFlash_Chip_Mode), (64 bytes).
    Removing lib_eflash.o(i.LIB_GetSerialNumber), (76 bytes).
    Removing lib_eflash.o(i.Lib_GetVersion), (12 bytes).
    Removing event_groups.o(i.vEventGroupClearBitsCallback), (16 bytes).
    Removing event_groups.o(i.vEventGroupDelete), (36 bytes).
    Removing event_groups.o(i.vEventGroupSetBitsCallback), (16 bytes).
    Removing event_groups.o(i.xEventGroupGetBitsFromISR), (44 bytes).
    Removing event_groups.o(i.xEventGroupSync), (168 bytes).
    Removing queue.o(i.uxQueueMessagesWaiting), (18 bytes).
    Removing queue.o(i.uxQueueMessagesWaitingFromISR), (8 bytes).
    Removing queue.o(i.uxQueueSpacesAvailable), (24 bytes).
    Removing queue.o(i.vQueueDelete), (4 bytes).
    Removing queue.o(i.xQueueGenericSendFromISR), (138 bytes).
    Removing queue.o(i.xQueueGiveFromISR), (120 bytes).
    Removing queue.o(i.xQueueIsQueueEmptyFromISR), (16 bytes).
    Removing queue.o(i.xQueueIsQueueFullFromISR), (22 bytes).
    Removing queue.o(i.xQueuePeek), (268 bytes).
    Removing queue.o(i.xQueuePeekFromISR), (74 bytes).
    Removing queue.o(i.xQueueReceiveFromISR), (130 bytes).
    Removing tasks.o(i.pcTaskGetName), (24 bytes).
    Removing tasks.o(i.prvTaskIsTaskSuspended), (64 bytes).
    Removing tasks.o(i.ulTaskGenericNotifyTake), (136 bytes).
    Removing tasks.o(i.ulTaskGenericNotifyValueClear), (64 bytes).
    Removing tasks.o(i.uxTaskGetNumberOfTasks), (12 bytes).
    Removing tasks.o(i.uxTaskPriorityGet), (36 bytes).
    Removing tasks.o(i.uxTaskPriorityGetFromISR), (56 bytes).
    Removing tasks.o(i.vTaskDelete), (212 bytes).
    Removing tasks.o(i.vTaskEndScheduler), (36 bytes).
    Removing tasks.o(i.vTaskGenericNotifyGiveFromISR), (336 bytes).
    Removing tasks.o(i.vTaskPrioritySet), (296 bytes).
    Removing tasks.o(i.vTaskResume), (172 bytes).
    Removing tasks.o(i.vTaskSetTimeOutState), (36 bytes).
    Removing tasks.o(i.vTaskSuspend), (216 bytes).
    Removing tasks.o(i.xTaskCatchUpTicks), (32 bytes).
    Removing tasks.o(i.xTaskDelayUntil), (116 bytes).
    Removing tasks.o(i.xTaskGenericNotify), (332 bytes).
    Removing tasks.o(i.xTaskGenericNotifyFromISR), (504 bytes).
    Removing tasks.o(i.xTaskGenericNotifyStateClear), (64 bytes).
    Removing tasks.o(i.xTaskGenericNotifyWait), (172 bytes).
    Removing tasks.o(i.xTaskGetCurrentTaskHandle), (12 bytes).
    Removing tasks.o(i.xTaskGetTickCount), (12 bytes).
    Removing tasks.o(i.xTaskGetTickCountFromISR), (12 bytes).
    Removing tasks.o(i.xTaskResumeFromISR), (216 bytes).
    Removing list.o(i.vListInsertEnd), (24 bytes).
    Removing port.o(i.vPortEndScheduler), (2 bytes).
    Removing dadd.o(.text), (334 bytes).
    Removing dmul.o(.text), (228 bytes).
    Removing ddiv.o(.text), (222 bytes).
    Removing dfixul.o(.text), (48 bytes).
    Removing cdrcmple.o(.text), (48 bytes).
    Removing depilogue.o(.text), (186 bytes).

1371 unused section(s) (total 89416 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strstr.c         0x00000000   Number         0  strstr.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  useno.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\Src\Drv\libSwithOSC500MHz.c           0x00000000   Number         0  libswithosc500mhz.o ABSOLUTE
    ..\Src\Source\drv\clcd_drv.c             0x00000000   Number         0  clcd_drv.o ABSOLUTE
    ..\Src\Source\drv\dcmi_drv.c             0x00000000   Number         0  dcmi_drv.o ABSOLUTE
    ..\\Src\\Source\\drv\\clcd_drv.c         0x00000000   Number         0  clcd_drv.o ABSOLUTE
    ..\\Src\\Source\\drv\\dcmi_drv.c         0x00000000   Number         0  dcmi_drv.o ABSOLUTE
    BMP\acorn.c                              0x00000000   Number         0  acorn.o ABSOLUTE
    BMP\acorn1.c                             0x00000000   Number         0  acorn1.o ABSOLUTE
    Common\\startup_ARMCM4.s                 0x00000000   Number         0  startup_armcm4.o ABSOLUTE
    Common\\sys.c                            0x00000000   Number         0  sys.o ABSOLUTE
    Common\\system_ARMCM4.c                  0x00000000   Number         0  system_armcm4.o ABSOLUTE
    Common\common.c                          0x00000000   Number         0  common.o ABSOLUTE
    Common\sys.c                             0x00000000   Number         0  sys.o ABSOLUTE
    Common\system_ARMCM4.c                   0x00000000   Number         0  system_armcm4.o ABSOLUTE
    Device\Winbond.c                         0x00000000   Number         0  winbond.o ABSOLUTE
    Device\\Winbond.c                        0x00000000   Number         0  winbond.o ABSOLUTE
    Device\\ft5216.c                         0x00000000   Number         0  ft5216.o ABSOLUTE
    Device\\inputHZ.c                        0x00000000   Number         0  inputhz.o ABSOLUTE
    Device\\lcd.c                            0x00000000   Number         0  lcd.o ABSOLUTE
    Device\\pwm.c                            0x00000000   Number         0  pwm.o ABSOLUTE
    Device\\rtc.c                            0x00000000   Number         0  rtc.o ABSOLUTE
    Device\\tp.c                             0x00000000   Number         0  tp.o ABSOLUTE
    Device\data.c                            0x00000000   Number         0  data.o ABSOLUTE
    Device\font_data.c                       0x00000000   Number         0  font_data.o ABSOLUTE
    Device\ft5216.c                          0x00000000   Number         0  ft5216.o ABSOLUTE
    Device\inputHZ.c                         0x00000000   Number         0  inputhz.o ABSOLUTE
    Device\lcd.c                             0x00000000   Number         0  lcd.o ABSOLUTE
    Device\pwm.c                             0x00000000   Number         0  pwm.o ABSOLUTE
    Device\rtc.c                             0x00000000   Number         0  rtc.o ABSOLUTE
    Device\tp.c                              0x00000000   Number         0  tp.o ABSOLUTE
    Driver\\dac.c                            0x00000000   Number         0  dac.o ABSOLUTE
    Driver\\dac_wav.c                        0x00000000   Number         0  dac_wav.o ABSOLUTE
    Driver\\debug.c                          0x00000000   Number         0  debug.o ABSOLUTE
    Driver\\delay.c                          0x00000000   Number         0  delay.o ABSOLUTE
    Driver\\i2c.c                            0x00000000   Number         0  i2c.o ABSOLUTE
    Driver\\pit.c                            0x00000000   Number         0  pit.o ABSOLUTE
    Driver\dac.c                             0x00000000   Number         0  dac.o ABSOLUTE
    Driver\dac_wav.c                         0x00000000   Number         0  dac_wav.o ABSOLUTE
    Driver\debug.c                           0x00000000   Number         0  debug.o ABSOLUTE
    Driver\delay.c                           0x00000000   Number         0  delay.o ABSOLUTE
    Driver\i2c.c                             0x00000000   Number         0  i2c.o ABSOLUTE
    Driver\pit.c                             0x00000000   Number         0  pit.o ABSOLUTE
    LT776_Graphic\LT776_grac.c               0x00000000   Number         0  lt776_grac.o ABSOLUTE
    LT776_Graphic\misc_c.c                   0x00000000   Number         0  misc_c.o ABSOLUTE
    MCU_drv\\drv\\src\\adc_drv.c             0x00000000   Number         0  adc_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\cache_drv.c           0x00000000   Number         0  cache_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\can_drv.c             0x00000000   Number         0  can_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\cpm_drv.c             0x00000000   Number         0  cpm_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\dac_drv.c             0x00000000   Number         0  dac_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\dma2d_drv.c           0x00000000   Number         0  dma2d_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\dma_drv.c             0x00000000   Number         0  dma_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\edma_drv.c            0x00000000   Number         0  edma_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\eflash_drv.c          0x00000000   Number         0  eflash_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\eport_drv.c           0x00000000   Number         0  eport_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\i2c_drv.c             0x00000000   Number         0  i2c_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\interrupt.c           0x00000000   Number         0  interrupt.o ABSOLUTE
    MCU_drv\\drv\\src\\ioctrl_drv.c          0x00000000   Number         0  ioctrl_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\pit32_drv.c           0x00000000   Number         0  pit32_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\pwm_drv.c             0x00000000   Number         0  pwm_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\reset_drv.c           0x00000000   Number         0  reset_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\rtc_drv.c             0x00000000   Number         0  rtc_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\sdram2lcd_drv.c       0x00000000   Number         0  sdram2lcd_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\sdram_drv.c           0x00000000   Number         0  sdram_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\spi_drv.c             0x00000000   Number         0  spi_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\ssi_drv.c             0x00000000   Number         0  ssi_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\tc_drv.c              0x00000000   Number         0  tc_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\uart_drv.c            0x00000000   Number         0  uart_drv.o ABSOLUTE
    MCU_drv\\drv\\src\\wdt_drv.c             0x00000000   Number         0  wdt_drv.o ABSOLUTE
    MCU_drv\drv\src\adc_drv.c                0x00000000   Number         0  adc_drv.o ABSOLUTE
    MCU_drv\drv\src\cache_drv.c              0x00000000   Number         0  cache_drv.o ABSOLUTE
    MCU_drv\drv\src\can_drv.c                0x00000000   Number         0  can_drv.o ABSOLUTE
    MCU_drv\drv\src\cpm_drv.c                0x00000000   Number         0  cpm_drv.o ABSOLUTE
    MCU_drv\drv\src\dac_drv.c                0x00000000   Number         0  dac_drv.o ABSOLUTE
    MCU_drv\drv\src\dma2d_drv.c              0x00000000   Number         0  dma2d_drv.o ABSOLUTE
    MCU_drv\drv\src\dma_drv.c                0x00000000   Number         0  dma_drv.o ABSOLUTE
    MCU_drv\drv\src\edma_drv.c               0x00000000   Number         0  edma_drv.o ABSOLUTE
    MCU_drv\drv\src\eflash_drv.c             0x00000000   Number         0  eflash_drv.o ABSOLUTE
    MCU_drv\drv\src\eport_drv.c              0x00000000   Number         0  eport_drv.o ABSOLUTE
    MCU_drv\drv\src\i2c_drv.c                0x00000000   Number         0  i2c_drv.o ABSOLUTE
    MCU_drv\drv\src\interrupt.c              0x00000000   Number         0  interrupt.o ABSOLUTE
    MCU_drv\drv\src\ioctrl_drv.c             0x00000000   Number         0  ioctrl_drv.o ABSOLUTE
    MCU_drv\drv\src\pit32_drv.c              0x00000000   Number         0  pit32_drv.o ABSOLUTE
    MCU_drv\drv\src\pwm_drv.c                0x00000000   Number         0  pwm_drv.o ABSOLUTE
    MCU_drv\drv\src\reset_drv.c              0x00000000   Number         0  reset_drv.o ABSOLUTE
    MCU_drv\drv\src\rtc_drv.c                0x00000000   Number         0  rtc_drv.o ABSOLUTE
    MCU_drv\drv\src\sdio_drv.c               0x00000000   Number         0  sdio_drv.o ABSOLUTE
    MCU_drv\drv\src\sdram2lcd_drv.c          0x00000000   Number         0  sdram2lcd_drv.o ABSOLUTE
    MCU_drv\drv\src\sdram_drv.c              0x00000000   Number         0  sdram_drv.o ABSOLUTE
    MCU_drv\drv\src\spi_drv.c                0x00000000   Number         0  spi_drv.o ABSOLUTE
    MCU_drv\drv\src\ssi_drv.c                0x00000000   Number         0  ssi_drv.o ABSOLUTE
    MCU_drv\drv\src\tc_drv.c                 0x00000000   Number         0  tc_drv.o ABSOLUTE
    MCU_drv\drv\src\uart_drv.c               0x00000000   Number         0  uart_drv.o ABSOLUTE
    MCU_drv\drv\src\wdt_drv.c                0x00000000   Number         0  wdt_drv.o ABSOLUTE
    MCU_hal\\hal\\src\\cache_hal.c           0x00000000   Number         0  cache_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\can_hal.c             0x00000000   Number         0  can_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\clcd_hal.c            0x00000000   Number         0  clcd_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\cpm_hal.c             0x00000000   Number         0  cpm_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\dcmi_hal.c            0x00000000   Number         0  dcmi_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\dma2d_hal.c           0x00000000   Number         0  dma2d_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\dma_hal.c             0x00000000   Number         0  dma_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\eflash_hal.c          0x00000000   Number         0  eflash_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\eport_hal.c           0x00000000   Number         0  eport_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\hal.c                 0x00000000   Number         0  hal.o ABSOLUTE
    MCU_hal\\hal\\src\\i2c_hal.c             0x00000000   Number         0  i2c_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\ioctrl_hal.c          0x00000000   Number         0  ioctrl_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\lowpower_hal.c        0x00000000   Number         0  lowpower_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\pit32_hal.c           0x00000000   Number         0  pit32_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\psram_hal.c           0x00000000   Number         0  psram_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\pwm_hal.c             0x00000000   Number         0  pwm_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\reset_hal.c           0x00000000   Number         0  reset_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\rtc_hal.c             0x00000000   Number         0  rtc_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\sdram2lcd_hal.c       0x00000000   Number         0  sdram2lcd_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\sdram_hal.c           0x00000000   Number         0  sdram_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\spi_hal.c             0x00000000   Number         0  spi_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\ssi_hal.c             0x00000000   Number         0  ssi_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\systick_hal.c         0x00000000   Number         0  systick_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\tc_hal.c              0x00000000   Number         0  tc_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\uart_hal.c            0x00000000   Number         0  uart_hal.o ABSOLUTE
    MCU_hal\\hal\\src\\wdt_hal.c             0x00000000   Number         0  wdt_hal.o ABSOLUTE
    MCU_hal\hal\src\cache_hal.c              0x00000000   Number         0  cache_hal.o ABSOLUTE
    MCU_hal\hal\src\can_hal.c                0x00000000   Number         0  can_hal.o ABSOLUTE
    MCU_hal\hal\src\clcd_hal.c               0x00000000   Number         0  clcd_hal.o ABSOLUTE
    MCU_hal\hal\src\cpm_hal.c                0x00000000   Number         0  cpm_hal.o ABSOLUTE
    MCU_hal\hal\src\dcmi_hal.c               0x00000000   Number         0  dcmi_hal.o ABSOLUTE
    MCU_hal\hal\src\dma2d_hal.c              0x00000000   Number         0  dma2d_hal.o ABSOLUTE
    MCU_hal\hal\src\dma_hal.c                0x00000000   Number         0  dma_hal.o ABSOLUTE
    MCU_hal\hal\src\eflash_hal.c             0x00000000   Number         0  eflash_hal.o ABSOLUTE
    MCU_hal\hal\src\eport_hal.c              0x00000000   Number         0  eport_hal.o ABSOLUTE
    MCU_hal\hal\src\hal.c                    0x00000000   Number         0  hal.o ABSOLUTE
    MCU_hal\hal\src\i2c_hal.c                0x00000000   Number         0  i2c_hal.o ABSOLUTE
    MCU_hal\hal\src\ioctrl_hal.c             0x00000000   Number         0  ioctrl_hal.o ABSOLUTE
    MCU_hal\hal\src\lowpower_hal.c           0x00000000   Number         0  lowpower_hal.o ABSOLUTE
    MCU_hal\hal\src\pit32_hal.c              0x00000000   Number         0  pit32_hal.o ABSOLUTE
    MCU_hal\hal\src\psram_hal.c              0x00000000   Number         0  psram_hal.o ABSOLUTE
    MCU_hal\hal\src\pwm_hal.c                0x00000000   Number         0  pwm_hal.o ABSOLUTE
    MCU_hal\hal\src\reset_hal.c              0x00000000   Number         0  reset_hal.o ABSOLUTE
    MCU_hal\hal\src\rtc_hal.c                0x00000000   Number         0  rtc_hal.o ABSOLUTE
    MCU_hal\hal\src\sdcard_hal.c             0x00000000   Number         0  sdcard_hal.o ABSOLUTE
    MCU_hal\hal\src\sdram2lcd_hal.c          0x00000000   Number         0  sdram2lcd_hal.o ABSOLUTE
    MCU_hal\hal\src\sdram_hal.c              0x00000000   Number         0  sdram_hal.o ABSOLUTE
    MCU_hal\hal\src\spi_hal.c                0x00000000   Number         0  spi_hal.o ABSOLUTE
    MCU_hal\hal\src\ssi_hal.c                0x00000000   Number         0  ssi_hal.o ABSOLUTE
    MCU_hal\hal\src\systick_hal.c            0x00000000   Number         0  systick_hal.o ABSOLUTE
    MCU_hal\hal\src\tc_hal.c                 0x00000000   Number         0  tc_hal.o ABSOLUTE
    MCU_hal\hal\src\uart_hal.c               0x00000000   Number         0  uart_hal.o ABSOLUTE
    MCU_hal\hal\src\wdt_hal.c                0x00000000   Number         0  wdt_hal.o ABSOLUTE
    User\\bsp.c                              0x00000000   Number         0  bsp.o ABSOLUTE
    User\\main.c                             0x00000000   Number         0  main.o ABSOLUTE
    User\bsp.c                               0x00000000   Number         0  bsp.o ABSOLUTE
    User\main.c                              0x00000000   Number         0  main.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    lib_eflash.c                             0x00000000   Number         0  lib_eflash.o ABSOLUTE
    src\\port.c                              0x00000000   Number         0  port.o ABSOLUTE
    src\event_groups.c                       0x00000000   Number         0  event_groups.o ABSOLUTE
    src\list.c                               0x00000000   Number         0  list.o ABSOLUTE
    src\port.c                               0x00000000   Number         0  port.o ABSOLUTE
    src\queue.c                              0x00000000   Number         0  queue.o ABSOLUTE
    src\tasks.c                              0x00000000   Number         0  tasks.o ABSOLUTE
    RESET                                    0x08008000   Section      840  startup_armcm4.o(RESET)
    .ARM.Collect$$$$00000000                 0x08008348   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x08008348   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x0800834c   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x08008350   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x08008350   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x08008350   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x08008358   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x08008358   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x08008358   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x08008358   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .emb_text                                0x0800835c   Section      190  port.o(.emb_text)
    $v0                                      0x0800835c   Number         0  port.o(.emb_text)
    .text                                    0x0800841c   Section      148  startup_armcm4.o(.text)
    $v0                                      0x0800841c   Number         0  startup_armcm4.o(.text)
    .text                                    0x080084b0   Section        0  memcpya.o(.text)
    .text                                    0x080084d4   Section        0  memseta.o(.text)
    .text                                    0x080084f8   Section        0  uldiv.o(.text)
    .text                                    0x0800855c   Section       36  init.o(.text)
    .text                                    0x08008580   Section        0  llshl.o(.text)
    .text                                    0x0800859e   Section        0  llushr.o(.text)
    .text                                    0x080085be   Section        0  __dczerorl2.o(.text)
    i.AES_IRQHandler                         0x08008614   Section        0  interrupt.o(i.AES_IRQHandler)
    i.ASYNC_TIMER_IRQHandler                 0x08008616   Section        0  interrupt.o(i.ASYNC_TIMER_IRQHandler)
    i.BusFault_Handler                       0x08008618   Section        0  interrupt.o(i.BusFault_Handler)
    i.CAN0_3_IRQHandler                      0x08008634   Section        0  interrupt.o(i.CAN0_3_IRQHandler)
    i.CAN12_15_IRQHandler                    0x08008636   Section        0  interrupt.o(i.CAN12_15_IRQHandler)
    i.CAN16_31_IRQHandler                    0x08008638   Section        0  interrupt.o(i.CAN16_31_IRQHandler)
    i.CAN32_63_IRQHandler                    0x0800863a   Section        0  interrupt.o(i.CAN32_63_IRQHandler)
    i.CAN4_7_IRQHandler                      0x0800863c   Section        0  interrupt.o(i.CAN4_7_IRQHandler)
    i.CAN8_11_IRQHandler                     0x08008640   Section        0  interrupt.o(i.CAN8_11_IRQHandler)
    i.CLCD_IRQHandler                        0x08008644   Section        0  lcd.o(i.CLCD_IRQHandler)
    i.CTI2C_read_byte                        0x08008664   Section        0  i2c.o(i.CTI2C_read_byte)
    i.CTI2C_start                            0x08008700   Section        0  i2c.o(i.CTI2C_start)
    CTI2C_start                              0x08008701   Thumb Code    68  i2c.o(i.CTI2C_start)
    i.CTI2C_stop                             0x08008748   Section        0  i2c.o(i.CTI2C_stop)
    CTI2C_stop                               0x08008749   Thumb Code    68  i2c.o(i.CTI2C_stop)
    i.CTI2C_write_byte                       0x08008790   Section        0  i2c.o(i.CTI2C_write_byte)
    i.CTP_Init                               0x08008820   Section        0  ft5216.o(i.CTP_Init)
    i.CTP_io_Init                            0x08008838   Section        0  ft5216.o(i.CTP_io_Init)
    i.CT_DELAY_US                            0x08008914   Section        0  i2c.o(i.CT_DELAY_US)
    i.CT_Read_Nbyte                          0x08008926   Section        0  i2c.o(i.CT_Read_Nbyte)
    i.CT_Write_Nbyte                         0x0800898c   Section        0  i2c.o(i.CT_Write_Nbyte)
    i.Canvas_image_width                     0x080089d0   Section        0  bsp.o(i.Canvas_image_width)
    i.ClearScreen                            0x080089dc   Section        0  lt776_grac.o(i.ClearScreen)
    i.ConfigBacklight                        0x080089f0   Section        0  pwm.o(i.ConfigBacklight)
    i.ConfigBeep                             0x08008a04   Section        0  pwm.o(i.ConfigBeep)
    i.DAC_IRQHandler                         0x08008a18   Section        0  interrupt.o(i.DAC_IRQHandler)
    i.DMA1_IRQHandler                        0x08008a1a   Section        0  interrupt.o(i.DMA1_IRQHandler)
    i.DMA2D_IRQHandler                       0x08008a1c   Section        0  interrupt.o(i.DMA2D_IRQHandler)
    i.DMA2_IRQHandler                        0x08008a20   Section        0  dac_wav.o(i.DMA2_IRQHandler)
    i.DMA_DAC_Tran                           0x08008ab0   Section        0  dac_wav.o(i.DMA_DAC_Tran)
    i.DMA_Tran                               0x08008b08   Section        0  dac_wav.o(i.DMA_Tran)
    i.DRV_CAN4_7_Handler                     0x08008b14   Section        0  debug.o(i.DRV_CAN4_7_Handler)
    i.DRV_CLCD_Cmd                           0x08008ce8   Section        0  clcd_drv.o(i.DRV_CLCD_Cmd)
    i.DRV_CLCD_SetClkDiv                     0x08008d04   Section        0  clcd_drv.o(i.DRV_CLCD_SetClkDiv)
    i.DRV_CLCD_SetControlRegister            0x08008d34   Section        0  clcd_drv.o(i.DRV_CLCD_SetControlRegister)
    i.DRV_CLCD_SetTiming0                    0x08008d48   Section        0  clcd_drv.o(i.DRV_CLCD_SetTiming0)
    i.DRV_CLCD_SetTiming1                    0x08008d6e   Section        0  clcd_drv.o(i.DRV_CLCD_SetTiming1)
    i.DRV_CLCD_SetTiming2                    0x08008d90   Section        0  clcd_drv.o(i.DRV_CLCD_SetTiming2)
    i.DRV_CLCD_SetTiming3                    0x08008db4   Section        0  clcd_drv.o(i.DRV_CLCD_SetTiming3)
    i.DRV_CPM_GetCOREClHz                    0x08008dc8   Section        0  cpm_drv.o(i.DRV_CPM_GetCOREClHz)
    i.DRV_CPM_GetIPSClHz                     0x08008e18   Section        0  cpm_drv.o(i.DRV_CPM_GetIPSClHz)
    i.DRV_CPM_GetSDRAMClHz                   0x08008e3c   Section        0  cpm_drv.o(i.DRV_CPM_GetSDRAMClHz)
    i.DRV_CPM_GetSYSClHz                     0x08008e58   Section        0  cpm_drv.o(i.DRV_CPM_GetSYSClHz)
    i.DRV_CPM_SetAdcClkDiv                   0x08008e70   Section        0  cpm_drv.o(i.DRV_CPM_SetAdcClkDiv)
    i.DRV_CPM_SetAhb3ClkDiv                  0x08008e92   Section        0  cpm_drv.o(i.DRV_CPM_SetAhb3ClkDiv)
    i.DRV_CPM_SetArithClkDiv                 0x08008eb4   Section        0  cpm_drv.o(i.DRV_CPM_SetArithClkDiv)
    i.DRV_CPM_SetClcdClkDiv                  0x08008ed6   Section        0  cpm_drv.o(i.DRV_CPM_SetClcdClkDiv)
    i.DRV_CPM_SetClkoutClkDiv                0x08008ef8   Section        0  cpm_drv.o(i.DRV_CPM_SetClkoutClkDiv)
    i.DRV_CPM_SetCoreClkDiv                  0x08008f1a   Section        0  cpm_drv.o(i.DRV_CPM_SetCoreClkDiv)
    i.DRV_CPM_SetDcmi_pixClkDiv              0x08008f30   Section        0  cpm_drv.o(i.DRV_CPM_SetDcmi_pixClkDiv)
    i.DRV_CPM_SetDcmi_sensorClkDiv           0x08008f52   Section        0  cpm_drv.o(i.DRV_CPM_SetDcmi_sensorClkDiv)
    i.DRV_CPM_SetDma2d_sramClkDiv            0x08008f74   Section        0  cpm_drv.o(i.DRV_CPM_SetDma2d_sramClkDiv)
    i.DRV_CPM_SetIpsClkDiv                   0x08008f94   Section        0  cpm_drv.o(i.DRV_CPM_SetIpsClkDiv)
    i.DRV_CPM_SetMccAdrClkDiv                0x08008fb4   Section        0  cpm_drv.o(i.DRV_CPM_SetMccAdrClkDiv)
    i.DRV_CPM_SetMccClkDiv                   0x08008fce   Section        0  cpm_drv.o(i.DRV_CPM_SetMccClkDiv)
    i.DRV_CPM_SetMeshClkDiv                  0x08008fee   Section        0  cpm_drv.o(i.DRV_CPM_SetMeshClkDiv)
    i.DRV_CPM_SetMipi_sampleClkDiv           0x08009010   Section        0  cpm_drv.o(i.DRV_CPM_SetMipi_sampleClkDiv)
    i.DRV_CPM_SetSd_hostClkDiv               0x08009032   Section        0  cpm_drv.o(i.DRV_CPM_SetSd_hostClkDiv)
    i.DRV_CPM_SetSdram2lcdClkDiv             0x08009054   Section        0  cpm_drv.o(i.DRV_CPM_SetSdram2lcdClkDiv)
    i.DRV_CPM_SetSdramClkDiv                 0x08009072   Section        0  cpm_drv.o(i.DRV_CPM_SetSdramClkDiv)
    i.DRV_CPM_SetSdram_smClkDiv              0x08009094   Section        0  cpm_drv.o(i.DRV_CPM_SetSdram_smClkDiv)
    i.DRV_CPM_SetSystemClkDiv                0x080090b6   Section        0  cpm_drv.o(i.DRV_CPM_SetSystemClkDiv)
    i.DRV_CPM_SetTcClkDiv                    0x080090ce   Section        0  cpm_drv.o(i.DRV_CPM_SetTcClkDiv)
    i.DRV_CPM_SetTraceClkDiv                 0x080090ec   Section        0  cpm_drv.o(i.DRV_CPM_SetTraceClkDiv)
    i.DRV_CPM_SystemClkOSC400MSelect         0x0800910e   Section        0  cpm_drv.o(i.DRV_CPM_SystemClkOSC400MSelect)
    i.DRV_CPM_SystemClkOSC480MSelect         0x08009132   Section        0  cpm_drv.o(i.DRV_CPM_SystemClkOSC480MSelect)
    i.DRV_CPM_SystemClkOSC8MSelect           0x08009156   Section        0  cpm_drv.o(i.DRV_CPM_SystemClkOSC8MSelect)
    i.DRV_CPM_SystemClkOSCEXTSelect          0x08009178   Section        0  cpm_drv.o(i.DRV_CPM_SystemClkOSCEXTSelect)
    i.DRV_DCACHE_Init                        0x0800919c   Section        0  cache_drv.o(i.DRV_DCACHE_Init)
    i.DRV_EFM_Init                           0x080092f8   Section        0  eflash_drv.o(i.DRV_EFM_Init)
    i.DRV_EPORT_SetIT                        0x080092fc   Section        0  eport_drv.o(i.DRV_EPORT_SetIT)
    i.DRV_EPORT_SetTriggerMode               0x08009310   Section        0  eport_drv.o(i.DRV_EPORT_SetTriggerMode)
    i.DRV_I2C_GpioInit                       0x080093a6   Section        0  i2c_drv.o(i.DRV_I2C_GpioInit)
    i.DRV_I2C_ReadPin                        0x0800941c   Section        0  i2c_drv.o(i.DRV_I2C_ReadPin)
    i.DRV_ICACHE_Init                        0x0800942c   Section        0  cache_drv.o(i.DRV_ICACHE_Init)
    i.DRV_IOCTRL_SwapDis                     0x08009588   Section        0  ioctrl_drv.o(i.DRV_IOCTRL_SwapDis)
    i.DRV_IOCTRL_SwapEn                      0x08009598   Section        0  ioctrl_drv.o(i.DRV_IOCTRL_SwapEn)
    i.DRV_IOCTRL_SwapintDisable              0x080095a8   Section        0  ioctrl_drv.o(i.DRV_IOCTRL_SwapintDisable)
    i.DRV_IOCTRL_SwapintEn                   0x080095b8   Section        0  ioctrl_drv.o(i.DRV_IOCTRL_SwapintEn)
    i.DRV_PWM_CHxAutoLoadMode                0x080095c8   Section        0  pwm_drv.o(i.DRV_PWM_CHxAutoLoadMode)
    i.DRV_PWM_CHxCmd                         0x08009676   Section        0  pwm_drv.o(i.DRV_PWM_CHxCmd)
    i.DRV_PWM_CHxDeadZoneCmd                 0x08009722   Section        0  pwm_drv.o(i.DRV_PWM_CHxDeadZoneCmd)
    i.DRV_PWM_CHxInverteCmd                  0x08009790   Section        0  pwm_drv.o(i.DRV_PWM_CHxInverteCmd)
    i.DRV_PWM_CHxPullupCmd                   0x08009842   Section        0  pwm_drv.o(i.DRV_PWM_CHxPullupCmd)
    i.DRV_PWM_CHxTimerInterruptCmd           0x080098ee   Section        0  pwm_drv.o(i.DRV_PWM_CHxTimerInterruptCmd)
    i.DRV_PWM_CHxTimerInverteCmd             0x0800999a   Section        0  pwm_drv.o(i.DRV_PWM_CHxTimerInverteCmd)
    i.DRV_PWM_ConfigCHxClkDiv                0x08009a48   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxClkDiv)
    i.DRV_PWM_ConfigCHxDeadZone              0x08009aa8   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxDeadZone)
    i.DRV_PWM_ConfigCHxEdgeinterrupt         0x08009aea   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxEdgeinterrupt)
    i.DRV_PWM_ConfigCHxPeriod                0x08009b50   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxPeriod)
    i.DRV_PWM_ConfigCHxPerscaler             0x08009bb2   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxPerscaler)
    i.DRV_PWM_ConfigCHxWidth                 0x08009bf4   Section        0  pwm_drv.o(i.DRV_PWM_ConfigCHxWidth)
    i.DRV_PWM_SetCHxDirection                0x08009c56   Section        0  pwm_drv.o(i.DRV_PWM_SetCHxDirection)
    i.DRV_PWM_SetCHxLevel                    0x08009d00   Section        0  pwm_drv.o(i.DRV_PWM_SetCHxLevel)
    i.DRV_RTC_GetTimeCounter                 0x08009dac   Section        0  rtc_drv.o(i.DRV_RTC_GetTimeCounter)
    i.DRV_RTC_SetTimeCounter                 0x08009dd4   Section        0  rtc_drv.o(i.DRV_RTC_SetTimeCounter)
    i.DRV_SDRAM_Init                         0x08009df0   Section        0  sdram_drv.o(i.DRV_SDRAM_Init)
    i.DRV_SSI_CS_DisInit                     0x08009e94   Section        0  ssi_drv.o(i.DRV_SSI_CS_DisInit)
    i.DRV_SSI_CS_Init                        0x08009eb8   Section        0  ssi_drv.o(i.DRV_SSI_CS_Init)
    i.DRV_SSI_Cmd                            0x08009ef0   Section        0  ssi_drv.o(i.DRV_SSI_Cmd)
    i.DRV_SSI_GetFlag                        0x08009f04   Section        0  ssi_drv.o(i.DRV_SSI_GetFlag)
    i.DRV_SSI_Init                           0x08009f1c   Section        0  ssi_drv.o(i.DRV_SSI_Init)
    i.DRV_SSI_WaitonFlagTimeout              0x08009fec   Section        0  ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout)
    i.DelayMS                                0x0800a030   Section        0  delay.o(i.DelayMS)
    i.DigitToHexAscii                        0x0800a080   Section        0  misc_c.o(i.DigitToHexAscii)
    i.EFM_IRQHandler                         0x0800a08e   Section        0  interrupt.o(i.EFM_IRQHandler)
    i.ENCR1_IRQHandler                       0x0800a090   Section        0  interrupt.o(i.ENCR1_IRQHandler)
    i.ENCR_IRQHandler                        0x0800a092   Section        0  interrupt.o(i.ENCR_IRQHandler)
    i.EPORT0_0_IRQHandler                    0x0800a094   Section        0  interrupt.o(i.EPORT0_0_IRQHandler)
    i.EPORT0_1_IRQHandler                    0x0800a096   Section        0  interrupt.o(i.EPORT0_1_IRQHandler)
    i.EPORT0_2_IRQHandler                    0x0800a098   Section        0  interrupt.o(i.EPORT0_2_IRQHandler)
    i.EPORT0_3_IRQHandler                    0x0800a09a   Section        0  interrupt.o(i.EPORT0_3_IRQHandler)
    i.EPORT0_4_IRQHandler                    0x0800a09c   Section        0  interrupt.o(i.EPORT0_4_IRQHandler)
    i.EPORT0_5_IRQHandler                    0x0800a0a0   Section        0  ft5216.o(i.EPORT0_5_IRQHandler)
    i.EPORT0_6_IRQHandler                    0x0800a0bc   Section        0  interrupt.o(i.EPORT0_6_IRQHandler)
    i.EPORT0_7_IRQHandler                    0x0800a0be   Section        0  interrupt.o(i.EPORT0_7_IRQHandler)
    i.EPORT10_0_IRQHandler                   0x0800a0c0   Section        0  interrupt.o(i.EPORT10_0_IRQHandler)
    i.EPORT10_1_IRQHandler                   0x0800a0c2   Section        0  interrupt.o(i.EPORT10_1_IRQHandler)
    i.EPORT10_2_IRQHandler                   0x0800a0c4   Section        0  interrupt.o(i.EPORT10_2_IRQHandler)
    i.EPORT10_3_IRQHandler                   0x0800a0c6   Section        0  interrupt.o(i.EPORT10_3_IRQHandler)
    i.EPORT10_4_IRQHandler                   0x0800a0c8   Section        0  interrupt.o(i.EPORT10_4_IRQHandler)
    i.EPORT10_5_IRQHandler                   0x0800a0ca   Section        0  interrupt.o(i.EPORT10_5_IRQHandler)
    i.EPORT10_6_IRQHandler                   0x0800a0cc   Section        0  interrupt.o(i.EPORT10_6_IRQHandler)
    i.EPORT10_7_IRQHandler                   0x0800a0ce   Section        0  interrupt.o(i.EPORT10_7_IRQHandler)
    i.EPORT11_0_IRQHandler                   0x0800a0d0   Section        0  interrupt.o(i.EPORT11_0_IRQHandler)
    i.EPORT11_1_IRQHandler                   0x0800a0d2   Section        0  interrupt.o(i.EPORT11_1_IRQHandler)
    i.EPORT11_2_IRQHandler                   0x0800a0d4   Section        0  interrupt.o(i.EPORT11_2_IRQHandler)
    i.EPORT11_3_IRQHandler                   0x0800a0d6   Section        0  interrupt.o(i.EPORT11_3_IRQHandler)
    i.EPORT11_4_IRQHandler                   0x0800a0d8   Section        0  interrupt.o(i.EPORT11_4_IRQHandler)
    i.EPORT11_5_IRQHandler                   0x0800a0da   Section        0  interrupt.o(i.EPORT11_5_IRQHandler)
    i.EPORT11_6_IRQHandler                   0x0800a0dc   Section        0  interrupt.o(i.EPORT11_6_IRQHandler)
    i.EPORT11_7_IRQHandler                   0x0800a0de   Section        0  interrupt.o(i.EPORT11_7_IRQHandler)
    i.EPORT12_0_IRQHandler                   0x0800a0e0   Section        0  interrupt.o(i.EPORT12_0_IRQHandler)
    i.EPORT12_1_IRQHandler                   0x0800a0e2   Section        0  interrupt.o(i.EPORT12_1_IRQHandler)
    i.EPORT12_2_IRQHandler                   0x0800a0e4   Section        0  interrupt.o(i.EPORT12_2_IRQHandler)
    i.EPORT12_3_IRQHandler                   0x0800a0e6   Section        0  interrupt.o(i.EPORT12_3_IRQHandler)
    i.EPORT12_4_IRQHandler                   0x0800a0e8   Section        0  interrupt.o(i.EPORT12_4_IRQHandler)
    i.EPORT12_5_IRQHandler                   0x0800a0ea   Section        0  interrupt.o(i.EPORT12_5_IRQHandler)
    i.EPORT12_6_IRQHandler                   0x0800a0ec   Section        0  interrupt.o(i.EPORT12_6_IRQHandler)
    i.EPORT12_7_IRQHandler                   0x0800a0ee   Section        0  interrupt.o(i.EPORT12_7_IRQHandler)
    i.EPORT13_0_IRQHandler                   0x0800a0f0   Section        0  interrupt.o(i.EPORT13_0_IRQHandler)
    i.EPORT13_1_IRQHandler                   0x0800a0f2   Section        0  interrupt.o(i.EPORT13_1_IRQHandler)
    i.EPORT13_2_IRQHandler                   0x0800a0f4   Section        0  interrupt.o(i.EPORT13_2_IRQHandler)
    i.EPORT13_3_IRQHandler                   0x0800a0f6   Section        0  interrupt.o(i.EPORT13_3_IRQHandler)
    i.EPORT13_4_IRQHandler                   0x0800a0f8   Section        0  interrupt.o(i.EPORT13_4_IRQHandler)
    i.EPORT13_5_IRQHandler                   0x0800a0fa   Section        0  interrupt.o(i.EPORT13_5_IRQHandler)
    i.EPORT13_6_IRQHandler                   0x0800a0fc   Section        0  interrupt.o(i.EPORT13_6_IRQHandler)
    i.EPORT13_7_IRQHandler                   0x0800a0fe   Section        0  interrupt.o(i.EPORT13_7_IRQHandler)
    i.EPORT14_0_IRQHandler                   0x0800a100   Section        0  interrupt.o(i.EPORT14_0_IRQHandler)
    i.EPORT14_1_IRQHandler                   0x0800a102   Section        0  interrupt.o(i.EPORT14_1_IRQHandler)
    i.EPORT14_2_IRQHandler                   0x0800a104   Section        0  interrupt.o(i.EPORT14_2_IRQHandler)
    i.EPORT14_3_IRQHandler                   0x0800a106   Section        0  interrupt.o(i.EPORT14_3_IRQHandler)
    i.EPORT14_4_IRQHandler                   0x0800a108   Section        0  interrupt.o(i.EPORT14_4_IRQHandler)
    i.EPORT14_5_IRQHandler                   0x0800a10a   Section        0  interrupt.o(i.EPORT14_5_IRQHandler)
    i.EPORT14_6_IRQHandler                   0x0800a10c   Section        0  interrupt.o(i.EPORT14_6_IRQHandler)
    i.EPORT14_7_IRQHandler                   0x0800a10e   Section        0  interrupt.o(i.EPORT14_7_IRQHandler)
    i.EPORT15_0_IRQHandler                   0x0800a110   Section        0  interrupt.o(i.EPORT15_0_IRQHandler)
    i.EPORT15_1_IRQHandler                   0x0800a112   Section        0  interrupt.o(i.EPORT15_1_IRQHandler)
    i.EPORT15_2_IRQHandler                   0x0800a114   Section        0  interrupt.o(i.EPORT15_2_IRQHandler)
    i.EPORT15_3_IRQHandler                   0x0800a116   Section        0  interrupt.o(i.EPORT15_3_IRQHandler)
    i.EPORT15_4_IRQHandler                   0x0800a118   Section        0  interrupt.o(i.EPORT15_4_IRQHandler)
    i.EPORT15_5_IRQHandler                   0x0800a11a   Section        0  interrupt.o(i.EPORT15_5_IRQHandler)
    i.EPORT15_6_IRQHandler                   0x0800a11c   Section        0  interrupt.o(i.EPORT15_6_IRQHandler)
    i.EPORT15_7_IRQHandler                   0x0800a11e   Section        0  interrupt.o(i.EPORT15_7_IRQHandler)
    i.EPORT1_0_IRQHandler                    0x0800a120   Section        0  interrupt.o(i.EPORT1_0_IRQHandler)
    i.EPORT1_1_IRQHandler                    0x0800a122   Section        0  interrupt.o(i.EPORT1_1_IRQHandler)
    i.EPORT1_2_IRQHandler                    0x0800a124   Section        0  interrupt.o(i.EPORT1_2_IRQHandler)
    i.EPORT1_3_IRQHandler                    0x0800a126   Section        0  interrupt.o(i.EPORT1_3_IRQHandler)
    i.EPORT1_4_IRQHandler                    0x0800a128   Section        0  interrupt.o(i.EPORT1_4_IRQHandler)
    i.EPORT1_5_IRQHandler                    0x0800a12a   Section        0  interrupt.o(i.EPORT1_5_IRQHandler)
    i.EPORT1_6_IRQHandler                    0x0800a12c   Section        0  interrupt.o(i.EPORT1_6_IRQHandler)
    i.EPORT1_7_IRQHandler                    0x0800a12e   Section        0  interrupt.o(i.EPORT1_7_IRQHandler)
    i.EPORT2_0_IRQHandler                    0x0800a130   Section        0  interrupt.o(i.EPORT2_0_IRQHandler)
    i.EPORT2_1_IRQHandler                    0x0800a132   Section        0  interrupt.o(i.EPORT2_1_IRQHandler)
    i.EPORT2_2_IRQHandler                    0x0800a134   Section        0  interrupt.o(i.EPORT2_2_IRQHandler)
    i.EPORT2_3_IRQHandler                    0x0800a136   Section        0  interrupt.o(i.EPORT2_3_IRQHandler)
    i.EPORT2_4_IRQHandler                    0x0800a138   Section        0  interrupt.o(i.EPORT2_4_IRQHandler)
    i.EPORT2_5_IRQHandler                    0x0800a13a   Section        0  interrupt.o(i.EPORT2_5_IRQHandler)
    i.EPORT2_6_IRQHandler                    0x0800a13c   Section        0  interrupt.o(i.EPORT2_6_IRQHandler)
    i.EPORT2_7_IRQHandler                    0x0800a13e   Section        0  interrupt.o(i.EPORT2_7_IRQHandler)
    i.EPORT3_0_IRQHandler                    0x0800a140   Section        0  interrupt.o(i.EPORT3_0_IRQHandler)
    i.EPORT3_1_IRQHandler                    0x0800a142   Section        0  interrupt.o(i.EPORT3_1_IRQHandler)
    i.EPORT3_2_IRQHandler                    0x0800a144   Section        0  interrupt.o(i.EPORT3_2_IRQHandler)
    i.EPORT3_3_IRQHandler                    0x0800a146   Section        0  interrupt.o(i.EPORT3_3_IRQHandler)
    i.EPORT3_4_IRQHandler                    0x0800a148   Section        0  interrupt.o(i.EPORT3_4_IRQHandler)
    i.EPORT3_5_IRQHandler                    0x0800a14a   Section        0  interrupt.o(i.EPORT3_5_IRQHandler)
    i.EPORT3_6_IRQHandler                    0x0800a14c   Section        0  interrupt.o(i.EPORT3_6_IRQHandler)
    i.EPORT3_7_IRQHandler                    0x0800a14e   Section        0  interrupt.o(i.EPORT3_7_IRQHandler)
    i.EPORT4_0_IRQHandler                    0x0800a150   Section        0  interrupt.o(i.EPORT4_0_IRQHandler)
    i.EPORT4_1_IRQHandler                    0x0800a152   Section        0  interrupt.o(i.EPORT4_1_IRQHandler)
    i.EPORT4_2_IRQHandler                    0x0800a154   Section        0  interrupt.o(i.EPORT4_2_IRQHandler)
    i.EPORT4_3_IRQHandler                    0x0800a156   Section        0  interrupt.o(i.EPORT4_3_IRQHandler)
    i.EPORT4_4_IRQHandler                    0x0800a158   Section        0  interrupt.o(i.EPORT4_4_IRQHandler)
    i.EPORT4_5_IRQHandler                    0x0800a15a   Section        0  interrupt.o(i.EPORT4_5_IRQHandler)
    i.EPORT4_6_IRQHandler                    0x0800a15c   Section        0  interrupt.o(i.EPORT4_6_IRQHandler)
    i.EPORT4_7_IRQHandler                    0x0800a15e   Section        0  interrupt.o(i.EPORT4_7_IRQHandler)
    i.EPORT5_0_IRQHandler                    0x0800a160   Section        0  interrupt.o(i.EPORT5_0_IRQHandler)
    i.EPORT5_1_IRQHandler                    0x0800a162   Section        0  interrupt.o(i.EPORT5_1_IRQHandler)
    i.EPORT5_2_IRQHandler                    0x0800a164   Section        0  interrupt.o(i.EPORT5_2_IRQHandler)
    i.EPORT5_3_IRQHandler                    0x0800a166   Section        0  interrupt.o(i.EPORT5_3_IRQHandler)
    i.EPORT5_4_IRQHandler                    0x0800a168   Section        0  interrupt.o(i.EPORT5_4_IRQHandler)
    i.EPORT5_5_IRQHandler                    0x0800a16a   Section        0  interrupt.o(i.EPORT5_5_IRQHandler)
    i.EPORT5_6_IRQHandler                    0x0800a16c   Section        0  interrupt.o(i.EPORT5_6_IRQHandler)
    i.EPORT5_7_IRQHandler                    0x0800a16e   Section        0  interrupt.o(i.EPORT5_7_IRQHandler)
    i.EPORT6_0_IRQHandler                    0x0800a170   Section        0  interrupt.o(i.EPORT6_0_IRQHandler)
    i.EPORT6_1_IRQHandler                    0x0800a172   Section        0  interrupt.o(i.EPORT6_1_IRQHandler)
    i.EPORT6_2_IRQHandler                    0x0800a174   Section        0  interrupt.o(i.EPORT6_2_IRQHandler)
    i.EPORT6_3_IRQHandler                    0x0800a176   Section        0  interrupt.o(i.EPORT6_3_IRQHandler)
    i.EPORT6_4_IRQHandler                    0x0800a178   Section        0  interrupt.o(i.EPORT6_4_IRQHandler)
    i.EPORT6_5_IRQHandler                    0x0800a17a   Section        0  interrupt.o(i.EPORT6_5_IRQHandler)
    i.EPORT6_6_IRQHandler                    0x0800a17c   Section        0  interrupt.o(i.EPORT6_6_IRQHandler)
    i.EPORT6_7_IRQHandler                    0x0800a17e   Section        0  interrupt.o(i.EPORT6_7_IRQHandler)
    i.EPORT7_0_IRQHandler                    0x0800a180   Section        0  interrupt.o(i.EPORT7_0_IRQHandler)
    i.EPORT7_1_IRQHandler                    0x0800a182   Section        0  interrupt.o(i.EPORT7_1_IRQHandler)
    i.EPORT7_2_IRQHandler                    0x0800a184   Section        0  interrupt.o(i.EPORT7_2_IRQHandler)
    i.EPORT7_3_IRQHandler                    0x0800a186   Section        0  interrupt.o(i.EPORT7_3_IRQHandler)
    i.EPORT7_4_IRQHandler                    0x0800a188   Section        0  interrupt.o(i.EPORT7_4_IRQHandler)
    i.EPORT7_5_IRQHandler                    0x0800a18a   Section        0  interrupt.o(i.EPORT7_5_IRQHandler)
    i.EPORT7_6_IRQHandler                    0x0800a18c   Section        0  interrupt.o(i.EPORT7_6_IRQHandler)
    i.EPORT7_7_IRQHandler                    0x0800a18e   Section        0  interrupt.o(i.EPORT7_7_IRQHandler)
    i.EPORT8_0_IRQHandler                    0x0800a190   Section        0  interrupt.o(i.EPORT8_0_IRQHandler)
    i.EPORT8_1_IRQHandler                    0x0800a192   Section        0  interrupt.o(i.EPORT8_1_IRQHandler)
    i.EPORT8_2_IRQHandler                    0x0800a194   Section        0  interrupt.o(i.EPORT8_2_IRQHandler)
    i.EPORT8_3_IRQHandler                    0x0800a196   Section        0  interrupt.o(i.EPORT8_3_IRQHandler)
    i.EPORT8_4_IRQHandler                    0x0800a198   Section        0  interrupt.o(i.EPORT8_4_IRQHandler)
    i.EPORT8_5_IRQHandler                    0x0800a19a   Section        0  interrupt.o(i.EPORT8_5_IRQHandler)
    i.EPORT8_6_IRQHandler                    0x0800a19c   Section        0  interrupt.o(i.EPORT8_6_IRQHandler)
    i.EPORT8_7_IRQHandler                    0x0800a19e   Section        0  interrupt.o(i.EPORT8_7_IRQHandler)
    i.EPORT9_0_IRQHandler                    0x0800a1a0   Section        0  interrupt.o(i.EPORT9_0_IRQHandler)
    i.EPORT9_1_IRQHandler                    0x0800a1a2   Section        0  interrupt.o(i.EPORT9_1_IRQHandler)
    i.EPORT9_2_IRQHandler                    0x0800a1a4   Section        0  interrupt.o(i.EPORT9_2_IRQHandler)
    i.EPORT9_3_IRQHandler                    0x0800a1a6   Section        0  interrupt.o(i.EPORT9_3_IRQHandler)
    i.EPORT9_4_IRQHandler                    0x0800a1a8   Section        0  interrupt.o(i.EPORT9_4_IRQHandler)
    i.EPORT9_5_IRQHandler                    0x0800a1aa   Section        0  interrupt.o(i.EPORT9_5_IRQHandler)
    i.EPORT9_6_IRQHandler                    0x0800a1ac   Section        0  interrupt.o(i.EPORT9_6_IRQHandler)
    i.EPORT9_7_IRQHandler                    0x0800a1ae   Section        0  interrupt.o(i.EPORT9_7_IRQHandler)
    i.FT5216_Scan                            0x0800a1b0   Section        0  ft5216.o(i.FT5216_Scan)
    i.HAL_CACHE_Close                        0x0800a1d0   Section        0  cache_hal.o(i.HAL_CACHE_Close)
    i.HAL_CACHE_Init                         0x0800a200   Section        0  cache_hal.o(i.HAL_CACHE_Init)
    i.HAL_CLCD_Init                          0x0800a228   Section        0  clcd_hal.o(i.HAL_CLCD_Init)
    i.HAL_CPM_GETCLCK                        0x0800a2a8   Section        0  cpm_hal.o(i.HAL_CPM_GETCLCK)
    i.HAL_CPM_IRQHandler                     0x0800a2ec   Section        0  cpm_hal.o(i.HAL_CPM_IRQHandler)
    i.HAL_CPM_SSI_SYSCLKConfig               0x0800a3d8   Section        0  cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig)
    i.HAL_CPM_SYSCLKConfig                   0x0800a4c0   Section        0  cpm_hal.o(i.HAL_CPM_SYSCLKConfig)
    i.HAL_CPM_SetCLKDiv                      0x0800a584   Section        0  cpm_hal.o(i.HAL_CPM_SetCLKDiv)
    i.HAL_CPM_SwitchOSC500MHz                0x0800a624   Section        0  libswithosc500mhz.o(i.HAL_CPM_SwitchOSC500MHz)
    i.HAL_EFLASH_Init                        0x0800a6c8   Section        0  eflash_hal.o(i.HAL_EFLASH_Init)
    i.HAL_I2C_GPIOInit                       0x0800a6d4   Section        0  i2c_hal.o(i.HAL_I2C_GPIOInit)
    i.HAL_I2C_GPIOReadPin                    0x0800a6d8   Section        0  i2c_hal.o(i.HAL_I2C_GPIOReadPin)
    i.HAL_IOCTRL_Swap                        0x0800a6de   Section        0  ioctrl_hal.o(i.HAL_IOCTRL_Swap)
    i.HAL_IOCTRL_Swapint                     0x0800a6ea   Section        0  ioctrl_hal.o(i.HAL_IOCTRL_Swapint)
    i.HAL_Init                               0x0800a6f8   Section        0  hal.o(i.HAL_Init)
    i.HAL_PIT32_IRQHandler                   0x0800a748   Section        0  pit32_hal.o(i.HAL_PIT32_IRQHandler)
    i.HAL_PWM_CHxCmd                         0x0800a764   Section        0  pwm_hal.o(i.HAL_PWM_CHxCmd)
    i.HAL_PWM_CaptureCallback                0x0800a76e   Section        0  pwm_hal.o(i.HAL_PWM_CaptureCallback)
    i.HAL_PWM_ConfigCallbackRegistry         0x0800a770   Section        0  pwm_hal.o(i.HAL_PWM_ConfigCallbackRegistry)
    HAL_PWM_ConfigCallbackRegistry           0x0800a771   Thumb Code    28  pwm_hal.o(i.HAL_PWM_ConfigCallbackRegistry)
    i.HAL_PWM_FallingCallback                0x0800a78c   Section        0  pwm_hal.o(i.HAL_PWM_FallingCallback)
    i.HAL_PWM_Init                           0x0800a790   Section        0  pwm_hal.o(i.HAL_PWM_Init)
    i.HAL_PWM_InputInit                      0x0800a7fc   Section        0  pwm_hal.o(i.HAL_PWM_InputInit)
    HAL_PWM_InputInit                        0x0800a7fd   Thumb Code   234  pwm_hal.o(i.HAL_PWM_InputInit)
    i.HAL_PWM_OutputInit                     0x0800a8f4   Section        0  pwm_hal.o(i.HAL_PWM_OutputInit)
    HAL_PWM_OutputInit                       0x0800a8f5   Thumb Code   304  pwm_hal.o(i.HAL_PWM_OutputInit)
    i.HAL_PWM_RisingCallback                 0x0800aa24   Section        0  pwm_hal.o(i.HAL_PWM_RisingCallback)
    i.HAL_SDRAM_Init                         0x0800aa26   Section        0  sdram_hal.o(i.HAL_SDRAM_Init)
    i.HLA_CLCD_Cmd                           0x0800aa7c   Section        0  clcd_hal.o(i.HLA_CLCD_Cmd)
    i.HLA_CLCD_UpuerPannelBaseAddr           0x0800aa82   Section        0  clcd_hal.o(i.HLA_CLCD_UpuerPannelBaseAddr)
    i.HardFault_Handler                      0x0800aa88   Section        0  interrupt.o(i.HardFault_Handler)
    i.I2C1_IRQHandler                        0x0800aaa8   Section        0  interrupt.o(i.I2C1_IRQHandler)
    i.I2C2_IRQHandler                        0x0800aaaa   Section        0  interrupt.o(i.I2C2_IRQHandler)
    i.I2C3_IRQHandler                        0x0800aaac   Section        0  interrupt.o(i.I2C3_IRQHandler)
    i.INTX_ENABLE                            0x0800aaae   Section        0  sys.o(i.INTX_ENABLE)
    i.InitBacklight                          0x0800aab4   Section        0  pwm.o(i.InitBacklight)
    i.InitBeep                               0x0800aaf8   Section        0  pwm.o(i.InitBeep)
    i.InitLcd                                0x0800ab3c   Section        0  lcd.o(i.InitLcd)
    i.Is_Leap_Year                           0x0800ac34   Section        0  rtc.o(i.Is_Leap_Year)
    i.LIB_EFLASH_Init                        0x0800ac5c   Section        0  lib_eflash.o(i.LIB_EFLASH_Init)
    i.LIB_EFLASH_SetMainPermission           0x0800acb8   Section        0  lib_eflash.o(i.LIB_EFLASH_SetMainPermission)
    i.LIB_EFLASH_SetRWSC                     0x0800ad08   Section        0  lib_eflash.o(i.LIB_EFLASH_SetRWSC)
    LIB_EFLASH_SetRWSC                       0x0800ad09   Thumb Code    22  lib_eflash.o(i.LIB_EFLASH_SetRWSC)
    i.LIB_EFLASH_SetVerifyCnt                0x0800ad24   Section        0  lib_eflash.o(i.LIB_EFLASH_SetVerifyCnt)
    i.LT768_DrawPoint                        0x0800ad48   Section        0  bsp.o(i.LT768_DrawPoint)
    i.LT768_TFT_ShowAscii                    0x0800ad60   Section        0  bsp.o(i.LT768_TFT_ShowAscii)
    i.LT768_TFT_Show_Internal_Char           0x0800adc4   Section        0  bsp.o(i.LT768_TFT_Show_Internal_Char)
    i.LT_ReadParam                           0x0800af40   Section        0  bsp.o(i.LT_ReadParam)
    i.LT_RtcInit                             0x0800af8c   Section        0  rtc.o(i.LT_RtcInit)
    i.LT_UsartTimeDisable                    0x0800b034   Section        0  pit.o(i.LT_UsartTimeDisable)
    i.LT_UsartTimeEnable                     0x0800b04c   Section        0  pit.o(i.LT_UsartTimeEnable)
    i.LT_UsartTimeSetCounter                 0x0800b064   Section        0  pit.o(i.LT_UsartTimeSetCounter)
    i.MCC_IRQHandler                         0x0800b078   Section        0  interrupt.o(i.MCC_IRQHandler)
    i.MIPI_IRQHandler                        0x0800b07a   Section        0  interrupt.o(i.MIPI_IRQHandler)
    i.MemManage_Handler                      0x0800b07c   Section        0  interrupt.o(i.MemManage_Handler)
    i.NVIC_Init                              0x0800b09c   Section        0  sys.o(i.NVIC_Init)
    i.NVIC_PriorityGroupConfig               0x0800b0e8   Section        0  sys.o(i.NVIC_PriorityGroupConfig)
    i.PCI_DET_IRQHandler                     0x0800b10c   Section        0  interrupt.o(i.PCI_DET_IRQHandler)
    i.PCI_IRQHandler                         0x0800b10e   Section        0  interrupt.o(i.PCI_IRQHandler)
    i.PIT1_IRQHandler                        0x0800b112   Section        0  pit.o(i.PIT1_IRQHandler)
    i.PIT3_IRQHandler                        0x0800b114   Section        0  interrupt.o(i.PIT3_IRQHandler)
    i.PIT4_IRQHandler                        0x0800b118   Section        0  interrupt.o(i.PIT4_IRQHandler)
    i.PMU_IRQHandler                         0x0800b11c   Section        0  interrupt.o(i.PMU_IRQHandler)
    i.PMU_RTC_IRQHandler                     0x0800b120   Section        0  rtc.o(i.PMU_RTC_IRQHandler)
    i.PWM0_IRQHandler                        0x0800b140   Section        0  interrupt.o(i.PWM0_IRQHandler)
    i.PWM1_IRQHandler                        0x0800b142   Section        0  interrupt.o(i.PWM1_IRQHandler)
    i.PWM2_IRQHandler                        0x0800b144   Section        0  interrupt.o(i.PWM2_IRQHandler)
    i.PWM3_IRQHandler                        0x0800b146   Section        0  interrupt.o(i.PWM3_IRQHandler)
    i.PWM4_IRQHandler                        0x0800b148   Section        0  interrupt.o(i.PWM4_IRQHandler)
    i.PWM5_IRQHandler                        0x0800b14a   Section        0  interrupt.o(i.PWM5_IRQHandler)
    i.PWM6_IRQHandler                        0x0800b14c   Section        0  interrupt.o(i.PWM6_IRQHandler)
    i.PWM7_IRQHandler                        0x0800b14e   Section        0  interrupt.o(i.PWM7_IRQHandler)
    i.PeripheralInit                         0x0800b150   Section        0  main.o(i.PeripheralInit)
    i.Printf_Version                         0x0800b1c8   Section        0  main.o(i.Printf_Version)
    Printf_Version                           0x0800b1c9   Thumb Code    92  main.o(i.Printf_Version)
    i.Put16BitBMP                            0x0800b324   Section        0  lt776_grac.o(i.Put16BitBMP)
    i.QADC_IRQHandler                        0x0800b380   Section        0  interrupt.o(i.QADC_IRQHandler)
    i.RSA_IRQHandler                         0x0800b382   Section        0  interrupt.o(i.RSA_IRQHandler)
    i.RTC_Get                                0x0800b384   Section        0  rtc.o(i.RTC_Get)
    i.RTC_Get_Week                           0x0800b430   Section        0  rtc.o(i.RTC_Get_Week)
    i.RTC_Set                                0x0800b480   Section        0  rtc.o(i.RTC_Set)
    i.SCL_OUTPUT                             0x0800b510   Section        0  i2c.o(i.SCL_OUTPUT)
    i.SDA_INPUT                              0x0800b534   Section        0  i2c.o(i.SDA_INPUT)
    i.SDA_OUTPUT                             0x0800b558   Section        0  i2c.o(i.SDA_OUTPUT)
    i.SEC_PGD_LD_FD_IRQHandler               0x0800b57c   Section        0  interrupt.o(i.SEC_PGD_LD_FD_IRQHandler)
    i.SHA_IRQHandler                         0x0800b57e   Section        0  interrupt.o(i.SHA_IRQHandler)
    i.SMS4_IRQHandler                        0x0800b580   Section        0  interrupt.o(i.SMS4_IRQHandler)
    i.SPI1_IRQHandler                        0x0800b582   Section        0  interrupt.o(i.SPI1_IRQHandler)
    i.SPI2_IRQHandler                        0x0800b584   Section        0  interrupt.o(i.SPI2_IRQHandler)
    i.SPI3_IRQHandler                        0x0800b586   Section        0  interrupt.o(i.SPI3_IRQHandler)
    i.SPI5_STD_Init                          0x0800b588   Section        0  winbond.o(i.SPI5_STD_Init)
    i.SPIM1_IRQHandler                       0x0800b5e4   Section        0  interrupt.o(i.SPIM1_IRQHandler)
    i.SPIM2_IRQHandler                       0x0800b5e6   Section        0  interrupt.o(i.SPIM2_IRQHandler)
    i.SPIM3_IRQHandler                       0x0800b5e8   Section        0  interrupt.o(i.SPIM3_IRQHandler)
    i.Show16BitDecimal                       0x0800b5ea   Section        0  misc_c.o(i.Show16BitDecimal)
    i.SysSsiConfigure                        0x0800b64c   Section        0  ssi_drv.o(i.SysSsiConfigure)
    __tagsym$$used                           0x0800b64d   Number         0  ssi_drv.o(i.SysSsiConfigure)
    i.SysTick_Handler                        0x0800b6f8   Section        0  port.o(i.SysTick_Handler)
    i.SystemInit                             0x0800b72c   Section        0  system_armcm4.o(i.SystemInit)
    i.TC_IRQHandler                          0x0800b75c   Section        0  interrupt.o(i.TC_IRQHandler)
    i.TP_read_XY                             0x0800b760   Section        0  ft5216.o(i.TP_read_XY)
    i.TRNG_IRQHandler                        0x0800b828   Section        0  interrupt.o(i.TRNG_IRQHandler)
    i.TSI_IRQHandler                         0x0800b82a   Section        0  interrupt.o(i.TSI_IRQHandler)
    i.UART1_IRQHandler                       0x0800b82c   Section        0  interrupt.o(i.UART1_IRQHandler)
    i.UART1_IRQHandlerEvent                  0x0800b830   Section        0  debug.o(i.UART1_IRQHandlerEvent)
    i.UART2_IRQHandler                       0x0800b91c   Section        0  interrupt.o(i.UART2_IRQHandler)
    i.UART3_IRQHandler                       0x0800b91e   Section        0  interrupt.o(i.UART3_IRQHandler)
    i.UART4_IRQHandler                       0x0800b920   Section        0  interrupt.o(i.UART4_IRQHandler)
    i.UART_Debug_Init                        0x0800b924   Section        0  debug.o(i.UART_Debug_Init)
    i.USB_IRQHandler                         0x0800b964   Section        0  interrupt.o(i.USB_IRQHandler)
    i.USI3_IRQHandler                        0x0800b966   Section        0  interrupt.o(i.USI3_IRQHandler)
    i.UsageFault_Handler                     0x0800b968   Section        0  interrupt.o(i.UsageFault_Handler)
    i.__0printf$8                            0x0800b988   Section        0  printf8.o(i.__0printf$8)
    i.__scatterload_copy                     0x0800b9a8   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x0800b9b6   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x0800b9b8   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._printf_core                           0x0800b9c8   Section        0  printf8.o(i._printf_core)
    _printf_core                             0x0800b9c9   Thumb Code   996  printf8.o(i._printf_core)
    i._printf_post_padding                   0x0800bdd8   Section        0  printf8.o(i._printf_post_padding)
    _printf_post_padding                     0x0800bdd9   Thumb Code    36  printf8.o(i._printf_post_padding)
    i._printf_pre_padding                    0x0800bdfc   Section        0  printf8.o(i._printf_pre_padding)
    _printf_pre_padding                      0x0800bdfd   Thumb Code    46  printf8.o(i._printf_pre_padding)
    i.fputc                                  0x0800be2c   Section        0  debug.o(i.fputc)
    i.main                                   0x0800be44   Section        0  main.o(i.main)
    i.prvAddCurrentTaskToDelayedList         0x0800be58   Section        0  tasks.o(i.prvAddCurrentTaskToDelayedList)
    prvAddCurrentTaskToDelayedList           0x0800be59   Thumb Code   164  tasks.o(i.prvAddCurrentTaskToDelayedList)
    i.prvAddNewTaskToReadyList               0x0800bf18   Section        0  tasks.o(i.prvAddNewTaskToReadyList)
    prvAddNewTaskToReadyList                 0x0800bf19   Thumb Code   200  tasks.o(i.prvAddNewTaskToReadyList)
    i.prvCheckTasksWaitingTermination        0x0800bffc   Section        0  tasks.o(i.prvCheckTasksWaitingTermination)
    prvCheckTasksWaitingTermination          0x0800bffd   Thumb Code    60  tasks.o(i.prvCheckTasksWaitingTermination)
    i.prvCopyDataFromQueue                   0x0800c044   Section        0  queue.o(i.prvCopyDataFromQueue)
    prvCopyDataFromQueue                     0x0800c045   Thumb Code    42  queue.o(i.prvCopyDataFromQueue)
    i.prvCopyDataToQueue                     0x0800c06e   Section        0  queue.o(i.prvCopyDataToQueue)
    prvCopyDataToQueue                       0x0800c06f   Thumb Code   126  queue.o(i.prvCopyDataToQueue)
    i.prvDeleteTCB                           0x0800c0ec   Section        0  tasks.o(i.prvDeleteTCB)
    prvDeleteTCB                             0x0800c0ed   Thumb Code     2  tasks.o(i.prvDeleteTCB)
    i.prvGetDisinheritPriorityAfterTimeout   0x0800c0ee   Section        0  queue.o(i.prvGetDisinheritPriorityAfterTimeout)
    prvGetDisinheritPriorityAfterTimeout     0x0800c0ef   Thumb Code    20  queue.o(i.prvGetDisinheritPriorityAfterTimeout)
    i.prvIdleTask                            0x0800c104   Section        0  tasks.o(i.prvIdleTask)
    prvIdleTask                              0x0800c105   Thumb Code    32  tasks.o(i.prvIdleTask)
    i.prvInitialiseMutex                     0x0800c12c   Section        0  queue.o(i.prvInitialiseMutex)
    prvInitialiseMutex                       0x0800c12d   Thumb Code    30  queue.o(i.prvInitialiseMutex)
    i.prvInitialiseNewQueue                  0x0800c14a   Section        0  queue.o(i.prvInitialiseNewQueue)
    prvInitialiseNewQueue                    0x0800c14b   Thumb Code    38  queue.o(i.prvInitialiseNewQueue)
    i.prvInitialiseNewTask                   0x0800c170   Section        0  tasks.o(i.prvInitialiseNewTask)
    prvInitialiseNewTask                     0x0800c171   Thumb Code   144  tasks.o(i.prvInitialiseNewTask)
    i.prvInitialiseTaskLists                 0x0800c200   Section        0  tasks.o(i.prvInitialiseTaskLists)
    prvInitialiseTaskLists                   0x0800c201   Thumb Code    70  tasks.o(i.prvInitialiseTaskLists)
    i.prvIsQueueEmpty                        0x0800c268   Section        0  queue.o(i.prvIsQueueEmpty)
    prvIsQueueEmpty                          0x0800c269   Thumb Code    26  queue.o(i.prvIsQueueEmpty)
    i.prvIsQueueFull                         0x0800c282   Section        0  queue.o(i.prvIsQueueFull)
    prvIsQueueFull                           0x0800c283   Thumb Code    30  queue.o(i.prvIsQueueFull)
    i.prvResetNextTaskUnblockTime            0x0800c2a0   Section        0  tasks.o(i.prvResetNextTaskUnblockTime)
    prvResetNextTaskUnblockTime              0x0800c2a1   Thumb Code    40  tasks.o(i.prvResetNextTaskUnblockTime)
    i.prvTaskExitError                       0x0800c2d0   Section        0  port.o(i.prvTaskExitError)
    prvTaskExitError                         0x0800c2d1   Thumb Code    22  port.o(i.prvTaskExitError)
    i.prvTestWaitCondition                   0x0800c2e6   Section        0  event_groups.o(i.prvTestWaitCondition)
    prvTestWaitCondition                     0x0800c2e7   Thumb Code    30  event_groups.o(i.prvTestWaitCondition)
    i.prvUnlockQueue                         0x0800c304   Section        0  queue.o(i.prvUnlockQueue)
    prvUnlockQueue                           0x0800c305   Thumb Code   126  queue.o(i.prvUnlockQueue)
    i.pvTaskIncrementMutexHeldCount          0x0800c384   Section        0  tasks.o(i.pvTaskIncrementMutexHeldCount)
    i.pxPortInitialiseStack                  0x0800c3a4   Section        0  port.o(i.pxPortInitialiseStack)
    i.task_0_entry                           0x0800c3d0   Section        0  main.o(i.task_0_entry)
    i.task_1_entry                           0x0800c468   Section        0  main.o(i.task_1_entry)
    i.task_2_entry                           0x0800c51c   Section        0  main.o(i.task_2_entry)
    i.task_3_and_4_entry                     0x0800c5b8   Section        0  main.o(i.task_3_and_4_entry)
    i.task_5_entry                           0x0800c6a8   Section        0  main.o(i.task_5_entry)
    i.task_6_and_7_entry                     0x0800c754   Section        0  main.o(i.task_6_and_7_entry)
    i.task_touch_entry                       0x0800c840   Section        0  main.o(i.task_touch_entry)
    i.uxListRemove                           0x0800c928   Section        0  list.o(i.uxListRemove)
    i.uxTaskResetEventItemValue              0x0800c950   Section        0  tasks.o(i.uxTaskResetEventItemValue)
    i.vApplicationGetIdleTaskMemory          0x0800c96c   Section        0  main.o(i.vApplicationGetIdleTaskMemory)
    i.vListInitialise                        0x0800c984   Section        0  list.o(i.vListInitialise)
    i.vListInitialiseItem                    0x0800c99e   Section        0  list.o(i.vListInitialiseItem)
    i.vListInsert                            0x0800c9a4   Section        0  list.o(i.vListInsert)
    i.vPortEnterCritical                     0x0800c9d8   Section        0  port.o(i.vPortEnterCritical)
    i.vPortExitCritical                      0x0800c9fc   Section        0  port.o(i.vPortExitCritical)
    i.vPortSetupTimerInterrupt               0x0800ca1c   Section        0  port.o(i.vPortSetupTimerInterrupt)
    i.vTaskDelay                             0x0800ca34   Section        0  tasks.o(i.vTaskDelay)
    i.vTaskInternalSetTimeOutState           0x0800ca68   Section        0  tasks.o(i.vTaskInternalSetTimeOutState)
    i.vTaskMissedYield                       0x0800ca80   Section        0  tasks.o(i.vTaskMissedYield)
    i.vTaskPlaceOnEventList                  0x0800ca8c   Section        0  tasks.o(i.vTaskPlaceOnEventList)
    i.vTaskPlaceOnUnorderedEventList         0x0800caac   Section        0  tasks.o(i.vTaskPlaceOnUnorderedEventList)
    i.vTaskPriorityDisinheritAfterTimeout    0x0800cafc   Section        0  tasks.o(i.vTaskPriorityDisinheritAfterTimeout)
    i.vTaskRemoveFromUnorderedEventList      0x0800cbd0   Section        0  tasks.o(i.vTaskRemoveFromUnorderedEventList)
    i.vTaskStartScheduler                    0x0800cca0   Section        0  tasks.o(i.vTaskStartScheduler)
    i.vTaskSuspendAll                        0x0800cd34   Section        0  tasks.o(i.vTaskSuspendAll)
    i.vTaskSwitchContext                     0x0800cd44   Section        0  tasks.o(i.vTaskSwitchContext)
    i.xEventGroupClearBits                   0x0800cda4   Section        0  event_groups.o(i.xEventGroupClearBits)
    i.xEventGroupCreateStatic                0x0800cdc4   Section        0  event_groups.o(i.xEventGroupCreateStatic)
    i.xEventGroupSetBits                     0x0800cdda   Section        0  event_groups.o(i.xEventGroupSetBits)
    i.xEventGroupWaitBits                    0x0800ce6c   Section        0  event_groups.o(i.xEventGroupWaitBits)
    i.xPortStartScheduler                    0x0800cf38   Section        0  port.o(i.xPortStartScheduler)
    i.xQueueCreateMutexStatic                0x0800cf80   Section        0  queue.o(i.xQueueCreateMutexStatic)
    i.xQueueGenericCreateStatic              0x0800cfaa   Section        0  queue.o(i.xQueueGenericCreateStatic)
    i.xQueueGenericReset                     0x0800cfe4   Section        0  queue.o(i.xQueueGenericReset)
    i.xQueueGenericSend                      0x0800d084   Section        0  queue.o(i.xQueueGenericSend)
    i.xQueueReceive                          0x0800d19c   Section        0  queue.o(i.xQueueReceive)
    i.xQueueSemaphoreTake                    0x0800d2a0   Section        0  queue.o(i.xQueueSemaphoreTake)
    i.xTaskCheckForTimeOut                   0x0800d3d0   Section        0  tasks.o(i.xTaskCheckForTimeOut)
    i.xTaskCreateStatic                      0x0800d430   Section        0  tasks.o(i.xTaskCreateStatic)
    i.xTaskIncrementTick                     0x0800d478   Section        0  tasks.o(i.xTaskIncrementTick)
    i.xTaskPriorityDisinherit                0x0800d608   Section        0  tasks.o(i.xTaskPriorityDisinherit)
    i.xTaskPriorityInherit                   0x0800d6b4   Section        0  tasks.o(i.xTaskPriorityInherit)
    i.xTaskRemoveFromEventList               0x0800d7a0   Section        0  tasks.o(i.xTaskRemoveFromEventList)
    i.xTaskResumeAll                         0x0800d8a8   Section        0  tasks.o(i.xTaskResumeAll)
    i.x_application_define                   0x0800da04   Section        0  main.o(i.x_application_define)
    .constdata                               0x0800dbd8   Section       16  main.o(.constdata)
    .constdata                               0x0800dbe8   Section      216  cpm_hal.o(.constdata)
    .constdata                               0x0800dcc0   Section    32776  acorn.o(.constdata)
    .constdata                               0x08015cc8   Section    32776  acorn1.o(.constdata)
    .constdata                               0x0801dcd0   Section     1520  font_data.o(.constdata)
    .constdata                               0x0801e2c0   Section     3420  font_data.o(.constdata)
    .constdata                               0x0801f01c   Section     6080  font_data.o(.constdata)
    .constdata                               0x080207dc   Section       24  rtc.o(.constdata)
    .conststring                             0x080207f4   Section        5  main.o(.conststring)
    .data                                    0x20000000   Section       56  main.o(.data)
    mutex_handler                            0x20000004   Data           4  main.o(.data)
    queue_handler                            0x20000008   Data           4  main.o(.data)
    sem_handler                              0x2000000c   Data           4  main.o(.data)
    event_handler                            0x20000010   Data           4  main.o(.data)
    .data                                    0x20000038   Section        1  bsp.o(.data)
    .data                                    0x20000039   Section        4  bsp.o(.data)
    .data                                    0x20000040   Section       32  bsp.o(.data)
    .data                                    0x20000060   Section       70  can_drv.o(.data)
    a_TimeSegments                           0x20000070   Data          54  can_drv.o(.data)
    .data                                    0x200000a6   Section        8  can_drv.o(.data)
    .data                                    0x200000b0   Section        8  cpm_drv.o(.data)
    .data                                    0x200000b8   Section        4  cpm_drv.o(.data)
    .data                                    0x200000bc   Section        4  cpm_drv.o(.data)
    .data                                    0x200000c0   Section       12  dma_drv.o(.data)
    .data                                    0x200000cc   Section        8  clcd_hal.o(.data)
    flag                                     0x200000cc   Data           1  clcd_hal.o(.data)
    g_hclcd                                  0x200000d0   Data           4  clcd_hal.o(.data)
    .data                                    0x200000d4   Section        1  cpm_hal.o(.data)
    g_OSC500M_Flg                            0x200000d4   Data           1  cpm_hal.o(.data)
    .data                                    0x200000d8   Section        4  pit32_hal.o(.data)
    g_hpit32                                 0x200000d8   Data           4  pit32_hal.o(.data)
    .data                                    0x200000dc   Section        4  pwm_hal.o(.data)
    g_hpwm                                   0x200000dc   Data           4  pwm_hal.o(.data)
    .data                                    0x200000e0   Section        1  data.o(.data)
    .data                                    0x200000e1   Section        1  data.o(.data)
    .data                                    0x200000e2   Section        2  data.o(.data)
    .data                                    0x200000e4   Section        2  data.o(.data)
    .data                                    0x200000e6   Section        1  ft5216.o(.data)
    .data                                    0x200000e7   Section        1  lcd.o(.data)
    .data                                    0x200000e8   Section       10  rtc.o(.data)
    daycnt                                   0x200000e8   Data           2  rtc.o(.data)
    .data                                    0x200000f2   Section       14  dac_wav.o(.data)
    .data                                    0x20000100   Section       34  debug.o(.data)
    len                                      0x20000102   Data           1  debug.o(.data)
    frameStep                                0x20000103   Data           1  debug.o(.data)
    index                                    0x2000010c   Data           2  debug.o(.data)
    UART                                     0x20000110   Data           4  debug.o(.data)
    gRtcTme                                  0x20000114   Data           6  debug.o(.data)
    .data                                    0x20000124   Section        4  debug.o(.data)
    .data                                    0x20000128   Section       64  tasks.o(.data)
    pxDelayedTaskList                        0x2000012c   Data           4  tasks.o(.data)
    pxOverflowDelayedTaskList                0x20000130   Data           4  tasks.o(.data)
    uxDeletedTasksWaitingCleanUp             0x20000134   Data           4  tasks.o(.data)
    uxCurrentNumberOfTasks                   0x20000138   Data           4  tasks.o(.data)
    xTickCount                               0x2000013c   Data           4  tasks.o(.data)
    uxTopReadyPriority                       0x20000140   Data           4  tasks.o(.data)
    xSchedulerRunning                        0x20000144   Data           4  tasks.o(.data)
    xPendedTicks                             0x20000148   Data           4  tasks.o(.data)
    xYieldPending                            0x2000014c   Data           4  tasks.o(.data)
    xNumOfOverflows                          0x20000150   Data           4  tasks.o(.data)
    uxTaskNumber                             0x20000154   Data           4  tasks.o(.data)
    xNextTaskUnblockTime                     0x20000158   Data           4  tasks.o(.data)
    xIdleTaskHandle                          0x2000015c   Data           4  tasks.o(.data)
    uxSchedulerSuspended                     0x20000164   Data           4  tasks.o(.data)
    .data                                    0x20000168   Section        4  port.o(.data)
    uxCriticalNesting                        0x20000168   Data           4  port.o(.data)
    .bss                                     0x2000016c   Section    21720  main.o(.bss)
    mutex_0                                  0x2000016c   Data          72  main.o(.bss)
    queue_0                                  0x200001b4   Data          72  main.o(.bss)
    semaphore_0                              0x200001fc   Data          72  main.o(.bss)
    eventgroup_0                             0x20000244   Data          24  main.o(.bss)
    task0_buf                                0x20000ab0   Data          84  main.o(.bss)
    task1_buf                                0x20000b04   Data          84  main.o(.bss)
    task2_buf                                0x20000b58   Data          84  main.o(.bss)
    task3_buf                                0x20000bac   Data          84  main.o(.bss)
    task4_buf                                0x20000c00   Data          84  main.o(.bss)
    task5_buf                                0x20000c54   Data          84  main.o(.bss)
    task6_buf                                0x20000ca8   Data          84  main.o(.bss)
    task7_buf                                0x20000cfc   Data          84  main.o(.bss)
    task8_buf                                0x20000d50   Data          84  main.o(.bss)
    task0_stack                              0x20000da4   Data        2048  main.o(.bss)
    task1_stack                              0x200015a4   Data        2048  main.o(.bss)
    task2_stack                              0x20001da4   Data        2048  main.o(.bss)
    task3_stack                              0x200025a4   Data        2048  main.o(.bss)
    task4_stack                              0x20002da4   Data        2048  main.o(.bss)
    task5_stack                              0x200035a4   Data        2048  main.o(.bss)
    task6_stack                              0x20003da4   Data        2048  main.o(.bss)
    task7_stack                              0x200045a4   Data        2048  main.o(.bss)
    touch_stack                              0x20004da4   Data        2048  main.o(.bss)
    .bss                                     0x20005644   Section       36  can_drv.o(.bss)
    .bss                                     0x20005668   Section       16  dma_drv.o(.bss)
    .bss                                     0x20005678   Section     2054  data.o(.bss)
    .bss                                     0x20005e80   Section       52  data.o(.bss)
    .bss                                     0x20005eb4   Section      128  ft5216.o(.bss)
    .bss                                     0x20005f34   Section       48  lcd.o(.bss)
    .bss                                     0x20005f64   Section       72  pwm.o(.bss)
    .bss                                     0x20005fac   Section       36  winbond.o(.bss)
    .bss                                     0x20005fd0   Section     2048  dac_wav.o(.bss)
    .bss                                     0x200067d0   Section     3078  debug.o(.bss)
    .bss                                     0x200073d8   Section       24  lib_eflash.o(.bss)
    eflash_ops                               0x200073d8   Data          24  lib_eflash.o(.bss)
    .bss                                     0x200073f0   Section      200  tasks.o(.bss)
    pxReadyTasksLists                        0x200073f0   Data         100  tasks.o(.bss)
    xDelayedTaskList1                        0x20007454   Data          20  tasks.o(.bss)
    xDelayedTaskList2                        0x20007468   Data          20  tasks.o(.bss)
    xPendingReadyList                        0x2000747c   Data          20  tasks.o(.bss)
    xTasksWaitingTermination                 0x20007490   Data          20  tasks.o(.bss)
    xSuspendedTaskList                       0x200074a4   Data          20  tasks.o(.bss)
    STACK                                    0x200074b8   Section    20480  startup_armcm4.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$VFPi3$EXTD16$VFPS$VFMA$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    __use_no_errno                           0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_exception_handling              0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_fp                              0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_heap                            0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_heap_region                     0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_semihosting                     0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_semihosting_swi                 0x00000000   Number         0  useno.o ABSOLUTE
    __use_no_signal_handling                 0x00000000   Number         0  useno.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x00000348   Number         0  startup_armcm4.o ABSOLUTE
    __Vectors                                0x08008000   Data           4  startup_armcm4.o(RESET)
    __Vectors_End                            0x08008348   Data           0  startup_armcm4.o(RESET)
    __main                                   0x08008349   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x08008349   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x0800834d   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x08008351   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x08008351   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x08008351   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x08008351   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x08008359   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x08008359   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    SVC_Handler                              0x0800835d   Thumb Code    28  port.o(.emb_text)
    __asm___6_port_c_39a90d8d__prvStartFirstTask 0x0800837d   Thumb Code    36  port.o(.emb_text)
    __asm___6_port_c_39a90d8d__prvEnableVFP  0x080083a5   Thumb Code    16  port.o(.emb_text)
    PendSV_Handler                           0x080083b9   Thumb Code    88  port.o(.emb_text)
    vPortGetIPSR                             0x08008415   Thumb Code     6  port.o(.emb_text)
    Reset_Handler                            0x0800841d   Thumb Code   102  startup_armcm4.o(.text)
    NMI_Handler                              0x08008483   Thumb Code     2  startup_armcm4.o(.text)
    DebugMon_Handler                         0x0800848f   Thumb Code     2  startup_armcm4.o(.text)
    CANBOFF_IRQHandler                       0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    CANERR_IRQHandler                        0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    DCMI_IRQHandler                          0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    GMAC_IRQHandler                          0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    I2S_IRQHandler                           0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    PIT2_IRQHandler                          0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    PWMT_IRQHandler                          0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    SDHOST_IRQHandler                        0x08008495   Thumb Code     0  startup_armcm4.o(.text)
    __aeabi_memcpy                           0x080084b1   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x080084b1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x080084b1   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x080084d5   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x080084d5   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x080084d5   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x080084e3   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x080084e3   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x080084e3   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x080084e7   Thumb Code    18  memseta.o(.text)
    __aeabi_uldivmod                         0x080084f9   Thumb Code    98  uldiv.o(.text)
    __scatterload                            0x0800855d   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x0800855d   Thumb Code     0  init.o(.text)
    __aeabi_llsl                             0x08008581   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x08008581   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x0800859f   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x0800859f   Thumb Code     0  llushr.o(.text)
    __decompress                             0x080085bf   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x080085bf   Thumb Code    86  __dczerorl2.o(.text)
    AES_IRQHandler                           0x08008615   Thumb Code     2  interrupt.o(i.AES_IRQHandler)
    ASYNC_TIMER_IRQHandler                   0x08008617   Thumb Code     2  interrupt.o(i.ASYNC_TIMER_IRQHandler)
    BusFault_Handler                         0x08008619   Thumb Code     6  interrupt.o(i.BusFault_Handler)
    CAN0_3_IRQHandler                        0x08008635   Thumb Code     2  interrupt.o(i.CAN0_3_IRQHandler)
    CAN12_15_IRQHandler                      0x08008637   Thumb Code     2  interrupt.o(i.CAN12_15_IRQHandler)
    CAN16_31_IRQHandler                      0x08008639   Thumb Code     2  interrupt.o(i.CAN16_31_IRQHandler)
    CAN32_63_IRQHandler                      0x0800863b   Thumb Code     2  interrupt.o(i.CAN32_63_IRQHandler)
    CAN4_7_IRQHandler                        0x0800863d   Thumb Code     4  interrupt.o(i.CAN4_7_IRQHandler)
    CAN8_11_IRQHandler                       0x08008641   Thumb Code     2  interrupt.o(i.CAN8_11_IRQHandler)
    CLCD_IRQHandler                          0x08008645   Thumb Code    24  lcd.o(i.CLCD_IRQHandler)
    CTI2C_read_byte                          0x08008665   Thumb Code   152  i2c.o(i.CTI2C_read_byte)
    CTI2C_write_byte                         0x08008791   Thumb Code   138  i2c.o(i.CTI2C_write_byte)
    CTP_Init                                 0x08008821   Thumb Code    14  ft5216.o(i.CTP_Init)
    CTP_io_Init                              0x08008839   Thumb Code   212  ft5216.o(i.CTP_io_Init)
    CT_DELAY_US                              0x08008915   Thumb Code    18  i2c.o(i.CT_DELAY_US)
    CT_Read_Nbyte                            0x08008927   Thumb Code   102  i2c.o(i.CT_Read_Nbyte)
    CT_Write_Nbyte                           0x0800898d   Thumb Code    68  i2c.o(i.CT_Write_Nbyte)
    Canvas_image_width                       0x080089d1   Thumb Code     6  bsp.o(i.Canvas_image_width)
    ClearScreen                              0x080089dd   Thumb Code    20  lt776_grac.o(i.ClearScreen)
    ConfigBacklight                          0x080089f1   Thumb Code    14  pwm.o(i.ConfigBacklight)
    ConfigBeep                               0x08008a05   Thumb Code    14  pwm.o(i.ConfigBeep)
    DAC_IRQHandler                           0x08008a19   Thumb Code     2  interrupt.o(i.DAC_IRQHandler)
    DMA1_IRQHandler                          0x08008a1b   Thumb Code     2  interrupt.o(i.DMA1_IRQHandler)
    DMA2D_IRQHandler                         0x08008a1d   Thumb Code     2  interrupt.o(i.DMA2D_IRQHandler)
    DMA2_IRQHandler                          0x08008a21   Thumb Code   124  dac_wav.o(i.DMA2_IRQHandler)
    DMA_DAC_Tran                             0x08008ab1   Thumb Code    72  dac_wav.o(i.DMA_DAC_Tran)
    DMA_Tran                                 0x08008b09   Thumb Code    12  dac_wav.o(i.DMA_Tran)
    DRV_CAN4_7_Handler                       0x08008b15   Thumb Code   432  debug.o(i.DRV_CAN4_7_Handler)
    DRV_CLCD_Cmd                             0x08008ce9   Thumb Code    28  clcd_drv.o(i.DRV_CLCD_Cmd)
    DRV_CLCD_SetClkDiv                       0x08008d05   Thumb Code    48  clcd_drv.o(i.DRV_CLCD_SetClkDiv)
    DRV_CLCD_SetControlRegister              0x08008d35   Thumb Code    20  clcd_drv.o(i.DRV_CLCD_SetControlRegister)
    DRV_CLCD_SetTiming0                      0x08008d49   Thumb Code    38  clcd_drv.o(i.DRV_CLCD_SetTiming0)
    DRV_CLCD_SetTiming1                      0x08008d6f   Thumb Code    34  clcd_drv.o(i.DRV_CLCD_SetTiming1)
    DRV_CLCD_SetTiming2                      0x08008d91   Thumb Code    32  clcd_drv.o(i.DRV_CLCD_SetTiming2)
    DRV_CLCD_SetTiming3                      0x08008db5   Thumb Code    20  clcd_drv.o(i.DRV_CLCD_SetTiming3)
    DRV_CPM_GetCOREClHz                      0x08008dc9   Thumb Code    62  cpm_drv.o(i.DRV_CPM_GetCOREClHz)
    DRV_CPM_GetIPSClHz                       0x08008e19   Thumb Code    32  cpm_drv.o(i.DRV_CPM_GetIPSClHz)
    DRV_CPM_GetSDRAMClHz                     0x08008e3d   Thumb Code    22  cpm_drv.o(i.DRV_CPM_GetSDRAMClHz)
    DRV_CPM_GetSYSClHz                       0x08008e59   Thumb Code    20  cpm_drv.o(i.DRV_CPM_GetSYSClHz)
    DRV_CPM_SetAdcClkDiv                     0x08008e71   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetAdcClkDiv)
    DRV_CPM_SetAhb3ClkDiv                    0x08008e93   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetAhb3ClkDiv)
    DRV_CPM_SetArithClkDiv                   0x08008eb5   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetArithClkDiv)
    DRV_CPM_SetClcdClkDiv                    0x08008ed7   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetClcdClkDiv)
    DRV_CPM_SetClkoutClkDiv                  0x08008ef9   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetClkoutClkDiv)
    DRV_CPM_SetCoreClkDiv                    0x08008f1b   Thumb Code    22  cpm_drv.o(i.DRV_CPM_SetCoreClkDiv)
    DRV_CPM_SetDcmi_pixClkDiv                0x08008f31   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetDcmi_pixClkDiv)
    DRV_CPM_SetDcmi_sensorClkDiv             0x08008f53   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetDcmi_sensorClkDiv)
    DRV_CPM_SetDma2d_sramClkDiv              0x08008f75   Thumb Code    32  cpm_drv.o(i.DRV_CPM_SetDma2d_sramClkDiv)
    DRV_CPM_SetIpsClkDiv                     0x08008f95   Thumb Code    32  cpm_drv.o(i.DRV_CPM_SetIpsClkDiv)
    DRV_CPM_SetMccAdrClkDiv                  0x08008fb5   Thumb Code    26  cpm_drv.o(i.DRV_CPM_SetMccAdrClkDiv)
    DRV_CPM_SetMccClkDiv                     0x08008fcf   Thumb Code    32  cpm_drv.o(i.DRV_CPM_SetMccClkDiv)
    DRV_CPM_SetMeshClkDiv                    0x08008fef   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetMeshClkDiv)
    DRV_CPM_SetMipi_sampleClkDiv             0x08009011   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetMipi_sampleClkDiv)
    DRV_CPM_SetSd_hostClkDiv                 0x08009033   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetSd_hostClkDiv)
    DRV_CPM_SetSdram2lcdClkDiv               0x08009055   Thumb Code    30  cpm_drv.o(i.DRV_CPM_SetSdram2lcdClkDiv)
    DRV_CPM_SetSdramClkDiv                   0x08009073   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetSdramClkDiv)
    DRV_CPM_SetSdram_smClkDiv                0x08009095   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetSdram_smClkDiv)
    DRV_CPM_SetSystemClkDiv                  0x080090b7   Thumb Code    24  cpm_drv.o(i.DRV_CPM_SetSystemClkDiv)
    DRV_CPM_SetTcClkDiv                      0x080090cf   Thumb Code    30  cpm_drv.o(i.DRV_CPM_SetTcClkDiv)
    DRV_CPM_SetTraceClkDiv                   0x080090ed   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SetTraceClkDiv)
    DRV_CPM_SystemClkOSC400MSelect           0x0800910f   Thumb Code    36  cpm_drv.o(i.DRV_CPM_SystemClkOSC400MSelect)
    DRV_CPM_SystemClkOSC480MSelect           0x08009133   Thumb Code    36  cpm_drv.o(i.DRV_CPM_SystemClkOSC480MSelect)
    DRV_CPM_SystemClkOSC8MSelect             0x08009157   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SystemClkOSC8MSelect)
    DRV_CPM_SystemClkOSCEXTSelect            0x08009179   Thumb Code    34  cpm_drv.o(i.DRV_CPM_SystemClkOSCEXTSelect)
    DRV_DCACHE_Init                          0x0800919d   Thumb Code   344  cache_drv.o(i.DRV_DCACHE_Init)
    DRV_EFM_Init                             0x080092f9   Thumb Code     4  eflash_drv.o(i.DRV_EFM_Init)
    DRV_EPORT_SetIT                          0x080092fd   Thumb Code    20  eport_drv.o(i.DRV_EPORT_SetIT)
    DRV_EPORT_SetTriggerMode                 0x08009311   Thumb Code   150  eport_drv.o(i.DRV_EPORT_SetTriggerMode)
    DRV_I2C_GpioInit                         0x080093a7   Thumb Code   118  i2c_drv.o(i.DRV_I2C_GpioInit)
    DRV_I2C_ReadPin                          0x0800941d   Thumb Code    14  i2c_drv.o(i.DRV_I2C_ReadPin)
    DRV_ICACHE_Init                          0x0800942d   Thumb Code   344  cache_drv.o(i.DRV_ICACHE_Init)
    DRV_IOCTRL_SwapDis                       0x08009589   Thumb Code    16  ioctrl_drv.o(i.DRV_IOCTRL_SwapDis)
    DRV_IOCTRL_SwapEn                        0x08009599   Thumb Code    16  ioctrl_drv.o(i.DRV_IOCTRL_SwapEn)
    DRV_IOCTRL_SwapintDisable                0x080095a9   Thumb Code    16  ioctrl_drv.o(i.DRV_IOCTRL_SwapintDisable)
    DRV_IOCTRL_SwapintEn                     0x080095b9   Thumb Code    16  ioctrl_drv.o(i.DRV_IOCTRL_SwapintEn)
    DRV_PWM_CHxAutoLoadMode                  0x080095c9   Thumb Code   174  pwm_drv.o(i.DRV_PWM_CHxAutoLoadMode)
    DRV_PWM_CHxCmd                           0x08009677   Thumb Code   172  pwm_drv.o(i.DRV_PWM_CHxCmd)
    DRV_PWM_CHxDeadZoneCmd                   0x08009723   Thumb Code   110  pwm_drv.o(i.DRV_PWM_CHxDeadZoneCmd)
    DRV_PWM_CHxInverteCmd                    0x08009791   Thumb Code   178  pwm_drv.o(i.DRV_PWM_CHxInverteCmd)
    DRV_PWM_CHxPullupCmd                     0x08009843   Thumb Code   172  pwm_drv.o(i.DRV_PWM_CHxPullupCmd)
    DRV_PWM_CHxTimerInterruptCmd             0x080098ef   Thumb Code   172  pwm_drv.o(i.DRV_PWM_CHxTimerInterruptCmd)
    DRV_PWM_CHxTimerInverteCmd               0x0800999b   Thumb Code   174  pwm_drv.o(i.DRV_PWM_CHxTimerInverteCmd)
    DRV_PWM_ConfigCHxClkDiv                  0x08009a49   Thumb Code    96  pwm_drv.o(i.DRV_PWM_ConfigCHxClkDiv)
    DRV_PWM_ConfigCHxDeadZone                0x08009aa9   Thumb Code    66  pwm_drv.o(i.DRV_PWM_ConfigCHxDeadZone)
    DRV_PWM_ConfigCHxEdgeinterrupt           0x08009aeb   Thumb Code   102  pwm_drv.o(i.DRV_PWM_ConfigCHxEdgeinterrupt)
    DRV_PWM_ConfigCHxPeriod                  0x08009b51   Thumb Code    98  pwm_drv.o(i.DRV_PWM_ConfigCHxPeriod)
    DRV_PWM_ConfigCHxPerscaler               0x08009bb3   Thumb Code    66  pwm_drv.o(i.DRV_PWM_ConfigCHxPerscaler)
    DRV_PWM_ConfigCHxWidth                   0x08009bf5   Thumb Code    98  pwm_drv.o(i.DRV_PWM_ConfigCHxWidth)
    DRV_PWM_SetCHxDirection                  0x08009c57   Thumb Code   170  pwm_drv.o(i.DRV_PWM_SetCHxDirection)
    DRV_PWM_SetCHxLevel                      0x08009d01   Thumb Code   170  pwm_drv.o(i.DRV_PWM_SetCHxLevel)
    DRV_RTC_GetTimeCounter                   0x08009dad   Thumb Code    34  rtc_drv.o(i.DRV_RTC_GetTimeCounter)
    DRV_RTC_SetTimeCounter                   0x08009dd5   Thumb Code    24  rtc_drv.o(i.DRV_RTC_SetTimeCounter)
    DRV_SDRAM_Init                           0x08009df1   Thumb Code   150  sdram_drv.o(i.DRV_SDRAM_Init)
    DRV_SSI_CS_DisInit                       0x08009e95   Thumb Code    34  ssi_drv.o(i.DRV_SSI_CS_DisInit)
    DRV_SSI_CS_Init                          0x08009eb9   Thumb Code    48  ssi_drv.o(i.DRV_SSI_CS_Init)
    DRV_SSI_Cmd                              0x08009ef1   Thumb Code    20  ssi_drv.o(i.DRV_SSI_Cmd)
    DRV_SSI_GetFlag                          0x08009f05   Thumb Code    24  ssi_drv.o(i.DRV_SSI_GetFlag)
    DRV_SSI_Init                             0x08009f1d   Thumb Code   208  ssi_drv.o(i.DRV_SSI_Init)
    DRV_SSI_WaitonFlagTimeout                0x08009fed   Thumb Code    68  ssi_drv.o(i.DRV_SSI_WaitonFlagTimeout)
    DelayMS                                  0x0800a031   Thumb Code    70  delay.o(i.DelayMS)
    DigitToHexAscii                          0x0800a081   Thumb Code    14  misc_c.o(i.DigitToHexAscii)
    EFM_IRQHandler                           0x0800a08f   Thumb Code     2  interrupt.o(i.EFM_IRQHandler)
    ENCR1_IRQHandler                         0x0800a091   Thumb Code     2  interrupt.o(i.ENCR1_IRQHandler)
    ENCR_IRQHandler                          0x0800a093   Thumb Code     2  interrupt.o(i.ENCR_IRQHandler)
    EPORT0_0_IRQHandler                      0x0800a095   Thumb Code     2  interrupt.o(i.EPORT0_0_IRQHandler)
    EPORT0_1_IRQHandler                      0x0800a097   Thumb Code     2  interrupt.o(i.EPORT0_1_IRQHandler)
    EPORT0_2_IRQHandler                      0x0800a099   Thumb Code     2  interrupt.o(i.EPORT0_2_IRQHandler)
    EPORT0_3_IRQHandler                      0x0800a09b   Thumb Code     2  interrupt.o(i.EPORT0_3_IRQHandler)
    EPORT0_4_IRQHandler                      0x0800a09d   Thumb Code     2  interrupt.o(i.EPORT0_4_IRQHandler)
    EPORT0_5_IRQHandler                      0x0800a0a1   Thumb Code    18  ft5216.o(i.EPORT0_5_IRQHandler)
    EPORT0_6_IRQHandler                      0x0800a0bd   Thumb Code     2  interrupt.o(i.EPORT0_6_IRQHandler)
    EPORT0_7_IRQHandler                      0x0800a0bf   Thumb Code     2  interrupt.o(i.EPORT0_7_IRQHandler)
    EPORT10_0_IRQHandler                     0x0800a0c1   Thumb Code     2  interrupt.o(i.EPORT10_0_IRQHandler)
    EPORT10_1_IRQHandler                     0x0800a0c3   Thumb Code     2  interrupt.o(i.EPORT10_1_IRQHandler)
    EPORT10_2_IRQHandler                     0x0800a0c5   Thumb Code     2  interrupt.o(i.EPORT10_2_IRQHandler)
    EPORT10_3_IRQHandler                     0x0800a0c7   Thumb Code     2  interrupt.o(i.EPORT10_3_IRQHandler)
    EPORT10_4_IRQHandler                     0x0800a0c9   Thumb Code     2  interrupt.o(i.EPORT10_4_IRQHandler)
    EPORT10_5_IRQHandler                     0x0800a0cb   Thumb Code     2  interrupt.o(i.EPORT10_5_IRQHandler)
    EPORT10_6_IRQHandler                     0x0800a0cd   Thumb Code     2  interrupt.o(i.EPORT10_6_IRQHandler)
    EPORT10_7_IRQHandler                     0x0800a0cf   Thumb Code     2  interrupt.o(i.EPORT10_7_IRQHandler)
    EPORT11_0_IRQHandler                     0x0800a0d1   Thumb Code     2  interrupt.o(i.EPORT11_0_IRQHandler)
    EPORT11_1_IRQHandler                     0x0800a0d3   Thumb Code     2  interrupt.o(i.EPORT11_1_IRQHandler)
    EPORT11_2_IRQHandler                     0x0800a0d5   Thumb Code     2  interrupt.o(i.EPORT11_2_IRQHandler)
    EPORT11_3_IRQHandler                     0x0800a0d7   Thumb Code     2  interrupt.o(i.EPORT11_3_IRQHandler)
    EPORT11_4_IRQHandler                     0x0800a0d9   Thumb Code     2  interrupt.o(i.EPORT11_4_IRQHandler)
    EPORT11_5_IRQHandler                     0x0800a0db   Thumb Code     2  interrupt.o(i.EPORT11_5_IRQHandler)
    EPORT11_6_IRQHandler                     0x0800a0dd   Thumb Code     2  interrupt.o(i.EPORT11_6_IRQHandler)
    EPORT11_7_IRQHandler                     0x0800a0df   Thumb Code     2  interrupt.o(i.EPORT11_7_IRQHandler)
    EPORT12_0_IRQHandler                     0x0800a0e1   Thumb Code     2  interrupt.o(i.EPORT12_0_IRQHandler)
    EPORT12_1_IRQHandler                     0x0800a0e3   Thumb Code     2  interrupt.o(i.EPORT12_1_IRQHandler)
    EPORT12_2_IRQHandler                     0x0800a0e5   Thumb Code     2  interrupt.o(i.EPORT12_2_IRQHandler)
    EPORT12_3_IRQHandler                     0x0800a0e7   Thumb Code     2  interrupt.o(i.EPORT12_3_IRQHandler)
    EPORT12_4_IRQHandler                     0x0800a0e9   Thumb Code     2  interrupt.o(i.EPORT12_4_IRQHandler)
    EPORT12_5_IRQHandler                     0x0800a0eb   Thumb Code     2  interrupt.o(i.EPORT12_5_IRQHandler)
    EPORT12_6_IRQHandler                     0x0800a0ed   Thumb Code     2  interrupt.o(i.EPORT12_6_IRQHandler)
    EPORT12_7_IRQHandler                     0x0800a0ef   Thumb Code     2  interrupt.o(i.EPORT12_7_IRQHandler)
    EPORT13_0_IRQHandler                     0x0800a0f1   Thumb Code     2  interrupt.o(i.EPORT13_0_IRQHandler)
    EPORT13_1_IRQHandler                     0x0800a0f3   Thumb Code     2  interrupt.o(i.EPORT13_1_IRQHandler)
    EPORT13_2_IRQHandler                     0x0800a0f5   Thumb Code     2  interrupt.o(i.EPORT13_2_IRQHandler)
    EPORT13_3_IRQHandler                     0x0800a0f7   Thumb Code     2  interrupt.o(i.EPORT13_3_IRQHandler)
    EPORT13_4_IRQHandler                     0x0800a0f9   Thumb Code     2  interrupt.o(i.EPORT13_4_IRQHandler)
    EPORT13_5_IRQHandler                     0x0800a0fb   Thumb Code     2  interrupt.o(i.EPORT13_5_IRQHandler)
    EPORT13_6_IRQHandler                     0x0800a0fd   Thumb Code     2  interrupt.o(i.EPORT13_6_IRQHandler)
    EPORT13_7_IRQHandler                     0x0800a0ff   Thumb Code     2  interrupt.o(i.EPORT13_7_IRQHandler)
    EPORT14_0_IRQHandler                     0x0800a101   Thumb Code     2  interrupt.o(i.EPORT14_0_IRQHandler)
    EPORT14_1_IRQHandler                     0x0800a103   Thumb Code     2  interrupt.o(i.EPORT14_1_IRQHandler)
    EPORT14_2_IRQHandler                     0x0800a105   Thumb Code     2  interrupt.o(i.EPORT14_2_IRQHandler)
    EPORT14_3_IRQHandler                     0x0800a107   Thumb Code     2  interrupt.o(i.EPORT14_3_IRQHandler)
    EPORT14_4_IRQHandler                     0x0800a109   Thumb Code     2  interrupt.o(i.EPORT14_4_IRQHandler)
    EPORT14_5_IRQHandler                     0x0800a10b   Thumb Code     2  interrupt.o(i.EPORT14_5_IRQHandler)
    EPORT14_6_IRQHandler                     0x0800a10d   Thumb Code     2  interrupt.o(i.EPORT14_6_IRQHandler)
    EPORT14_7_IRQHandler                     0x0800a10f   Thumb Code     2  interrupt.o(i.EPORT14_7_IRQHandler)
    EPORT15_0_IRQHandler                     0x0800a111   Thumb Code     2  interrupt.o(i.EPORT15_0_IRQHandler)
    EPORT15_1_IRQHandler                     0x0800a113   Thumb Code     2  interrupt.o(i.EPORT15_1_IRQHandler)
    EPORT15_2_IRQHandler                     0x0800a115   Thumb Code     2  interrupt.o(i.EPORT15_2_IRQHandler)
    EPORT15_3_IRQHandler                     0x0800a117   Thumb Code     2  interrupt.o(i.EPORT15_3_IRQHandler)
    EPORT15_4_IRQHandler                     0x0800a119   Thumb Code     2  interrupt.o(i.EPORT15_4_IRQHandler)
    EPORT15_5_IRQHandler                     0x0800a11b   Thumb Code     2  interrupt.o(i.EPORT15_5_IRQHandler)
    EPORT15_6_IRQHandler                     0x0800a11d   Thumb Code     2  interrupt.o(i.EPORT15_6_IRQHandler)
    EPORT15_7_IRQHandler                     0x0800a11f   Thumb Code     2  interrupt.o(i.EPORT15_7_IRQHandler)
    EPORT1_0_IRQHandler                      0x0800a121   Thumb Code     2  interrupt.o(i.EPORT1_0_IRQHandler)
    EPORT1_1_IRQHandler                      0x0800a123   Thumb Code     2  interrupt.o(i.EPORT1_1_IRQHandler)
    EPORT1_2_IRQHandler                      0x0800a125   Thumb Code     2  interrupt.o(i.EPORT1_2_IRQHandler)
    EPORT1_3_IRQHandler                      0x0800a127   Thumb Code     2  interrupt.o(i.EPORT1_3_IRQHandler)
    EPORT1_4_IRQHandler                      0x0800a129   Thumb Code     2  interrupt.o(i.EPORT1_4_IRQHandler)
    EPORT1_5_IRQHandler                      0x0800a12b   Thumb Code     2  interrupt.o(i.EPORT1_5_IRQHandler)
    EPORT1_6_IRQHandler                      0x0800a12d   Thumb Code     2  interrupt.o(i.EPORT1_6_IRQHandler)
    EPORT1_7_IRQHandler                      0x0800a12f   Thumb Code     2  interrupt.o(i.EPORT1_7_IRQHandler)
    EPORT2_0_IRQHandler                      0x0800a131   Thumb Code     2  interrupt.o(i.EPORT2_0_IRQHandler)
    EPORT2_1_IRQHandler                      0x0800a133   Thumb Code     2  interrupt.o(i.EPORT2_1_IRQHandler)
    EPORT2_2_IRQHandler                      0x0800a135   Thumb Code     2  interrupt.o(i.EPORT2_2_IRQHandler)
    EPORT2_3_IRQHandler                      0x0800a137   Thumb Code     2  interrupt.o(i.EPORT2_3_IRQHandler)
    EPORT2_4_IRQHandler                      0x0800a139   Thumb Code     2  interrupt.o(i.EPORT2_4_IRQHandler)
    EPORT2_5_IRQHandler                      0x0800a13b   Thumb Code     2  interrupt.o(i.EPORT2_5_IRQHandler)
    EPORT2_6_IRQHandler                      0x0800a13d   Thumb Code     2  interrupt.o(i.EPORT2_6_IRQHandler)
    EPORT2_7_IRQHandler                      0x0800a13f   Thumb Code     2  interrupt.o(i.EPORT2_7_IRQHandler)
    EPORT3_0_IRQHandler                      0x0800a141   Thumb Code     2  interrupt.o(i.EPORT3_0_IRQHandler)
    EPORT3_1_IRQHandler                      0x0800a143   Thumb Code     2  interrupt.o(i.EPORT3_1_IRQHandler)
    EPORT3_2_IRQHandler                      0x0800a145   Thumb Code     2  interrupt.o(i.EPORT3_2_IRQHandler)
    EPORT3_3_IRQHandler                      0x0800a147   Thumb Code     2  interrupt.o(i.EPORT3_3_IRQHandler)
    EPORT3_4_IRQHandler                      0x0800a149   Thumb Code     2  interrupt.o(i.EPORT3_4_IRQHandler)
    EPORT3_5_IRQHandler                      0x0800a14b   Thumb Code     2  interrupt.o(i.EPORT3_5_IRQHandler)
    EPORT3_6_IRQHandler                      0x0800a14d   Thumb Code     2  interrupt.o(i.EPORT3_6_IRQHandler)
    EPORT3_7_IRQHandler                      0x0800a14f   Thumb Code     2  interrupt.o(i.EPORT3_7_IRQHandler)
    EPORT4_0_IRQHandler                      0x0800a151   Thumb Code     2  interrupt.o(i.EPORT4_0_IRQHandler)
    EPORT4_1_IRQHandler                      0x0800a153   Thumb Code     2  interrupt.o(i.EPORT4_1_IRQHandler)
    EPORT4_2_IRQHandler                      0x0800a155   Thumb Code     2  interrupt.o(i.EPORT4_2_IRQHandler)
    EPORT4_3_IRQHandler                      0x0800a157   Thumb Code     2  interrupt.o(i.EPORT4_3_IRQHandler)
    EPORT4_4_IRQHandler                      0x0800a159   Thumb Code     2  interrupt.o(i.EPORT4_4_IRQHandler)
    EPORT4_5_IRQHandler                      0x0800a15b   Thumb Code     2  interrupt.o(i.EPORT4_5_IRQHandler)
    EPORT4_6_IRQHandler                      0x0800a15d   Thumb Code     2  interrupt.o(i.EPORT4_6_IRQHandler)
    EPORT4_7_IRQHandler                      0x0800a15f   Thumb Code     2  interrupt.o(i.EPORT4_7_IRQHandler)
    EPORT5_0_IRQHandler                      0x0800a161   Thumb Code     2  interrupt.o(i.EPORT5_0_IRQHandler)
    EPORT5_1_IRQHandler                      0x0800a163   Thumb Code     2  interrupt.o(i.EPORT5_1_IRQHandler)
    EPORT5_2_IRQHandler                      0x0800a165   Thumb Code     2  interrupt.o(i.EPORT5_2_IRQHandler)
    EPORT5_3_IRQHandler                      0x0800a167   Thumb Code     2  interrupt.o(i.EPORT5_3_IRQHandler)
    EPORT5_4_IRQHandler                      0x0800a169   Thumb Code     2  interrupt.o(i.EPORT5_4_IRQHandler)
    EPORT5_5_IRQHandler                      0x0800a16b   Thumb Code     2  interrupt.o(i.EPORT5_5_IRQHandler)
    EPORT5_6_IRQHandler                      0x0800a16d   Thumb Code     2  interrupt.o(i.EPORT5_6_IRQHandler)
    EPORT5_7_IRQHandler                      0x0800a16f   Thumb Code     2  interrupt.o(i.EPORT5_7_IRQHandler)
    EPORT6_0_IRQHandler                      0x0800a171   Thumb Code     2  interrupt.o(i.EPORT6_0_IRQHandler)
    EPORT6_1_IRQHandler                      0x0800a173   Thumb Code     2  interrupt.o(i.EPORT6_1_IRQHandler)
    EPORT6_2_IRQHandler                      0x0800a175   Thumb Code     2  interrupt.o(i.EPORT6_2_IRQHandler)
    EPORT6_3_IRQHandler                      0x0800a177   Thumb Code     2  interrupt.o(i.EPORT6_3_IRQHandler)
    EPORT6_4_IRQHandler                      0x0800a179   Thumb Code     2  interrupt.o(i.EPORT6_4_IRQHandler)
    EPORT6_5_IRQHandler                      0x0800a17b   Thumb Code     2  interrupt.o(i.EPORT6_5_IRQHandler)
    EPORT6_6_IRQHandler                      0x0800a17d   Thumb Code     2  interrupt.o(i.EPORT6_6_IRQHandler)
    EPORT6_7_IRQHandler                      0x0800a17f   Thumb Code     2  interrupt.o(i.EPORT6_7_IRQHandler)
    EPORT7_0_IRQHandler                      0x0800a181   Thumb Code     2  interrupt.o(i.EPORT7_0_IRQHandler)
    EPORT7_1_IRQHandler                      0x0800a183   Thumb Code     2  interrupt.o(i.EPORT7_1_IRQHandler)
    EPORT7_2_IRQHandler                      0x0800a185   Thumb Code     2  interrupt.o(i.EPORT7_2_IRQHandler)
    EPORT7_3_IRQHandler                      0x0800a187   Thumb Code     2  interrupt.o(i.EPORT7_3_IRQHandler)
    EPORT7_4_IRQHandler                      0x0800a189   Thumb Code     2  interrupt.o(i.EPORT7_4_IRQHandler)
    EPORT7_5_IRQHandler                      0x0800a18b   Thumb Code     2  interrupt.o(i.EPORT7_5_IRQHandler)
    EPORT7_6_IRQHandler                      0x0800a18d   Thumb Code     2  interrupt.o(i.EPORT7_6_IRQHandler)
    EPORT7_7_IRQHandler                      0x0800a18f   Thumb Code     2  interrupt.o(i.EPORT7_7_IRQHandler)
    EPORT8_0_IRQHandler                      0x0800a191   Thumb Code     2  interrupt.o(i.EPORT8_0_IRQHandler)
    EPORT8_1_IRQHandler                      0x0800a193   Thumb Code     2  interrupt.o(i.EPORT8_1_IRQHandler)
    EPORT8_2_IRQHandler                      0x0800a195   Thumb Code     2  interrupt.o(i.EPORT8_2_IRQHandler)
    EPORT8_3_IRQHandler                      0x0800a197   Thumb Code     2  interrupt.o(i.EPORT8_3_IRQHandler)
    EPORT8_4_IRQHandler                      0x0800a199   Thumb Code     2  interrupt.o(i.EPORT8_4_IRQHandler)
    EPORT8_5_IRQHandler                      0x0800a19b   Thumb Code     2  interrupt.o(i.EPORT8_5_IRQHandler)
    EPORT8_6_IRQHandler                      0x0800a19d   Thumb Code     2  interrupt.o(i.EPORT8_6_IRQHandler)
    EPORT8_7_IRQHandler                      0x0800a19f   Thumb Code     2  interrupt.o(i.EPORT8_7_IRQHandler)
    EPORT9_0_IRQHandler                      0x0800a1a1   Thumb Code     2  interrupt.o(i.EPORT9_0_IRQHandler)
    EPORT9_1_IRQHandler                      0x0800a1a3   Thumb Code     2  interrupt.o(i.EPORT9_1_IRQHandler)
    EPORT9_2_IRQHandler                      0x0800a1a5   Thumb Code     2  interrupt.o(i.EPORT9_2_IRQHandler)
    EPORT9_3_IRQHandler                      0x0800a1a7   Thumb Code     2  interrupt.o(i.EPORT9_3_IRQHandler)
    EPORT9_4_IRQHandler                      0x0800a1a9   Thumb Code     2  interrupt.o(i.EPORT9_4_IRQHandler)
    EPORT9_5_IRQHandler                      0x0800a1ab   Thumb Code     2  interrupt.o(i.EPORT9_5_IRQHandler)
    EPORT9_6_IRQHandler                      0x0800a1ad   Thumb Code     2  interrupt.o(i.EPORT9_6_IRQHandler)
    EPORT9_7_IRQHandler                      0x0800a1af   Thumb Code     2  interrupt.o(i.EPORT9_7_IRQHandler)
    FT5216_Scan                              0x0800a1b1   Thumb Code    26  ft5216.o(i.FT5216_Scan)
    HAL_CACHE_Close                          0x0800a1d1   Thumb Code    48  cache_hal.o(i.HAL_CACHE_Close)
    HAL_CACHE_Init                           0x0800a201   Thumb Code    40  cache_hal.o(i.HAL_CACHE_Init)
    HAL_CLCD_Init                            0x0800a229   Thumb Code   122  clcd_hal.o(i.HAL_CLCD_Init)
    HAL_CPM_GETCLCK                          0x0800a2a9   Thumb Code    46  cpm_hal.o(i.HAL_CPM_GETCLCK)
    HAL_CPM_IRQHandler                       0x0800a2ed   Thumb Code   166  cpm_hal.o(i.HAL_CPM_IRQHandler)
    HAL_CPM_SSI_SYSCLKConfig                 0x0800a3d9   Thumb Code   198  cpm_hal.o(i.HAL_CPM_SSI_SYSCLKConfig)
    HAL_CPM_SYSCLKConfig                     0x0800a4c1   Thumb Code   170  cpm_hal.o(i.HAL_CPM_SYSCLKConfig)
    HAL_CPM_SetCLKDiv                        0x0800a585   Thumb Code   158  cpm_hal.o(i.HAL_CPM_SetCLKDiv)
    HAL_CPM_SwitchOSC500MHz                  0x0800a625   Thumb Code   152  libswithosc500mhz.o(i.HAL_CPM_SwitchOSC500MHz)
    HAL_EFLASH_Init                          0x0800a6c9   Thumb Code    12  eflash_hal.o(i.HAL_EFLASH_Init)
    HAL_I2C_GPIOInit                         0x0800a6d5   Thumb Code     4  i2c_hal.o(i.HAL_I2C_GPIOInit)
    HAL_I2C_GPIOReadPin                      0x0800a6d9   Thumb Code     6  i2c_hal.o(i.HAL_I2C_GPIOReadPin)
    HAL_IOCTRL_Swap                          0x0800a6df   Thumb Code    12  ioctrl_hal.o(i.HAL_IOCTRL_Swap)
    HAL_IOCTRL_Swapint                       0x0800a6eb   Thumb Code    12  ioctrl_hal.o(i.HAL_IOCTRL_Swapint)
    HAL_Init                                 0x0800a6f9   Thumb Code    70  hal.o(i.HAL_Init)
    HAL_PIT32_IRQHandler                     0x0800a749   Thumb Code    24  pit32_hal.o(i.HAL_PIT32_IRQHandler)
    HAL_PWM_CHxCmd                           0x0800a765   Thumb Code    10  pwm_hal.o(i.HAL_PWM_CHxCmd)
    HAL_PWM_CaptureCallback                  0x0800a76f   Thumb Code     2  pwm_hal.o(i.HAL_PWM_CaptureCallback)
    HAL_PWM_FallingCallback                  0x0800a78d   Thumb Code     2  pwm_hal.o(i.HAL_PWM_FallingCallback)
    HAL_PWM_Init                             0x0800a791   Thumb Code   104  pwm_hal.o(i.HAL_PWM_Init)
    HAL_PWM_RisingCallback                   0x0800aa25   Thumb Code     2  pwm_hal.o(i.HAL_PWM_RisingCallback)
    HAL_SDRAM_Init                           0x0800aa27   Thumb Code    86  sdram_hal.o(i.HAL_SDRAM_Init)
    HLA_CLCD_Cmd                             0x0800aa7d   Thumb Code     6  clcd_hal.o(i.HLA_CLCD_Cmd)
    HLA_CLCD_UpuerPannelBaseAddr             0x0800aa83   Thumb Code     6  clcd_hal.o(i.HLA_CLCD_UpuerPannelBaseAddr)
    HardFault_Handler                        0x0800aa89   Thumb Code     6  interrupt.o(i.HardFault_Handler)
    I2C1_IRQHandler                          0x0800aaa9   Thumb Code     2  interrupt.o(i.I2C1_IRQHandler)
    I2C2_IRQHandler                          0x0800aaab   Thumb Code     2  interrupt.o(i.I2C2_IRQHandler)
    I2C3_IRQHandler                          0x0800aaad   Thumb Code     2  interrupt.o(i.I2C3_IRQHandler)
    INTX_ENABLE                              0x0800aaaf   Thumb Code     4  sys.o(i.INTX_ENABLE)
    InitBacklight                            0x0800aab5   Thumb Code    60  pwm.o(i.InitBacklight)
    InitBeep                                 0x0800aaf9   Thumb Code    60  pwm.o(i.InitBeep)
    InitLcd                                  0x0800ab3d   Thumb Code   192  lcd.o(i.InitLcd)
    Is_Leap_Year                             0x0800ac35   Thumb Code    38  rtc.o(i.Is_Leap_Year)
    LIB_EFLASH_Init                          0x0800ac5d   Thumb Code    76  lib_eflash.o(i.LIB_EFLASH_Init)
    LIB_EFLASH_SetMainPermission             0x0800acb9   Thumb Code    72  lib_eflash.o(i.LIB_EFLASH_SetMainPermission)
    LIB_EFLASH_SetVerifyCnt                  0x0800ad25   Thumb Code    30  lib_eflash.o(i.LIB_EFLASH_SetVerifyCnt)
    LT768_DrawPoint                          0x0800ad49   Thumb Code    20  bsp.o(i.LT768_DrawPoint)
    LT768_TFT_ShowAscii                      0x0800ad61   Thumb Code    96  bsp.o(i.LT768_TFT_ShowAscii)
    LT768_TFT_Show_Internal_Char             0x0800adc5   Thumb Code   364  bsp.o(i.LT768_TFT_Show_Internal_Char)
    LT_ReadParam                             0x0800af41   Thumb Code    70  bsp.o(i.LT_ReadParam)
    LT_RtcInit                               0x0800af8d   Thumb Code   148  rtc.o(i.LT_RtcInit)
    LT_UsartTimeDisable                      0x0800b035   Thumb Code    20  pit.o(i.LT_UsartTimeDisable)
    LT_UsartTimeEnable                       0x0800b04d   Thumb Code    20  pit.o(i.LT_UsartTimeEnable)
    LT_UsartTimeSetCounter                   0x0800b065   Thumb Code    16  pit.o(i.LT_UsartTimeSetCounter)
    MCC_IRQHandler                           0x0800b079   Thumb Code     2  interrupt.o(i.MCC_IRQHandler)
    MIPI_IRQHandler                          0x0800b07b   Thumb Code     2  interrupt.o(i.MIPI_IRQHandler)
    MemManage_Handler                        0x0800b07d   Thumb Code     6  interrupt.o(i.MemManage_Handler)
    NVIC_Init                                0x0800b09d   Thumb Code    74  sys.o(i.NVIC_Init)
    NVIC_PriorityGroupConfig                 0x0800b0e9   Thumb Code    26  sys.o(i.NVIC_PriorityGroupConfig)
    PCI_DET_IRQHandler                       0x0800b10d   Thumb Code     2  interrupt.o(i.PCI_DET_IRQHandler)
    PCI_IRQHandler                           0x0800b10f   Thumb Code     4  interrupt.o(i.PCI_IRQHandler)
    PIT1_IRQHandler                          0x0800b113   Thumb Code     2  pit.o(i.PIT1_IRQHandler)
    PIT3_IRQHandler                          0x0800b115   Thumb Code     4  interrupt.o(i.PIT3_IRQHandler)
    PIT4_IRQHandler                          0x0800b119   Thumb Code     4  interrupt.o(i.PIT4_IRQHandler)
    PMU_IRQHandler                           0x0800b11d   Thumb Code     2  interrupt.o(i.PMU_IRQHandler)
    PMU_RTC_IRQHandler                       0x0800b121   Thumb Code    24  rtc.o(i.PMU_RTC_IRQHandler)
    PWM0_IRQHandler                          0x0800b141   Thumb Code     2  interrupt.o(i.PWM0_IRQHandler)
    PWM1_IRQHandler                          0x0800b143   Thumb Code     2  interrupt.o(i.PWM1_IRQHandler)
    PWM2_IRQHandler                          0x0800b145   Thumb Code     2  interrupt.o(i.PWM2_IRQHandler)
    PWM3_IRQHandler                          0x0800b147   Thumb Code     2  interrupt.o(i.PWM3_IRQHandler)
    PWM4_IRQHandler                          0x0800b149   Thumb Code     2  interrupt.o(i.PWM4_IRQHandler)
    PWM5_IRQHandler                          0x0800b14b   Thumb Code     2  interrupt.o(i.PWM5_IRQHandler)
    PWM6_IRQHandler                          0x0800b14d   Thumb Code     2  interrupt.o(i.PWM6_IRQHandler)
    PWM7_IRQHandler                          0x0800b14f   Thumb Code     2  interrupt.o(i.PWM7_IRQHandler)
    PeripheralInit                           0x0800b151   Thumb Code   108  main.o(i.PeripheralInit)
    Put16BitBMP                              0x0800b325   Thumb Code    92  lt776_grac.o(i.Put16BitBMP)
    QADC_IRQHandler                          0x0800b381   Thumb Code     2  interrupt.o(i.QADC_IRQHandler)
    RSA_IRQHandler                           0x0800b383   Thumb Code     2  interrupt.o(i.RSA_IRQHandler)
    RTC_Get                                  0x0800b385   Thumb Code   162  rtc.o(i.RTC_Get)
    RTC_Get_Week                             0x0800b431   Thumb Code    76  rtc.o(i.RTC_Get_Week)
    RTC_Set                                  0x0800b481   Thumb Code   138  rtc.o(i.RTC_Set)
    SCL_OUTPUT                               0x0800b511   Thumb Code    32  i2c.o(i.SCL_OUTPUT)
    SDA_INPUT                                0x0800b535   Thumb Code    32  i2c.o(i.SDA_INPUT)
    SDA_OUTPUT                               0x0800b559   Thumb Code    30  i2c.o(i.SDA_OUTPUT)
    SEC_PGD_LD_FD_IRQHandler                 0x0800b57d   Thumb Code     2  interrupt.o(i.SEC_PGD_LD_FD_IRQHandler)
    SHA_IRQHandler                           0x0800b57f   Thumb Code     2  interrupt.o(i.SHA_IRQHandler)
    SMS4_IRQHandler                          0x0800b581   Thumb Code     2  interrupt.o(i.SMS4_IRQHandler)
    SPI1_IRQHandler                          0x0800b583   Thumb Code     2  interrupt.o(i.SPI1_IRQHandler)
    SPI2_IRQHandler                          0x0800b585   Thumb Code     2  interrupt.o(i.SPI2_IRQHandler)
    SPI3_IRQHandler                          0x0800b587   Thumb Code     2  interrupt.o(i.SPI3_IRQHandler)
    SPI5_STD_Init                            0x0800b589   Thumb Code    84  winbond.o(i.SPI5_STD_Init)
    SPIM1_IRQHandler                         0x0800b5e5   Thumb Code     2  interrupt.o(i.SPIM1_IRQHandler)
    SPIM2_IRQHandler                         0x0800b5e7   Thumb Code     2  interrupt.o(i.SPIM2_IRQHandler)
    SPIM3_IRQHandler                         0x0800b5e9   Thumb Code     2  interrupt.o(i.SPIM3_IRQHandler)
    Show16BitDecimal                         0x0800b5eb   Thumb Code    96  misc_c.o(i.Show16BitDecimal)
    SysSsiConfigure                          0x0800b64d   Thumb Code   164  ssi_drv.o(i.SysSsiConfigure)
    SysTick_Handler                          0x0800b6f9   Thumb Code    46  port.o(i.SysTick_Handler)
    SystemInit                               0x0800b72d   Thumb Code    40  system_armcm4.o(i.SystemInit)
    TC_IRQHandler                            0x0800b75d   Thumb Code     2  interrupt.o(i.TC_IRQHandler)
    TP_read_XY                               0x0800b761   Thumb Code   178  ft5216.o(i.TP_read_XY)
    TRNG_IRQHandler                          0x0800b829   Thumb Code     2  interrupt.o(i.TRNG_IRQHandler)
    TSI_IRQHandler                           0x0800b82b   Thumb Code     2  interrupt.o(i.TSI_IRQHandler)
    UART1_IRQHandler                         0x0800b82d   Thumb Code     4  interrupt.o(i.UART1_IRQHandler)
    UART1_IRQHandlerEvent                    0x0800b831   Thumb Code   208  debug.o(i.UART1_IRQHandlerEvent)
    UART2_IRQHandler                         0x0800b91d   Thumb Code     2  interrupt.o(i.UART2_IRQHandler)
    UART3_IRQHandler                         0x0800b91f   Thumb Code     2  interrupt.o(i.UART3_IRQHandler)
    UART4_IRQHandler                         0x0800b921   Thumb Code     2  interrupt.o(i.UART4_IRQHandler)
    UART_Debug_Init                          0x0800b925   Thumb Code    56  debug.o(i.UART_Debug_Init)
    USB_IRQHandler                           0x0800b965   Thumb Code     2  interrupt.o(i.USB_IRQHandler)
    USI3_IRQHandler                          0x0800b967   Thumb Code     2  interrupt.o(i.USI3_IRQHandler)
    UsageFault_Handler                       0x0800b969   Thumb Code     6  interrupt.o(i.UsageFault_Handler)
    __0printf$8                              0x0800b989   Thumb Code    22  printf8.o(i.__0printf$8)
    __1printf$8                              0x0800b989   Thumb Code     0  printf8.o(i.__0printf$8)
    __2printf                                0x0800b989   Thumb Code     0  printf8.o(i.__0printf$8)
    __scatterload_copy                       0x0800b9a9   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x0800b9b7   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x0800b9b9   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    fputc                                    0x0800be2d   Thumb Code    20  debug.o(i.fputc)
    main                                     0x0800be45   Thumb Code    18  main.o(i.main)
    pvTaskIncrementMutexHeldCount            0x0800c385   Thumb Code    26  tasks.o(i.pvTaskIncrementMutexHeldCount)
    pxPortInitialiseStack                    0x0800c3a5   Thumb Code    38  port.o(i.pxPortInitialiseStack)
    task_0_entry                             0x0800c3d1   Thumb Code   126  main.o(i.task_0_entry)
    task_1_entry                             0x0800c469   Thumb Code   152  main.o(i.task_1_entry)
    task_2_entry                             0x0800c51d   Thumb Code   134  main.o(i.task_2_entry)
    task_3_and_4_entry                       0x0800c5b9   Thumb Code   216  main.o(i.task_3_and_4_entry)
    task_5_entry                             0x0800c6a9   Thumb Code   148  main.o(i.task_5_entry)
    task_6_and_7_entry                       0x0800c755   Thumb Code   216  main.o(i.task_6_and_7_entry)
    task_touch_entry                         0x0800c841   Thumb Code   202  main.o(i.task_touch_entry)
    uxListRemove                             0x0800c929   Thumb Code    40  list.o(i.uxListRemove)
    uxTaskResetEventItemValue                0x0800c951   Thumb Code    24  tasks.o(i.uxTaskResetEventItemValue)
    vApplicationGetIdleTaskMemory            0x0800c96d   Thumb Code    18  main.o(i.vApplicationGetIdleTaskMemory)
    vListInitialise                          0x0800c985   Thumb Code    26  list.o(i.vListInitialise)
    vListInitialiseItem                      0x0800c99f   Thumb Code     6  list.o(i.vListInitialiseItem)
    vListInsert                              0x0800c9a5   Thumb Code    52  list.o(i.vListInsert)
    vPortEnterCritical                       0x0800c9d9   Thumb Code    30  port.o(i.vPortEnterCritical)
    vPortExitCritical                        0x0800c9fd   Thumb Code    28  port.o(i.vPortExitCritical)
    vPortSetupTimerInterrupt                 0x0800ca1d   Thumb Code    20  port.o(i.vPortSetupTimerInterrupt)
    vTaskDelay                               0x0800ca35   Thumb Code    46  tasks.o(i.vTaskDelay)
    vTaskInternalSetTimeOutState             0x0800ca69   Thumb Code    14  tasks.o(i.vTaskInternalSetTimeOutState)
    vTaskMissedYield                         0x0800ca81   Thumb Code     8  tasks.o(i.vTaskMissedYield)
    vTaskPlaceOnEventList                    0x0800ca8d   Thumb Code    28  tasks.o(i.vTaskPlaceOnEventList)
    vTaskPlaceOnUnorderedEventList           0x0800caad   Thumb Code    74  tasks.o(i.vTaskPlaceOnUnorderedEventList)
    vTaskPriorityDisinheritAfterTimeout      0x0800cafd   Thumb Code   204  tasks.o(i.vTaskPriorityDisinheritAfterTimeout)
    vTaskRemoveFromUnorderedEventList        0x0800cbd1   Thumb Code   190  tasks.o(i.vTaskRemoveFromUnorderedEventList)
    vTaskStartScheduler                      0x0800cca1   Thumb Code   114  tasks.o(i.vTaskStartScheduler)
    vTaskSuspendAll                          0x0800cd35   Thumb Code    12  tasks.o(i.vTaskSuspendAll)
    vTaskSwitchContext                       0x0800cd45   Thumb Code    76  tasks.o(i.vTaskSwitchContext)
    xEventGroupClearBits                     0x0800cda5   Thumb Code    32  event_groups.o(i.xEventGroupClearBits)
    xEventGroupCreateStatic                  0x0800cdc5   Thumb Code    22  event_groups.o(i.xEventGroupCreateStatic)
    xEventGroupSetBits                       0x0800cddb   Thumb Code   146  event_groups.o(i.xEventGroupSetBits)
    xEventGroupWaitBits                      0x0800ce6d   Thumb Code   198  event_groups.o(i.xEventGroupWaitBits)
    xPortStartScheduler                      0x0800cf39   Thumb Code    58  port.o(i.xPortStartScheduler)
    xQueueCreateMutexStatic                  0x0800cf81   Thumb Code    42  queue.o(i.xQueueCreateMutexStatic)
    xQueueGenericCreateStatic                0x0800cfab   Thumb Code    56  queue.o(i.xQueueGenericCreateStatic)
    xQueueGenericReset                       0x0800cfe5   Thumb Code   156  queue.o(i.xQueueGenericReset)
    xQueueGenericSend                        0x0800d085   Thumb Code   276  queue.o(i.xQueueGenericSend)
    xQueueReceive                            0x0800d19d   Thumb Code   256  queue.o(i.xQueueReceive)
    xQueueSemaphoreTake                      0x0800d2a1   Thumb Code   300  queue.o(i.xQueueSemaphoreTake)
    xTaskCheckForTimeOut                     0x0800d3d1   Thumb Code    88  tasks.o(i.xTaskCheckForTimeOut)
    xTaskCreateStatic                        0x0800d431   Thumb Code    72  tasks.o(i.xTaskCreateStatic)
    xTaskIncrementTick                       0x0800d479   Thumb Code   356  tasks.o(i.xTaskIncrementTick)
    xTaskPriorityDisinherit                  0x0800d609   Thumb Code   162  tasks.o(i.xTaskPriorityDisinherit)
    xTaskPriorityInherit                     0x0800d6b5   Thumb Code   224  tasks.o(i.xTaskPriorityInherit)
    xTaskRemoveFromEventList                 0x0800d7a1   Thumb Code   240  tasks.o(i.xTaskRemoveFromEventList)
    xTaskResumeAll                           0x0800d8a9   Thumb Code   310  tasks.o(i.xTaskResumeAll)
    x_application_define                     0x0800da05   Thumb Code   288  main.o(i.x_application_define)
    updata_bin_data                          0x0800dbe8   Data         216  cpm_hal.o(.constdata)
    BMP_Acorn                                0x0800dcc0   Data       32776  acorn.o(.constdata)
    BMP_Acorn1                               0x08015cc8   Data       32776  acorn1.o(.constdata)
    asc2_1608                                0x0801dcd0   Data        1520  font_data.o(.constdata)
    asc2_2412                                0x0801e2c0   Data        3420  font_data.o(.constdata)
    asc2_3216                                0x0801f01c   Data        6080  font_data.o(.constdata)
    table_week                               0x080207dc   Data          12  rtc.o(.constdata)
    mon_table                                0x080207e8   Data          12  rtc.o(.constdata)
    Region$$Table$$Base                      0x080207fc   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x0802081c   Number         0  anon$$obj.o(Region$$Table)
    version                                  0x20000000   Data           4  main.o(.data)
    task_0_counter                           0x20000014   Data           4  main.o(.data)
    task_1_counter                           0x20000018   Data           4  main.o(.data)
    task_2_counter                           0x2000001c   Data           4  main.o(.data)
    task_3_counter                           0x20000020   Data           4  main.o(.data)
    task_4_counter                           0x20000024   Data           4  main.o(.data)
    task_5_counter                           0x20000028   Data           4  main.o(.data)
    task_6_counter                           0x2000002c   Data           4  main.o(.data)
    task_7_counter                           0x20000030   Data           4  main.o(.data)
    task_touch_counter                       0x20000034   Data           4  main.o(.data)
    FF_Update_Flag                           0x20000038   Data           1  bsp.o(.data)
    ENDBYTE_Buf                              0x20000039   Data           4  bsp.o(.data)
    Flash_type                               0x20000040   Data           1  bsp.o(.data)
    gPCLKRISING                              0x20000041   Data           1  bsp.o(.data)
    gHSYNCPolarity                           0x20000042   Data           1  bsp.o(.data)
    gVSYNCPolarity                           0x20000043   Data           1  bsp.o(.data)
    gDEPolarity                              0x20000044   Data           1  bsp.o(.data)
    LCD_XSIZE_TFT                            0x20000046   Data           2  bsp.o(.data)
    LCD_YSIZE_TFT                            0x20000048   Data           2  bsp.o(.data)
    LCD_VBPD                                 0x2000004a   Data           2  bsp.o(.data)
    LCD_VFPD                                 0x2000004c   Data           2  bsp.o(.data)
    LCD_VSPW                                 0x2000004e   Data           2  bsp.o(.data)
    LCD_HBPD                                 0x20000050   Data           2  bsp.o(.data)
    LCD_HFPD                                 0x20000052   Data           2  bsp.o(.data)
    LCD_HSPW                                 0x20000054   Data           2  bsp.o(.data)
    Lay_Canvas_Width                         0x20000056   Data           2  bsp.o(.data)
    Lay_Canvas_Addr                          0x20000058   Data           4  bsp.o(.data)
    gBaudrate                                0x2000005c   Data           4  bsp.o(.data)
    gCanIFlag1                               0x20000060   Data           4  can_drv.o(.data)
    gCanIFlag2                               0x20000064   Data           4  can_drv.o(.data)
    gCanFifoEnable                           0x20000068   Data           4  can_drv.o(.data)
    gCanFifoRxLen                            0x2000006c   Data           4  can_drv.o(.data)
    canDataBuf                               0x200000a6   Data           8  can_drv.o(.data)
    g_core_clk                               0x200000b0   Data           4  cpm_drv.o(.data)
    g_sys_clk                                0x200000b4   Data           4  cpm_drv.o(.data)
    g_ips_clk                                0x200000b8   Data           4  cpm_drv.o(.data)
    g_sdram_clk                              0x200000bc   Data           4  cpm_drv.o(.data)
    DMA_CHX                                  0x200000c0   Data           1  dma_drv.o(.data)
    dma_isr_flag                             0x200000c4   Data           4  dma_drv.o(.data)
    m_dma_control                            0x200000c8   Data           4  dma_drv.o(.data)
    First_press                              0x200000e0   Data           1  data.o(.data)
    wbuf_select                              0x200000e1   Data           1  data.o(.data)
    First_pressX                             0x200000e2   Data           2  data.o(.data)
    First_pressY                             0x200000e4   Data           2  data.o(.data)
    ctp_active_index                         0x200000e6   Data           1  ft5216.o(.data)
    LCD_frame_flag                           0x200000e7   Data           1  lcd.o(.data)
    calendar                                 0x200000ea   Data           8  rtc.o(.data)
    finishflag                               0x200000f2   Data           1  dac_wav.o(.data)
    last_select                              0x200000f3   Data           1  dac_wav.o(.data)
    bufflen                                  0x200000f4   Data           2  dac_wav.o(.data)
    numflag                                  0x200000f6   Data           2  dac_wav.o(.data)
    buffnum                                  0x200000f8   Data           2  dac_wav.o(.data)
    bufflast                                 0x200000fa   Data           2  dac_wav.o(.data)
    hdac                                     0x200000fc   Data           4  dac_wav.o(.data)
    Frame_AA_OK                              0x20000100   Data           1  debug.o(.data)
    can_count                                0x20000101   Data           1  debug.o(.data)
    Rx_Count_short                           0x20000104   Data           2  debug.o(.data)
    Rx_Count_long                            0x20000106   Data           2  debug.o(.data)
    Rx_Num                                   0x20000108   Data           2  debug.o(.data)
    rxIndex                                  0x2000010a   Data           2  debug.o(.data)
    uartCountDown                            0x2000010e   Data           2  debug.o(.data)
    canNewBuf                                0x2000011a   Data           8  debug.o(.data)
    __stdout                                 0x20000124   Data           4  debug.o(.data)
    pxCurrentTCB                             0x20000128   Data           4  tasks.o(.data)
    uxTopUsedPriority                        0x20000160   Data           4  tasks.o(.data)
    idle_buf                                 0x2000025c   Data          84  main.o(.bss)
    idle_stack                               0x200002b0   Data        2048  main.o(.bss)
    task1_queue                              0x200055a4   Data         160  main.o(.bss)
    gCantRxMsg                               0x20005644   Data          36  can_drv.o(.bss)
    m_dma_channel                            0x20005668   Data          16  dma_drv.o(.bss)
    gUsartRx                                 0x20005678   Data        2054  data.o(.bss)
    gTpInfo                                  0x20005e80   Data          52  data.o(.bss)
    READ_BUFF                                0x20005eb4   Data         128  ft5216.o(.bss)
    hclcd                                    0x20005f34   Data          48  lcd.o(.bss)
    hpwm                                     0x20005f64   Data          36  pwm.o(.bss)
    hBlPwm                                   0x20005f88   Data          36  pwm.o(.bss)
    SPI5                                     0x20005fac   Data          36  winbond.o(.bss)
    dac_data_buff_1                          0x20005fd0   Data        1024  dac_wav.o(.bss)
    dac_data_buff_2                          0x200063d0   Data        1024  dac_wav.o(.bss)
    Rx_Buffer_short                          0x200067d0   Data         256  debug.o(.bss)
    Rx_Buffer_long                           0x200068d0   Data        2050  debug.o(.bss)
    gUartRev                                 0x200070d2   Data         516  debug.o(.bss)
    rxBuf                                    0x200072d6   Data         256  debug.o(.bss)
    __initial_sp                             0x2000c4b8   Data           0  startup_armcm4.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x08008349

  Load Region LR_IROM1 (Base: 0x08008000, Size: 0x00018988, Max: 0x00034000, ABSOLUTE, COMPRESSED[0x0001885c])

    Execution Region ER_IROM1 (Exec base: 0x08008000, Load base: 0x08008000, Size: 0x0001881c, Max: 0x00034000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x08008000   0x08008000   0x00000348   Data   RO         8876    RESET               startup_armcm4.o
    0x08008348   0x08008348   0x00000000   Code   RO        11469  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x08008348   0x08008348   0x00000004   Code   RO        11741    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x0800834c   0x0800834c   0x00000004   Code   RO        11744    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x08008350   0x08008350   0x00000000   Code   RO        11746    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x08008350   0x08008350   0x00000000   Code   RO        11748    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x08008350   0x08008350   0x00000008   Code   RO        11749    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x08008358   0x08008358   0x00000000   Code   RO        11751    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x08008358   0x08008358   0x00000000   Code   RO        11753    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x08008358   0x08008358   0x00000004   Code   RO        11742    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x0800835c   0x0800835c   0x000000be   Code   RO        11392    .emb_text           LT776_FreeRTOS.lib(port.o)
    0x0800841a   0x0800841a   0x00000002   PAD
    0x0800841c   0x0800841c   0x00000094   Code   RO         8877    .text               startup_armcm4.o
    0x080084b0   0x080084b0   0x00000024   Code   RO        11472    .text               mc_w.l(memcpya.o)
    0x080084d4   0x080084d4   0x00000024   Code   RO        11474    .text               mc_w.l(memseta.o)
    0x080084f8   0x080084f8   0x00000062   Code   RO        11757    .text               mc_w.l(uldiv.o)
    0x0800855a   0x0800855a   0x00000002   PAD
    0x0800855c   0x0800855c   0x00000024   Code   RO        11770    .text               mc_w.l(init.o)
    0x08008580   0x08008580   0x0000001e   Code   RO        11772    .text               mc_w.l(llshl.o)
    0x0800859e   0x0800859e   0x00000020   Code   RO        11774    .text               mc_w.l(llushr.o)
    0x080085be   0x080085be   0x00000056   Code   RO        11788    .text               mc_w.l(__dczerorl2.o)
    0x08008614   0x08008614   0x00000002   Code   RO         1827    i.AES_IRQHandler    interrupt.o
    0x08008616   0x08008616   0x00000002   Code   RO         1828    i.ASYNC_TIMER_IRQHandler  interrupt.o
    0x08008618   0x08008618   0x0000001c   Code   RO         1831    i.BusFault_Handler  interrupt.o
    0x08008634   0x08008634   0x00000002   Code   RO         1832    i.CAN0_3_IRQHandler  interrupt.o
    0x08008636   0x08008636   0x00000002   Code   RO         1833    i.CAN12_15_IRQHandler  interrupt.o
    0x08008638   0x08008638   0x00000002   Code   RO         1834    i.CAN16_31_IRQHandler  interrupt.o
    0x0800863a   0x0800863a   0x00000002   Code   RO         1835    i.CAN32_63_IRQHandler  interrupt.o
    0x0800863c   0x0800863c   0x00000004   Code   RO         1836    i.CAN4_7_IRQHandler  interrupt.o
    0x08008640   0x08008640   0x00000002   Code   RO         1837    i.CAN8_11_IRQHandler  interrupt.o
    0x08008642   0x08008642   0x00000002   PAD
    0x08008644   0x08008644   0x00000020   Code   RO         9279    i.CLCD_IRQHandler   lcd.o
    0x08008664   0x08008664   0x0000009c   Code   RO        10253    i.CTI2C_read_byte   i2c.o
    0x08008700   0x08008700   0x00000048   Code   RO        10254    i.CTI2C_start       i2c.o
    0x08008748   0x08008748   0x00000048   Code   RO        10255    i.CTI2C_stop        i2c.o
    0x08008790   0x08008790   0x00000090   Code   RO        10256    i.CTI2C_write_byte  i2c.o
    0x08008820   0x08008820   0x00000018   Code   RO         9021    i.CTP_Init          ft5216.o
    0x08008838   0x08008838   0x000000dc   Code   RO         9022    i.CTP_io_Init       ft5216.o
    0x08008914   0x08008914   0x00000012   Code   RO        10257    i.CT_DELAY_US       i2c.o
    0x08008926   0x08008926   0x00000066   Code   RO        10258    i.CT_Read_Nbyte     i2c.o
    0x0800898c   0x0800898c   0x00000044   Code   RO        10259    i.CT_Write_Nbyte    i2c.o
    0x080089d0   0x080089d0   0x0000000c   Code   RO          376    i.Canvas_image_width  bsp.o
    0x080089dc   0x080089dc   0x00000014   Code   RO         8881    i.ClearScreen       lt776_grac.o
    0x080089f0   0x080089f0   0x00000014   Code   RO         9356    i.ConfigBacklight   pwm.o
    0x08008a04   0x08008a04   0x00000014   Code   RO         9357    i.ConfigBeep        pwm.o
    0x08008a18   0x08008a18   0x00000002   Code   RO         1839    i.DAC_IRQHandler    interrupt.o
    0x08008a1a   0x08008a1a   0x00000002   Code   RO         1840    i.DMA1_IRQHandler   interrupt.o
    0x08008a1c   0x08008a1c   0x00000002   Code   RO         1841    i.DMA2D_IRQHandler  interrupt.o
    0x08008a1e   0x08008a1e   0x00000002   PAD
    0x08008a20   0x08008a20   0x00000090   Code   RO         9961    i.DMA2_IRQHandler   dac_wav.o
    0x08008ab0   0x08008ab0   0x00000058   Code   RO         9962    i.DMA_DAC_Tran      dac_wav.o
    0x08008b08   0x08008b08   0x0000000c   Code   RO         9964    i.DMA_Tran          dac_wav.o
    0x08008b14   0x08008b14   0x000001d4   Code   RO        10031    i.DRV_CAN4_7_Handler  debug.o
    0x08008ce8   0x08008ce8   0x0000001c   Code   RO        10392    i.DRV_CLCD_Cmd      libCLCD.lib(clcd_drv.o)
    0x08008d04   0x08008d04   0x00000030   Code   RO        10399    i.DRV_CLCD_SetClkDiv  libCLCD.lib(clcd_drv.o)
    0x08008d34   0x08008d34   0x00000014   Code   RO        10400    i.DRV_CLCD_SetControlRegister  libCLCD.lib(clcd_drv.o)
    0x08008d48   0x08008d48   0x00000026   Code   RO        10401    i.DRV_CLCD_SetTiming0  libCLCD.lib(clcd_drv.o)
    0x08008d6e   0x08008d6e   0x00000022   Code   RO        10402    i.DRV_CLCD_SetTiming1  libCLCD.lib(clcd_drv.o)
    0x08008d90   0x08008d90   0x00000024   Code   RO        10403    i.DRV_CLCD_SetTiming2  libCLCD.lib(clcd_drv.o)
    0x08008db4   0x08008db4   0x00000014   Code   RO        10404    i.DRV_CLCD_SetTiming3  libCLCD.lib(clcd_drv.o)
    0x08008dc8   0x08008dc8   0x00000050   Code   RO          905    i.DRV_CPM_GetCOREClHz  cpm_drv.o
    0x08008e18   0x08008e18   0x00000024   Code   RO          907    i.DRV_CPM_GetIPSClHz  cpm_drv.o
    0x08008e3c   0x08008e3c   0x0000001c   Code   RO          908    i.DRV_CPM_GetSDRAMClHz  cpm_drv.o
    0x08008e58   0x08008e58   0x00000018   Code   RO          909    i.DRV_CPM_GetSYSClHz  cpm_drv.o
    0x08008e70   0x08008e70   0x00000022   Code   RO          913    i.DRV_CPM_SetAdcClkDiv  cpm_drv.o
    0x08008e92   0x08008e92   0x00000022   Code   RO          914    i.DRV_CPM_SetAhb3ClkDiv  cpm_drv.o
    0x08008eb4   0x08008eb4   0x00000022   Code   RO          915    i.DRV_CPM_SetArithClkDiv  cpm_drv.o
    0x08008ed6   0x08008ed6   0x00000022   Code   RO          916    i.DRV_CPM_SetClcdClkDiv  cpm_drv.o
    0x08008ef8   0x08008ef8   0x00000022   Code   RO          917    i.DRV_CPM_SetClkoutClkDiv  cpm_drv.o
    0x08008f1a   0x08008f1a   0x00000016   Code   RO          918    i.DRV_CPM_SetCoreClkDiv  cpm_drv.o
    0x08008f30   0x08008f30   0x00000022   Code   RO          919    i.DRV_CPM_SetDcmi_pixClkDiv  cpm_drv.o
    0x08008f52   0x08008f52   0x00000022   Code   RO          920    i.DRV_CPM_SetDcmi_sensorClkDiv  cpm_drv.o
    0x08008f74   0x08008f74   0x00000020   Code   RO          921    i.DRV_CPM_SetDma2d_sramClkDiv  cpm_drv.o
    0x08008f94   0x08008f94   0x00000020   Code   RO          922    i.DRV_CPM_SetIpsClkDiv  cpm_drv.o
    0x08008fb4   0x08008fb4   0x0000001a   Code   RO          923    i.DRV_CPM_SetMccAdrClkDiv  cpm_drv.o
    0x08008fce   0x08008fce   0x00000020   Code   RO          924    i.DRV_CPM_SetMccClkDiv  cpm_drv.o
    0x08008fee   0x08008fee   0x00000022   Code   RO          925    i.DRV_CPM_SetMeshClkDiv  cpm_drv.o
    0x08009010   0x08009010   0x00000022   Code   RO          926    i.DRV_CPM_SetMipi_sampleClkDiv  cpm_drv.o
    0x08009032   0x08009032   0x00000022   Code   RO          928    i.DRV_CPM_SetSd_hostClkDiv  cpm_drv.o
    0x08009054   0x08009054   0x0000001e   Code   RO          929    i.DRV_CPM_SetSdram2lcdClkDiv  cpm_drv.o
    0x08009072   0x08009072   0x00000022   Code   RO          930    i.DRV_CPM_SetSdramClkDiv  cpm_drv.o
    0x08009094   0x08009094   0x00000022   Code   RO          931    i.DRV_CPM_SetSdram_smClkDiv  cpm_drv.o
    0x080090b6   0x080090b6   0x00000018   Code   RO          932    i.DRV_CPM_SetSystemClkDiv  cpm_drv.o
    0x080090ce   0x080090ce   0x0000001e   Code   RO          933    i.DRV_CPM_SetTcClkDiv  cpm_drv.o
    0x080090ec   0x080090ec   0x00000022   Code   RO          934    i.DRV_CPM_SetTraceClkDiv  cpm_drv.o
    0x0800910e   0x0800910e   0x00000024   Code   RO          935    i.DRV_CPM_SystemClkOSC400MSelect  cpm_drv.o
    0x08009132   0x08009132   0x00000024   Code   RO          936    i.DRV_CPM_SystemClkOSC480MSelect  cpm_drv.o
    0x08009156   0x08009156   0x00000022   Code   RO          937    i.DRV_CPM_SystemClkOSC8MSelect  cpm_drv.o
    0x08009178   0x08009178   0x00000022   Code   RO          938    i.DRV_CPM_SystemClkOSCEXTSelect  cpm_drv.o
    0x0800919a   0x0800919a   0x00000002   PAD
    0x0800919c   0x0800919c   0x0000015c   Code   RO          730    i.DRV_DCACHE_Init   cache_drv.o
    0x080092f8   0x080092f8   0x00000004   Code   RO         1442    i.DRV_EFM_Init      eflash_drv.o
    0x080092fc   0x080092fc   0x00000014   Code   RO         1516    i.DRV_EPORT_SetIT   eport_drv.o
    0x08009310   0x08009310   0x00000096   Code   RO         1519    i.DRV_EPORT_SetTriggerMode  eport_drv.o
    0x080093a6   0x080093a6   0x00000076   Code   RO         1598    i.DRV_I2C_GpioInit  i2c_drv.o
    0x0800941c   0x0800941c   0x0000000e   Code   RO         1610    i.DRV_I2C_ReadPin   i2c_drv.o
    0x0800942a   0x0800942a   0x00000002   PAD
    0x0800942c   0x0800942c   0x0000015c   Code   RO          732    i.DRV_ICACHE_Init   cache_drv.o
    0x08009588   0x08009588   0x00000010   Code   RO         3134    i.DRV_IOCTRL_SwapDis  ioctrl_drv.o
    0x08009598   0x08009598   0x00000010   Code   RO         3135    i.DRV_IOCTRL_SwapEn  ioctrl_drv.o
    0x080095a8   0x080095a8   0x00000010   Code   RO         3138    i.DRV_IOCTRL_SwapintDisable  ioctrl_drv.o
    0x080095b8   0x080095b8   0x00000010   Code   RO         3139    i.DRV_IOCTRL_SwapintEn  ioctrl_drv.o
    0x080095c8   0x080095c8   0x000000ae   Code   RO         3818    i.DRV_PWM_CHxAutoLoadMode  pwm_drv.o
    0x08009676   0x08009676   0x000000ac   Code   RO         3820    i.DRV_PWM_CHxCmd    pwm_drv.o
    0x08009722   0x08009722   0x0000006e   Code   RO         3821    i.DRV_PWM_CHxDeadZoneCmd  pwm_drv.o
    0x08009790   0x08009790   0x000000b2   Code   RO         3823    i.DRV_PWM_CHxInverteCmd  pwm_drv.o
    0x08009842   0x08009842   0x000000ac   Code   RO         3824    i.DRV_PWM_CHxPullupCmd  pwm_drv.o
    0x080098ee   0x080098ee   0x000000ac   Code   RO         3826    i.DRV_PWM_CHxTimerInterruptCmd  pwm_drv.o
    0x0800999a   0x0800999a   0x000000ae   Code   RO         3827    i.DRV_PWM_CHxTimerInverteCmd  pwm_drv.o
    0x08009a48   0x08009a48   0x00000060   Code   RO         3828    i.DRV_PWM_ConfigCHxClkDiv  pwm_drv.o
    0x08009aa8   0x08009aa8   0x00000042   Code   RO         3829    i.DRV_PWM_ConfigCHxDeadZone  pwm_drv.o
    0x08009aea   0x08009aea   0x00000066   Code   RO         3830    i.DRV_PWM_ConfigCHxEdgeinterrupt  pwm_drv.o
    0x08009b50   0x08009b50   0x00000062   Code   RO         3831    i.DRV_PWM_ConfigCHxPeriod  pwm_drv.o
    0x08009bb2   0x08009bb2   0x00000042   Code   RO         3832    i.DRV_PWM_ConfigCHxPerscaler  pwm_drv.o
    0x08009bf4   0x08009bf4   0x00000062   Code   RO         3833    i.DRV_PWM_ConfigCHxWidth  pwm_drv.o
    0x08009c56   0x08009c56   0x000000aa   Code   RO         3839    i.DRV_PWM_SetCHxDirection  pwm_drv.o
    0x08009d00   0x08009d00   0x000000aa   Code   RO         3840    i.DRV_PWM_SetCHxLevel  pwm_drv.o
    0x08009daa   0x08009daa   0x00000002   PAD
    0x08009dac   0x08009dac   0x00000028   Code   RO         4010    i.DRV_RTC_GetTimeCounter  rtc_drv.o
    0x08009dd4   0x08009dd4   0x0000001c   Code   RO         4013    i.DRV_RTC_SetTimeCounter  rtc_drv.o
    0x08009df0   0x08009df0   0x000000a4   Code   RO         4299    i.DRV_SDRAM_Init    sdram_drv.o
    0x08009e94   0x08009e94   0x00000022   Code   RO         4518    i.DRV_SSI_CS_DisInit  ssi_drv.o
    0x08009eb6   0x08009eb6   0x00000002   PAD
    0x08009eb8   0x08009eb8   0x00000038   Code   RO         4520    i.DRV_SSI_CS_Init   ssi_drv.o
    0x08009ef0   0x08009ef0   0x00000014   Code   RO         4522    i.DRV_SSI_Cmd       ssi_drv.o
    0x08009f04   0x08009f04   0x00000018   Code   RO         4551    i.DRV_SSI_GetFlag   ssi_drv.o
    0x08009f1c   0x08009f1c   0x000000d0   Code   RO         4552    i.DRV_SSI_Init      ssi_drv.o
    0x08009fec   0x08009fec   0x00000044   Code   RO         4565    i.DRV_SSI_WaitonFlagTimeout  ssi_drv.o
    0x0800a030   0x0800a030   0x00000050   Code   RO        10173    i.DelayMS           delay.o
    0x0800a080   0x0800a080   0x0000000e   Code   RO         8903    i.DigitToHexAscii   misc_c.o
    0x0800a08e   0x0800a08e   0x00000002   Code   RO         1843    i.EFM_IRQHandler    interrupt.o
    0x0800a090   0x0800a090   0x00000002   Code   RO         1844    i.ENCR1_IRQHandler  interrupt.o
    0x0800a092   0x0800a092   0x00000002   Code   RO         1845    i.ENCR_IRQHandler   interrupt.o
    0x0800a094   0x0800a094   0x00000002   Code   RO         1846    i.EPORT0_0_IRQHandler  interrupt.o
    0x0800a096   0x0800a096   0x00000002   Code   RO         1847    i.EPORT0_1_IRQHandler  interrupt.o
    0x0800a098   0x0800a098   0x00000002   Code   RO         1848    i.EPORT0_2_IRQHandler  interrupt.o
    0x0800a09a   0x0800a09a   0x00000002   Code   RO         1849    i.EPORT0_3_IRQHandler  interrupt.o
    0x0800a09c   0x0800a09c   0x00000002   Code   RO         1850    i.EPORT0_4_IRQHandler  interrupt.o
    0x0800a09e   0x0800a09e   0x00000002   PAD
    0x0800a0a0   0x0800a0a0   0x0000001c   Code   RO         9024    i.EPORT0_5_IRQHandler  ft5216.o
    0x0800a0bc   0x0800a0bc   0x00000002   Code   RO         1851    i.EPORT0_6_IRQHandler  interrupt.o
    0x0800a0be   0x0800a0be   0x00000002   Code   RO         1852    i.EPORT0_7_IRQHandler  interrupt.o
    0x0800a0c0   0x0800a0c0   0x00000002   Code   RO         1853    i.EPORT10_0_IRQHandler  interrupt.o
    0x0800a0c2   0x0800a0c2   0x00000002   Code   RO         1854    i.EPORT10_1_IRQHandler  interrupt.o
    0x0800a0c4   0x0800a0c4   0x00000002   Code   RO         1855    i.EPORT10_2_IRQHandler  interrupt.o
    0x0800a0c6   0x0800a0c6   0x00000002   Code   RO         1856    i.EPORT10_3_IRQHandler  interrupt.o
    0x0800a0c8   0x0800a0c8   0x00000002   Code   RO         1857    i.EPORT10_4_IRQHandler  interrupt.o
    0x0800a0ca   0x0800a0ca   0x00000002   Code   RO         1858    i.EPORT10_5_IRQHandler  interrupt.o
    0x0800a0cc   0x0800a0cc   0x00000002   Code   RO         1859    i.EPORT10_6_IRQHandler  interrupt.o
    0x0800a0ce   0x0800a0ce   0x00000002   Code   RO         1860    i.EPORT10_7_IRQHandler  interrupt.o
    0x0800a0d0   0x0800a0d0   0x00000002   Code   RO         1861    i.EPORT11_0_IRQHandler  interrupt.o
    0x0800a0d2   0x0800a0d2   0x00000002   Code   RO         1862    i.EPORT11_1_IRQHandler  interrupt.o
    0x0800a0d4   0x0800a0d4   0x00000002   Code   RO         1863    i.EPORT11_2_IRQHandler  interrupt.o
    0x0800a0d6   0x0800a0d6   0x00000002   Code   RO         1864    i.EPORT11_3_IRQHandler  interrupt.o
    0x0800a0d8   0x0800a0d8   0x00000002   Code   RO         1865    i.EPORT11_4_IRQHandler  interrupt.o
    0x0800a0da   0x0800a0da   0x00000002   Code   RO         1866    i.EPORT11_5_IRQHandler  interrupt.o
    0x0800a0dc   0x0800a0dc   0x00000002   Code   RO         1867    i.EPORT11_6_IRQHandler  interrupt.o
    0x0800a0de   0x0800a0de   0x00000002   Code   RO         1868    i.EPORT11_7_IRQHandler  interrupt.o
    0x0800a0e0   0x0800a0e0   0x00000002   Code   RO         1869    i.EPORT12_0_IRQHandler  interrupt.o
    0x0800a0e2   0x0800a0e2   0x00000002   Code   RO         1870    i.EPORT12_1_IRQHandler  interrupt.o
    0x0800a0e4   0x0800a0e4   0x00000002   Code   RO         1871    i.EPORT12_2_IRQHandler  interrupt.o
    0x0800a0e6   0x0800a0e6   0x00000002   Code   RO         1872    i.EPORT12_3_IRQHandler  interrupt.o
    0x0800a0e8   0x0800a0e8   0x00000002   Code   RO         1873    i.EPORT12_4_IRQHandler  interrupt.o
    0x0800a0ea   0x0800a0ea   0x00000002   Code   RO         1874    i.EPORT12_5_IRQHandler  interrupt.o
    0x0800a0ec   0x0800a0ec   0x00000002   Code   RO         1875    i.EPORT12_6_IRQHandler  interrupt.o
    0x0800a0ee   0x0800a0ee   0x00000002   Code   RO         1876    i.EPORT12_7_IRQHandler  interrupt.o
    0x0800a0f0   0x0800a0f0   0x00000002   Code   RO         1877    i.EPORT13_0_IRQHandler  interrupt.o
    0x0800a0f2   0x0800a0f2   0x00000002   Code   RO         1878    i.EPORT13_1_IRQHandler  interrupt.o
    0x0800a0f4   0x0800a0f4   0x00000002   Code   RO         1879    i.EPORT13_2_IRQHandler  interrupt.o
    0x0800a0f6   0x0800a0f6   0x00000002   Code   RO         1880    i.EPORT13_3_IRQHandler  interrupt.o
    0x0800a0f8   0x0800a0f8   0x00000002   Code   RO         1881    i.EPORT13_4_IRQHandler  interrupt.o
    0x0800a0fa   0x0800a0fa   0x00000002   Code   RO         1882    i.EPORT13_5_IRQHandler  interrupt.o
    0x0800a0fc   0x0800a0fc   0x00000002   Code   RO         1883    i.EPORT13_6_IRQHandler  interrupt.o
    0x0800a0fe   0x0800a0fe   0x00000002   Code   RO         1884    i.EPORT13_7_IRQHandler  interrupt.o
    0x0800a100   0x0800a100   0x00000002   Code   RO         1885    i.EPORT14_0_IRQHandler  interrupt.o
    0x0800a102   0x0800a102   0x00000002   Code   RO         1886    i.EPORT14_1_IRQHandler  interrupt.o
    0x0800a104   0x0800a104   0x00000002   Code   RO         1887    i.EPORT14_2_IRQHandler  interrupt.o
    0x0800a106   0x0800a106   0x00000002   Code   RO         1888    i.EPORT14_3_IRQHandler  interrupt.o
    0x0800a108   0x0800a108   0x00000002   Code   RO         1889    i.EPORT14_4_IRQHandler  interrupt.o
    0x0800a10a   0x0800a10a   0x00000002   Code   RO         1890    i.EPORT14_5_IRQHandler  interrupt.o
    0x0800a10c   0x0800a10c   0x00000002   Code   RO         1891    i.EPORT14_6_IRQHandler  interrupt.o
    0x0800a10e   0x0800a10e   0x00000002   Code   RO         1892    i.EPORT14_7_IRQHandler  interrupt.o
    0x0800a110   0x0800a110   0x00000002   Code   RO         1893    i.EPORT15_0_IRQHandler  interrupt.o
    0x0800a112   0x0800a112   0x00000002   Code   RO         1894    i.EPORT15_1_IRQHandler  interrupt.o
    0x0800a114   0x0800a114   0x00000002   Code   RO         1895    i.EPORT15_2_IRQHandler  interrupt.o
    0x0800a116   0x0800a116   0x00000002   Code   RO         1896    i.EPORT15_3_IRQHandler  interrupt.o
    0x0800a118   0x0800a118   0x00000002   Code   RO         1897    i.EPORT15_4_IRQHandler  interrupt.o
    0x0800a11a   0x0800a11a   0x00000002   Code   RO         1898    i.EPORT15_5_IRQHandler  interrupt.o
    0x0800a11c   0x0800a11c   0x00000002   Code   RO         1899    i.EPORT15_6_IRQHandler  interrupt.o
    0x0800a11e   0x0800a11e   0x00000002   Code   RO         1900    i.EPORT15_7_IRQHandler  interrupt.o
    0x0800a120   0x0800a120   0x00000002   Code   RO         1901    i.EPORT1_0_IRQHandler  interrupt.o
    0x0800a122   0x0800a122   0x00000002   Code   RO         1902    i.EPORT1_1_IRQHandler  interrupt.o
    0x0800a124   0x0800a124   0x00000002   Code   RO         1903    i.EPORT1_2_IRQHandler  interrupt.o
    0x0800a126   0x0800a126   0x00000002   Code   RO         1904    i.EPORT1_3_IRQHandler  interrupt.o
    0x0800a128   0x0800a128   0x00000002   Code   RO         1905    i.EPORT1_4_IRQHandler  interrupt.o
    0x0800a12a   0x0800a12a   0x00000002   Code   RO         1906    i.EPORT1_5_IRQHandler  interrupt.o
    0x0800a12c   0x0800a12c   0x00000002   Code   RO         1907    i.EPORT1_6_IRQHandler  interrupt.o
    0x0800a12e   0x0800a12e   0x00000002   Code   RO         1908    i.EPORT1_7_IRQHandler  interrupt.o
    0x0800a130   0x0800a130   0x00000002   Code   RO         1909    i.EPORT2_0_IRQHandler  interrupt.o
    0x0800a132   0x0800a132   0x00000002   Code   RO         1910    i.EPORT2_1_IRQHandler  interrupt.o
    0x0800a134   0x0800a134   0x00000002   Code   RO         1911    i.EPORT2_2_IRQHandler  interrupt.o
    0x0800a136   0x0800a136   0x00000002   Code   RO         1912    i.EPORT2_3_IRQHandler  interrupt.o
    0x0800a138   0x0800a138   0x00000002   Code   RO         1913    i.EPORT2_4_IRQHandler  interrupt.o
    0x0800a13a   0x0800a13a   0x00000002   Code   RO         1914    i.EPORT2_5_IRQHandler  interrupt.o
    0x0800a13c   0x0800a13c   0x00000002   Code   RO         1915    i.EPORT2_6_IRQHandler  interrupt.o
    0x0800a13e   0x0800a13e   0x00000002   Code   RO         1916    i.EPORT2_7_IRQHandler  interrupt.o
    0x0800a140   0x0800a140   0x00000002   Code   RO         1917    i.EPORT3_0_IRQHandler  interrupt.o
    0x0800a142   0x0800a142   0x00000002   Code   RO         1918    i.EPORT3_1_IRQHandler  interrupt.o
    0x0800a144   0x0800a144   0x00000002   Code   RO         1919    i.EPORT3_2_IRQHandler  interrupt.o
    0x0800a146   0x0800a146   0x00000002   Code   RO         1920    i.EPORT3_3_IRQHandler  interrupt.o
    0x0800a148   0x0800a148   0x00000002   Code   RO         1921    i.EPORT3_4_IRQHandler  interrupt.o
    0x0800a14a   0x0800a14a   0x00000002   Code   RO         1922    i.EPORT3_5_IRQHandler  interrupt.o
    0x0800a14c   0x0800a14c   0x00000002   Code   RO         1923    i.EPORT3_6_IRQHandler  interrupt.o
    0x0800a14e   0x0800a14e   0x00000002   Code   RO         1924    i.EPORT3_7_IRQHandler  interrupt.o
    0x0800a150   0x0800a150   0x00000002   Code   RO         1925    i.EPORT4_0_IRQHandler  interrupt.o
    0x0800a152   0x0800a152   0x00000002   Code   RO         1926    i.EPORT4_1_IRQHandler  interrupt.o
    0x0800a154   0x0800a154   0x00000002   Code   RO         1927    i.EPORT4_2_IRQHandler  interrupt.o
    0x0800a156   0x0800a156   0x00000002   Code   RO         1928    i.EPORT4_3_IRQHandler  interrupt.o
    0x0800a158   0x0800a158   0x00000002   Code   RO         1929    i.EPORT4_4_IRQHandler  interrupt.o
    0x0800a15a   0x0800a15a   0x00000002   Code   RO         1930    i.EPORT4_5_IRQHandler  interrupt.o
    0x0800a15c   0x0800a15c   0x00000002   Code   RO         1931    i.EPORT4_6_IRQHandler  interrupt.o
    0x0800a15e   0x0800a15e   0x00000002   Code   RO         1932    i.EPORT4_7_IRQHandler  interrupt.o
    0x0800a160   0x0800a160   0x00000002   Code   RO         1933    i.EPORT5_0_IRQHandler  interrupt.o
    0x0800a162   0x0800a162   0x00000002   Code   RO         1934    i.EPORT5_1_IRQHandler  interrupt.o
    0x0800a164   0x0800a164   0x00000002   Code   RO         1935    i.EPORT5_2_IRQHandler  interrupt.o
    0x0800a166   0x0800a166   0x00000002   Code   RO         1936    i.EPORT5_3_IRQHandler  interrupt.o
    0x0800a168   0x0800a168   0x00000002   Code   RO         1937    i.EPORT5_4_IRQHandler  interrupt.o
    0x0800a16a   0x0800a16a   0x00000002   Code   RO         1938    i.EPORT5_5_IRQHandler  interrupt.o
    0x0800a16c   0x0800a16c   0x00000002   Code   RO         1939    i.EPORT5_6_IRQHandler  interrupt.o
    0x0800a16e   0x0800a16e   0x00000002   Code   RO         1940    i.EPORT5_7_IRQHandler  interrupt.o
    0x0800a170   0x0800a170   0x00000002   Code   RO         1941    i.EPORT6_0_IRQHandler  interrupt.o
    0x0800a172   0x0800a172   0x00000002   Code   RO         1942    i.EPORT6_1_IRQHandler  interrupt.o
    0x0800a174   0x0800a174   0x00000002   Code   RO         1943    i.EPORT6_2_IRQHandler  interrupt.o
    0x0800a176   0x0800a176   0x00000002   Code   RO         1944    i.EPORT6_3_IRQHandler  interrupt.o
    0x0800a178   0x0800a178   0x00000002   Code   RO         1945    i.EPORT6_4_IRQHandler  interrupt.o
    0x0800a17a   0x0800a17a   0x00000002   Code   RO         1946    i.EPORT6_5_IRQHandler  interrupt.o
    0x0800a17c   0x0800a17c   0x00000002   Code   RO         1947    i.EPORT6_6_IRQHandler  interrupt.o
    0x0800a17e   0x0800a17e   0x00000002   Code   RO         1948    i.EPORT6_7_IRQHandler  interrupt.o
    0x0800a180   0x0800a180   0x00000002   Code   RO         1949    i.EPORT7_0_IRQHandler  interrupt.o
    0x0800a182   0x0800a182   0x00000002   Code   RO         1950    i.EPORT7_1_IRQHandler  interrupt.o
    0x0800a184   0x0800a184   0x00000002   Code   RO         1951    i.EPORT7_2_IRQHandler  interrupt.o
    0x0800a186   0x0800a186   0x00000002   Code   RO         1952    i.EPORT7_3_IRQHandler  interrupt.o
    0x0800a188   0x0800a188   0x00000002   Code   RO         1953    i.EPORT7_4_IRQHandler  interrupt.o
    0x0800a18a   0x0800a18a   0x00000002   Code   RO         1954    i.EPORT7_5_IRQHandler  interrupt.o
    0x0800a18c   0x0800a18c   0x00000002   Code   RO         1955    i.EPORT7_6_IRQHandler  interrupt.o
    0x0800a18e   0x0800a18e   0x00000002   Code   RO         1956    i.EPORT7_7_IRQHandler  interrupt.o
    0x0800a190   0x0800a190   0x00000002   Code   RO         1957    i.EPORT8_0_IRQHandler  interrupt.o
    0x0800a192   0x0800a192   0x00000002   Code   RO         1958    i.EPORT8_1_IRQHandler  interrupt.o
    0x0800a194   0x0800a194   0x00000002   Code   RO         1959    i.EPORT8_2_IRQHandler  interrupt.o
    0x0800a196   0x0800a196   0x00000002   Code   RO         1960    i.EPORT8_3_IRQHandler  interrupt.o
    0x0800a198   0x0800a198   0x00000002   Code   RO         1961    i.EPORT8_4_IRQHandler  interrupt.o
    0x0800a19a   0x0800a19a   0x00000002   Code   RO         1962    i.EPORT8_5_IRQHandler  interrupt.o
    0x0800a19c   0x0800a19c   0x00000002   Code   RO         1963    i.EPORT8_6_IRQHandler  interrupt.o
    0x0800a19e   0x0800a19e   0x00000002   Code   RO         1964    i.EPORT8_7_IRQHandler  interrupt.o
    0x0800a1a0   0x0800a1a0   0x00000002   Code   RO         1965    i.EPORT9_0_IRQHandler  interrupt.o
    0x0800a1a2   0x0800a1a2   0x00000002   Code   RO         1966    i.EPORT9_1_IRQHandler  interrupt.o
    0x0800a1a4   0x0800a1a4   0x00000002   Code   RO         1967    i.EPORT9_2_IRQHandler  interrupt.o
    0x0800a1a6   0x0800a1a6   0x00000002   Code   RO         1968    i.EPORT9_3_IRQHandler  interrupt.o
    0x0800a1a8   0x0800a1a8   0x00000002   Code   RO         1969    i.EPORT9_4_IRQHandler  interrupt.o
    0x0800a1aa   0x0800a1aa   0x00000002   Code   RO         1970    i.EPORT9_5_IRQHandler  interrupt.o
    0x0800a1ac   0x0800a1ac   0x00000002   Code   RO         1971    i.EPORT9_6_IRQHandler  interrupt.o
    0x0800a1ae   0x0800a1ae   0x00000002   Code   RO         1972    i.EPORT9_7_IRQHandler  interrupt.o
    0x0800a1b0   0x0800a1b0   0x00000020   Code   RO         9025    i.FT5216_Scan       ft5216.o
    0x0800a1d0   0x0800a1d0   0x00000030   Code   RO         5332    i.HAL_CACHE_Close   cache_hal.o
    0x0800a200   0x0800a200   0x00000028   Code   RO         5333    i.HAL_CACHE_Init    cache_hal.o
    0x0800a228   0x0800a228   0x00000080   Code   RO         5470    i.HAL_CLCD_Init     clcd_hal.o
    0x0800a2a8   0x0800a2a8   0x00000044   Code   RO         5528    i.HAL_CPM_GETCLCK   cpm_hal.o
    0x0800a2ec   0x0800a2ec   0x000000ec   Code   RO         5530    i.HAL_CPM_IRQHandler  cpm_hal.o
    0x0800a3d8   0x0800a3d8   0x000000e8   Code   RO         5533    i.HAL_CPM_SSI_SYSCLKConfig  cpm_hal.o
    0x0800a4c0   0x0800a4c0   0x000000c4   Code   RO         5534    i.HAL_CPM_SYSCLKConfig  cpm_hal.o
    0x0800a584   0x0800a584   0x0000009e   Code   RO         5535    i.HAL_CPM_SetCLKDiv  cpm_hal.o
    0x0800a622   0x0800a622   0x00000002   PAD
    0x0800a624   0x0800a624   0x000000a4   Code   RO        10748    i.HAL_CPM_SwitchOSC500MHz  libSwithOSC500MHz.lib(libswithosc500mhz.o)
    0x0800a6c8   0x0800a6c8   0x0000000c   Code   RO         5902    i.HAL_EFLASH_Init   eflash_hal.o
    0x0800a6d4   0x0800a6d4   0x00000004   Code   RO         6923    i.HAL_I2C_GPIOInit  i2c_hal.o
    0x0800a6d8   0x0800a6d8   0x00000006   Code   RO         6924    i.HAL_I2C_GPIOReadPin  i2c_hal.o
    0x0800a6de   0x0800a6de   0x0000000c   Code   RO         7112    i.HAL_IOCTRL_Swap   ioctrl_hal.o
    0x0800a6ea   0x0800a6ea   0x0000000c   Code   RO         7113    i.HAL_IOCTRL_Swapint  ioctrl_hal.o
    0x0800a6f6   0x0800a6f6   0x00000002   PAD
    0x0800a6f8   0x0800a6f8   0x00000050   Code   RO         6803    i.HAL_Init          hal.o
    0x0800a748   0x0800a748   0x0000001c   Code   RO         7235    i.HAL_PIT32_IRQHandler  pit32_hal.o
    0x0800a764   0x0800a764   0x0000000a   Code   RO         7379    i.HAL_PWM_CHxCmd    pwm_hal.o
    0x0800a76e   0x0800a76e   0x00000002   Code   RO         7386    i.HAL_PWM_CaptureCallback  pwm_hal.o
    0x0800a770   0x0800a770   0x0000001c   Code   RO         7396    i.HAL_PWM_ConfigCallbackRegistry  pwm_hal.o
    0x0800a78c   0x0800a78c   0x00000002   Code   RO         7397    i.HAL_PWM_FallingCallback  pwm_hal.o
    0x0800a78e   0x0800a78e   0x00000002   PAD
    0x0800a790   0x0800a790   0x0000006c   Code   RO         7406    i.HAL_PWM_Init      pwm_hal.o
    0x0800a7fc   0x0800a7fc   0x000000f8   Code   RO         7407    i.HAL_PWM_InputInit  pwm_hal.o
    0x0800a8f4   0x0800a8f4   0x00000130   Code   RO         7408    i.HAL_PWM_OutputInit  pwm_hal.o
    0x0800aa24   0x0800aa24   0x00000002   Code   RO         7409    i.HAL_PWM_RisingCallback  pwm_hal.o
    0x0800aa26   0x0800aa26   0x00000056   Code   RO         7865    i.HAL_SDRAM_Init    sdram_hal.o
    0x0800aa7c   0x0800aa7c   0x00000006   Code   RO         5471    i.HLA_CLCD_Cmd      clcd_hal.o
    0x0800aa82   0x0800aa82   0x00000006   Code   RO         5472    i.HLA_CLCD_UpuerPannelBaseAddr  clcd_hal.o
    0x0800aa88   0x0800aa88   0x00000020   Code   RO         1973    i.HardFault_Handler  interrupt.o
    0x0800aaa8   0x0800aaa8   0x00000002   Code   RO         1974    i.I2C1_IRQHandler   interrupt.o
    0x0800aaaa   0x0800aaaa   0x00000002   Code   RO         1975    i.I2C2_IRQHandler   interrupt.o
    0x0800aaac   0x0800aaac   0x00000002   Code   RO         1976    i.I2C3_IRQHandler   interrupt.o
    0x0800aaae   0x0800aaae   0x00000004   Code   RO         8775    i.INTX_ENABLE       sys.o
    0x0800aab2   0x0800aab2   0x00000002   PAD
    0x0800aab4   0x0800aab4   0x00000044   Code   RO         9358    i.InitBacklight     pwm.o
    0x0800aaf8   0x0800aaf8   0x00000044   Code   RO         9359    i.InitBeep          pwm.o
    0x0800ab3c   0x0800ab3c   0x000000f8   Code   RO         9280    i.InitLcd           lcd.o
    0x0800ac34   0x0800ac34   0x00000026   Code   RO         9809    i.Is_Leap_Year      rtc.o
    0x0800ac5a   0x0800ac5a   0x00000002   PAD
    0x0800ac5c   0x0800ac5c   0x0000005c   Code   RO        10615    i.LIB_EFLASH_Init   libeflash.lib(lib_eflash.o)
    0x0800acb8   0x0800acb8   0x00000050   Code   RO        10619    i.LIB_EFLASH_SetMainPermission  libeflash.lib(lib_eflash.o)
    0x0800ad08   0x0800ad08   0x0000001c   Code   RO        10620    i.LIB_EFLASH_SetRWSC  libeflash.lib(lib_eflash.o)
    0x0800ad24   0x0800ad24   0x00000024   Code   RO        10623    i.LIB_EFLASH_SetVerifyCnt  libeflash.lib(lib_eflash.o)
    0x0800ad48   0x0800ad48   0x00000018   Code   RO          380    i.LT768_DrawPoint   bsp.o
    0x0800ad60   0x0800ad60   0x00000064   Code   RO          381    i.LT768_TFT_ShowAscii  bsp.o
    0x0800adc4   0x0800adc4   0x0000017c   Code   RO          382    i.LT768_TFT_Show_Internal_Char  bsp.o
    0x0800af40   0x0800af40   0x0000004c   Code   RO          384    i.LT_ReadParam      bsp.o
    0x0800af8c   0x0800af8c   0x000000a8   Code   RO         9810    i.LT_RtcInit        rtc.o
    0x0800b034   0x0800b034   0x00000018   Code   RO        10334    i.LT_UsartTimeDisable  pit.o
    0x0800b04c   0x0800b04c   0x00000018   Code   RO        10335    i.LT_UsartTimeEnable  pit.o
    0x0800b064   0x0800b064   0x00000014   Code   RO        10336    i.LT_UsartTimeSetCounter  pit.o
    0x0800b078   0x0800b078   0x00000002   Code   RO         1978    i.MCC_IRQHandler    interrupt.o
    0x0800b07a   0x0800b07a   0x00000002   Code   RO         1979    i.MIPI_IRQHandler   interrupt.o
    0x0800b07c   0x0800b07c   0x00000020   Code   RO         1980    i.MemManage_Handler  interrupt.o
    0x0800b09c   0x0800b09c   0x0000004a   Code   RO         8776    i.NVIC_Init         sys.o
    0x0800b0e6   0x0800b0e6   0x00000002   PAD
    0x0800b0e8   0x0800b0e8   0x00000024   Code   RO         8777    i.NVIC_PriorityGroupConfig  sys.o
    0x0800b10c   0x0800b10c   0x00000002   Code   RO         1983    i.PCI_DET_IRQHandler  interrupt.o
    0x0800b10e   0x0800b10e   0x00000004   Code   RO         1984    i.PCI_IRQHandler    interrupt.o
    0x0800b112   0x0800b112   0x00000002   Code   RO        10337    i.PIT1_IRQHandler   pit.o
    0x0800b114   0x0800b114   0x00000004   Code   RO         1985    i.PIT3_IRQHandler   interrupt.o
    0x0800b118   0x0800b118   0x00000004   Code   RO         1986    i.PIT4_IRQHandler   interrupt.o
    0x0800b11c   0x0800b11c   0x00000002   Code   RO         1987    i.PMU_IRQHandler    interrupt.o
    0x0800b11e   0x0800b11e   0x00000002   PAD
    0x0800b120   0x0800b120   0x00000020   Code   RO         9811    i.PMU_RTC_IRQHandler  rtc.o
    0x0800b140   0x0800b140   0x00000002   Code   RO         1988    i.PWM0_IRQHandler   interrupt.o
    0x0800b142   0x0800b142   0x00000002   Code   RO         1989    i.PWM1_IRQHandler   interrupt.o
    0x0800b144   0x0800b144   0x00000002   Code   RO         1990    i.PWM2_IRQHandler   interrupt.o
    0x0800b146   0x0800b146   0x00000002   Code   RO         1991    i.PWM3_IRQHandler   interrupt.o
    0x0800b148   0x0800b148   0x00000002   Code   RO         1992    i.PWM4_IRQHandler   interrupt.o
    0x0800b14a   0x0800b14a   0x00000002   Code   RO         1993    i.PWM5_IRQHandler   interrupt.o
    0x0800b14c   0x0800b14c   0x00000002   Code   RO         1994    i.PWM6_IRQHandler   interrupt.o
    0x0800b14e   0x0800b14e   0x00000002   Code   RO         1995    i.PWM7_IRQHandler   interrupt.o
    0x0800b150   0x0800b150   0x00000078   Code   RO            5    i.PeripheralInit    main.o
    0x0800b1c8   0x0800b1c8   0x0000015c   Code   RO            6    i.Printf_Version    main.o
    0x0800b324   0x0800b324   0x0000005c   Code   RO         8882    i.Put16BitBMP       lt776_grac.o
    0x0800b380   0x0800b380   0x00000002   Code   RO         1996    i.QADC_IRQHandler   interrupt.o
    0x0800b382   0x0800b382   0x00000002   Code   RO         1997    i.RSA_IRQHandler    interrupt.o
    0x0800b384   0x0800b384   0x000000ac   Code   RO         9812    i.RTC_Get           rtc.o
    0x0800b430   0x0800b430   0x00000050   Code   RO         9813    i.RTC_Get_Week      rtc.o
    0x0800b480   0x0800b480   0x00000090   Code   RO         9814    i.RTC_Set           rtc.o
    0x0800b510   0x0800b510   0x00000024   Code   RO        10260    i.SCL_OUTPUT        i2c.o
    0x0800b534   0x0800b534   0x00000024   Code   RO        10261    i.SDA_INPUT         i2c.o
    0x0800b558   0x0800b558   0x00000024   Code   RO        10262    i.SDA_OUTPUT        i2c.o
    0x0800b57c   0x0800b57c   0x00000002   Code   RO         1998    i.SEC_PGD_LD_FD_IRQHandler  interrupt.o
    0x0800b57e   0x0800b57e   0x00000002   Code   RO         1999    i.SHA_IRQHandler    interrupt.o
    0x0800b580   0x0800b580   0x00000002   Code   RO         2000    i.SMS4_IRQHandler   interrupt.o
    0x0800b582   0x0800b582   0x00000002   Code   RO         2001    i.SPI1_IRQHandler   interrupt.o
    0x0800b584   0x0800b584   0x00000002   Code   RO         2002    i.SPI2_IRQHandler   interrupt.o
    0x0800b586   0x0800b586   0x00000002   Code   RO         2003    i.SPI3_IRQHandler   interrupt.o
    0x0800b588   0x0800b588   0x0000005c   Code   RO         9491    i.SPI5_STD_Init     winbond.o
    0x0800b5e4   0x0800b5e4   0x00000002   Code   RO         2004    i.SPIM1_IRQHandler  interrupt.o
    0x0800b5e6   0x0800b5e6   0x00000002   Code   RO         2005    i.SPIM2_IRQHandler  interrupt.o
    0x0800b5e8   0x0800b5e8   0x00000002   Code   RO         2006    i.SPIM3_IRQHandler  interrupt.o
    0x0800b5ea   0x0800b5ea   0x00000060   Code   RO         8904    i.Show16BitDecimal  misc_c.o
    0x0800b64a   0x0800b64a   0x00000002   PAD
    0x0800b64c   0x0800b64c   0x000000ac   Code   RO         4577    i.SysSsiConfigure   ssi_drv.o
    0x0800b6f8   0x0800b6f8   0x00000034   Code   RO        11393    i.SysTick_Handler   LT776_FreeRTOS.lib(port.o)
    0x0800b72c   0x0800b72c   0x00000030   Code   RO         8849    i.SystemInit        system_armcm4.o
    0x0800b75c   0x0800b75c   0x00000002   Code   RO         2008    i.TC_IRQHandler     interrupt.o
    0x0800b75e   0x0800b75e   0x00000002   PAD
    0x0800b760   0x0800b760   0x000000c8   Code   RO         9028    i.TP_read_XY        ft5216.o
    0x0800b828   0x0800b828   0x00000002   Code   RO         2009    i.TRNG_IRQHandler   interrupt.o
    0x0800b82a   0x0800b82a   0x00000002   Code   RO         2010    i.TSI_IRQHandler    interrupt.o
    0x0800b82c   0x0800b82c   0x00000004   Code   RO         2011    i.UART1_IRQHandler  interrupt.o
    0x0800b830   0x0800b830   0x000000ec   Code   RO        10039    i.UART1_IRQHandlerEvent  debug.o
    0x0800b91c   0x0800b91c   0x00000002   Code   RO         2012    i.UART2_IRQHandler  interrupt.o
    0x0800b91e   0x0800b91e   0x00000002   Code   RO         2013    i.UART3_IRQHandler  interrupt.o
    0x0800b920   0x0800b920   0x00000002   Code   RO         2014    i.UART4_IRQHandler  interrupt.o
    0x0800b922   0x0800b922   0x00000002   PAD
    0x0800b924   0x0800b924   0x00000040   Code   RO        10043    i.UART_Debug_Init   debug.o
    0x0800b964   0x0800b964   0x00000002   Code   RO         2015    i.USB_IRQHandler    interrupt.o
    0x0800b966   0x0800b966   0x00000002   Code   RO         2017    i.USI3_IRQHandler   interrupt.o
    0x0800b968   0x0800b968   0x00000020   Code   RO         2019    i.UsageFault_Handler  interrupt.o
    0x0800b988   0x0800b988   0x00000020   Code   RO        11687    i.__0printf$8       mc_w.l(printf8.o)
    0x0800b9a8   0x0800b9a8   0x0000000e   Code   RO        11782    i.__scatterload_copy  mc_w.l(handlers.o)
    0x0800b9b6   0x0800b9b6   0x00000002   Code   RO        11783    i.__scatterload_null  mc_w.l(handlers.o)
    0x0800b9b8   0x0800b9b8   0x0000000e   Code   RO        11784    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x0800b9c6   0x0800b9c6   0x00000002   PAD
    0x0800b9c8   0x0800b9c8   0x00000410   Code   RO        11694    i._printf_core      mc_w.l(printf8.o)
    0x0800bdd8   0x0800bdd8   0x00000024   Code   RO        11695    i._printf_post_padding  mc_w.l(printf8.o)
    0x0800bdfc   0x0800bdfc   0x0000002e   Code   RO        11696    i._printf_pre_padding  mc_w.l(printf8.o)
    0x0800be2a   0x0800be2a   0x00000002   PAD
    0x0800be2c   0x0800be2c   0x00000018   Code   RO        10048    i.fputc             debug.o
    0x0800be44   0x0800be44   0x00000012   Code   RO            7    i.main              main.o
    0x0800be56   0x0800be56   0x00000002   PAD
    0x0800be58   0x0800be58   0x000000c0   Code   RO        11026    i.prvAddCurrentTaskToDelayedList  LT776_FreeRTOS.lib(tasks.o)
    0x0800bf18   0x0800bf18   0x000000e4   Code   RO        11027    i.prvAddNewTaskToReadyList  LT776_FreeRTOS.lib(tasks.o)
    0x0800bffc   0x0800bffc   0x00000048   Code   RO        11028    i.prvCheckTasksWaitingTermination  LT776_FreeRTOS.lib(tasks.o)
    0x0800c044   0x0800c044   0x0000002a   Code   RO        10874    i.prvCopyDataFromQueue  LT776_FreeRTOS.lib(queue.o)
    0x0800c06e   0x0800c06e   0x0000007e   Code   RO        10875    i.prvCopyDataToQueue  LT776_FreeRTOS.lib(queue.o)
    0x0800c0ec   0x0800c0ec   0x00000002   Code   RO        11029    i.prvDeleteTCB      LT776_FreeRTOS.lib(tasks.o)
    0x0800c0ee   0x0800c0ee   0x00000014   Code   RO        10876    i.prvGetDisinheritPriorityAfterTimeout  LT776_FreeRTOS.lib(queue.o)
    0x0800c102   0x0800c102   0x00000002   PAD
    0x0800c104   0x0800c104   0x00000028   Code   RO        11030    i.prvIdleTask       LT776_FreeRTOS.lib(tasks.o)
    0x0800c12c   0x0800c12c   0x0000001e   Code   RO        10877    i.prvInitialiseMutex  LT776_FreeRTOS.lib(queue.o)
    0x0800c14a   0x0800c14a   0x00000026   Code   RO        10878    i.prvInitialiseNewQueue  LT776_FreeRTOS.lib(queue.o)
    0x0800c170   0x0800c170   0x00000090   Code   RO        11031    i.prvInitialiseNewTask  LT776_FreeRTOS.lib(tasks.o)
    0x0800c200   0x0800c200   0x00000068   Code   RO        11032    i.prvInitialiseTaskLists  LT776_FreeRTOS.lib(tasks.o)
    0x0800c268   0x0800c268   0x0000001a   Code   RO        10879    i.prvIsQueueEmpty   LT776_FreeRTOS.lib(queue.o)
    0x0800c282   0x0800c282   0x0000001e   Code   RO        10880    i.prvIsQueueFull    LT776_FreeRTOS.lib(queue.o)
    0x0800c2a0   0x0800c2a0   0x00000030   Code   RO        11033    i.prvResetNextTaskUnblockTime  LT776_FreeRTOS.lib(tasks.o)
    0x0800c2d0   0x0800c2d0   0x00000016   Code   RO        11394    i.prvTaskExitError  LT776_FreeRTOS.lib(port.o)
    0x0800c2e6   0x0800c2e6   0x0000001e   Code   RO        10770    i.prvTestWaitCondition  LT776_FreeRTOS.lib(event_groups.o)
    0x0800c304   0x0800c304   0x0000007e   Code   RO        10881    i.prvUnlockQueue    LT776_FreeRTOS.lib(queue.o)
    0x0800c382   0x0800c382   0x00000002   PAD
    0x0800c384   0x0800c384   0x00000020   Code   RO        11035    i.pvTaskIncrementMutexHeldCount  LT776_FreeRTOS.lib(tasks.o)
    0x0800c3a4   0x0800c3a4   0x0000002c   Code   RO        11395    i.pxPortInitialiseStack  LT776_FreeRTOS.lib(port.o)
    0x0800c3d0   0x0800c3d0   0x00000098   Code   RO            8    i.task_0_entry      main.o
    0x0800c468   0x0800c468   0x000000b4   Code   RO            9    i.task_1_entry      main.o
    0x0800c51c   0x0800c51c   0x0000009c   Code   RO           10    i.task_2_entry      main.o
    0x0800c5b8   0x0800c5b8   0x000000f0   Code   RO           11    i.task_3_and_4_entry  main.o
    0x0800c6a8   0x0800c6a8   0x000000ac   Code   RO           12    i.task_5_entry      main.o
    0x0800c754   0x0800c754   0x000000ec   Code   RO           13    i.task_6_and_7_entry  main.o
    0x0800c840   0x0800c840   0x000000e8   Code   RO           14    i.task_touch_entry  main.o
    0x0800c928   0x0800c928   0x00000028   Code   RO        11347    i.uxListRemove      LT776_FreeRTOS.lib(list.o)
    0x0800c950   0x0800c950   0x0000001c   Code   RO        11041    i.uxTaskResetEventItemValue  LT776_FreeRTOS.lib(tasks.o)
    0x0800c96c   0x0800c96c   0x00000018   Code   RO           15    i.vApplicationGetIdleTaskMemory  main.o
    0x0800c984   0x0800c984   0x0000001a   Code   RO        11348    i.vListInitialise   LT776_FreeRTOS.lib(list.o)
    0x0800c99e   0x0800c99e   0x00000006   Code   RO        11349    i.vListInitialiseItem  LT776_FreeRTOS.lib(list.o)
    0x0800c9a4   0x0800c9a4   0x00000034   Code   RO        11350    i.vListInsert       LT776_FreeRTOS.lib(list.o)
    0x0800c9d8   0x0800c9d8   0x00000024   Code   RO        11397    i.vPortEnterCritical  LT776_FreeRTOS.lib(port.o)
    0x0800c9fc   0x0800c9fc   0x00000020   Code   RO        11398    i.vPortExitCritical  LT776_FreeRTOS.lib(port.o)
    0x0800ca1c   0x0800ca1c   0x00000018   Code   RO        11399    i.vPortSetupTimerInterrupt  LT776_FreeRTOS.lib(port.o)
    0x0800ca34   0x0800ca34   0x00000034   Code   RO        11042    i.vTaskDelay        LT776_FreeRTOS.lib(tasks.o)
    0x0800ca68   0x0800ca68   0x00000018   Code   RO        11046    i.vTaskInternalSetTimeOutState  LT776_FreeRTOS.lib(tasks.o)
    0x0800ca80   0x0800ca80   0x0000000c   Code   RO        11047    i.vTaskMissedYield  LT776_FreeRTOS.lib(tasks.o)
    0x0800ca8c   0x0800ca8c   0x00000020   Code   RO        11048    i.vTaskPlaceOnEventList  LT776_FreeRTOS.lib(tasks.o)
    0x0800caac   0x0800caac   0x00000050   Code   RO        11049    i.vTaskPlaceOnUnorderedEventList  LT776_FreeRTOS.lib(tasks.o)
    0x0800cafc   0x0800cafc   0x000000d4   Code   RO        11050    i.vTaskPriorityDisinheritAfterTimeout  LT776_FreeRTOS.lib(tasks.o)
    0x0800cbd0   0x0800cbd0   0x000000d0   Code   RO        11052    i.vTaskRemoveFromUnorderedEventList  LT776_FreeRTOS.lib(tasks.o)
    0x0800cca0   0x0800cca0   0x00000094   Code   RO        11055    i.vTaskStartScheduler  LT776_FreeRTOS.lib(tasks.o)
    0x0800cd34   0x0800cd34   0x00000010   Code   RO        11057    i.vTaskSuspendAll   LT776_FreeRTOS.lib(tasks.o)
    0x0800cd44   0x0800cd44   0x00000060   Code   RO        11058    i.vTaskSwitchContext  LT776_FreeRTOS.lib(tasks.o)
    0x0800cda4   0x0800cda4   0x00000020   Code   RO        10774    i.xEventGroupClearBits  LT776_FreeRTOS.lib(event_groups.o)
    0x0800cdc4   0x0800cdc4   0x00000016   Code   RO        10775    i.xEventGroupCreateStatic  LT776_FreeRTOS.lib(event_groups.o)
    0x0800cdda   0x0800cdda   0x00000092   Code   RO        10777    i.xEventGroupSetBits  LT776_FreeRTOS.lib(event_groups.o)
    0x0800ce6c   0x0800ce6c   0x000000cc   Code   RO        10779    i.xEventGroupWaitBits  LT776_FreeRTOS.lib(event_groups.o)
    0x0800cf38   0x0800cf38   0x00000048   Code   RO        11400    i.xPortStartScheduler  LT776_FreeRTOS.lib(port.o)
    0x0800cf80   0x0800cf80   0x0000002a   Code   RO        10886    i.xQueueCreateMutexStatic  LT776_FreeRTOS.lib(queue.o)
    0x0800cfaa   0x0800cfaa   0x00000038   Code   RO        10887    i.xQueueGenericCreateStatic  LT776_FreeRTOS.lib(queue.o)
    0x0800cfe2   0x0800cfe2   0x00000002   PAD
    0x0800cfe4   0x0800cfe4   0x000000a0   Code   RO        10888    i.xQueueGenericReset  LT776_FreeRTOS.lib(queue.o)
    0x0800d084   0x0800d084   0x00000118   Code   RO        10889    i.xQueueGenericSend  LT776_FreeRTOS.lib(queue.o)
    0x0800d19c   0x0800d19c   0x00000104   Code   RO        10896    i.xQueueReceive     LT776_FreeRTOS.lib(queue.o)
    0x0800d2a0   0x0800d2a0   0x00000130   Code   RO        10898    i.xQueueSemaphoreTake  LT776_FreeRTOS.lib(queue.o)
    0x0800d3d0   0x0800d3d0   0x00000060   Code   RO        11060    i.xTaskCheckForTimeOut  LT776_FreeRTOS.lib(tasks.o)
    0x0800d430   0x0800d430   0x00000048   Code   RO        11061    i.xTaskCreateStatic  LT776_FreeRTOS.lib(tasks.o)
    0x0800d478   0x0800d478   0x00000190   Code   RO        11070    i.xTaskIncrementTick  LT776_FreeRTOS.lib(tasks.o)
    0x0800d608   0x0800d608   0x000000ac   Code   RO        11071    i.xTaskPriorityDisinherit  LT776_FreeRTOS.lib(tasks.o)
    0x0800d6b4   0x0800d6b4   0x000000ec   Code   RO        11072    i.xTaskPriorityInherit  LT776_FreeRTOS.lib(tasks.o)
    0x0800d7a0   0x0800d7a0   0x00000108   Code   RO        11073    i.xTaskRemoveFromEventList  LT776_FreeRTOS.lib(tasks.o)
    0x0800d8a8   0x0800d8a8   0x0000015c   Code   RO        11074    i.xTaskResumeAll    LT776_FreeRTOS.lib(tasks.o)
    0x0800da04   0x0800da04   0x000001d4   Code   RO           16    i.x_application_define  main.o
    0x0800dbd8   0x0800dbd8   0x00000010   Data   RO           18    .constdata          main.o
    0x0800dbe8   0x0800dbe8   0x000000d8   Data   RO         5541    .constdata          cpm_hal.o
    0x0800dcc0   0x0800dcc0   0x00008008   Data   RO         8727    .constdata          acorn.o
    0x08015cc8   0x08015cc8   0x00008008   Data   RO         8735    .constdata          acorn1.o
    0x0801dcd0   0x0801dcd0   0x000005f0   Data   RO         8999    .constdata          font_data.o
    0x0801e2c0   0x0801e2c0   0x00000d5c   Data   RO         9000    .constdata          font_data.o
    0x0801f01c   0x0801f01c   0x000017c0   Data   RO         9001    .constdata          font_data.o
    0x080207dc   0x080207dc   0x00000018   Data   RO         9815    .constdata          rtc.o
    0x080207f4   0x080207f4   0x00000005   Data   RO           19    .conststring        main.o
    0x080207f9   0x080207f9   0x00000003   PAD
    0x080207fc   0x080207fc   0x00000020   Data   RO        11780    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x20000000, Load base: 0x0802081c, Size: 0x0000c4b8, Max: 0x00020000, ABSOLUTE, COMPRESSED[0x00000040])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20000000   COMPRESSED   0x00000038   Data   RW           20    .data               main.o
    0x20000038   COMPRESSED   0x00000001   Data   RW          391    .data               bsp.o
    0x20000039   COMPRESSED   0x00000004   Data   RW          392    .data               bsp.o
    0x2000003d   COMPRESSED   0x00000003   PAD
    0x20000040   COMPRESSED   0x00000020   Data   RW          394    .data               bsp.o
    0x20000060   COMPRESSED   0x00000046   Data   RW          792    .data               can_drv.o
    0x200000a6   COMPRESSED   0x00000008   Data   RW          793    .data               can_drv.o
    0x200000ae   COMPRESSED   0x00000002   PAD
    0x200000b0   COMPRESSED   0x00000008   Data   RW          943    .data               cpm_drv.o
    0x200000b8   COMPRESSED   0x00000004   Data   RW          944    .data               cpm_drv.o
    0x200000bc   COMPRESSED   0x00000004   Data   RW          947    .data               cpm_drv.o
    0x200000c0   COMPRESSED   0x0000000c   Data   RW         1230    .data               dma_drv.o
    0x200000cc   COMPRESSED   0x00000008   Data   RW         5474    .data               clcd_hal.o
    0x200000d4   COMPRESSED   0x00000001   Data   RW         5543    .data               cpm_hal.o
    0x200000d5   COMPRESSED   0x00000003   PAD
    0x200000d8   COMPRESSED   0x00000004   Data   RW         7242    .data               pit32_hal.o
    0x200000dc   COMPRESSED   0x00000004   Data   RW         7412    .data               pwm_hal.o
    0x200000e0   COMPRESSED   0x00000001   Data   RW         8972    .data               data.o
    0x200000e1   COMPRESSED   0x00000001   Data   RW         8974    .data               data.o
    0x200000e2   COMPRESSED   0x00000002   Data   RW         8983    .data               data.o
    0x200000e4   COMPRESSED   0x00000002   Data   RW         8984    .data               data.o
    0x200000e6   COMPRESSED   0x00000001   Data   RW         9032    .data               ft5216.o
    0x200000e7   COMPRESSED   0x00000001   Data   RW         9282    .data               lcd.o
    0x200000e8   COMPRESSED   0x0000000a   Data   RW         9816    .data               rtc.o
    0x200000f2   COMPRESSED   0x0000000e   Data   RW         9969    .data               dac_wav.o
    0x20000100   COMPRESSED   0x00000022   Data   RW        10050    .data               debug.o
    0x20000122   COMPRESSED   0x00000002   PAD
    0x20000124   COMPRESSED   0x00000004   Data   RW        10055    .data               debug.o
    0x20000128   COMPRESSED   0x00000040   Data   RW        11077    .data               LT776_FreeRTOS.lib(tasks.o)
    0x20000168   COMPRESSED   0x00000004   Data   RW        11401    .data               LT776_FreeRTOS.lib(port.o)
    0x2000016c        -       0x000054d8   Zero   RW           17    .bss                main.o
    0x20005644        -       0x00000024   Zero   RW          790    .bss                can_drv.o
    0x20005668        -       0x00000010   Zero   RW         1228    .bss                dma_drv.o
    0x20005678        -       0x00000806   Zero   RW         8954    .bss                data.o
    0x20005e7e   COMPRESSED   0x00000002   PAD
    0x20005e80        -       0x00000034   Zero   RW         8955    .bss                data.o
    0x20005eb4        -       0x00000080   Zero   RW         9029    .bss                ft5216.o
    0x20005f34        -       0x00000030   Zero   RW         9281    .bss                lcd.o
    0x20005f64        -       0x00000048   Zero   RW         9361    .bss                pwm.o
    0x20005fac        -       0x00000024   Zero   RW         9534    .bss                winbond.o
    0x20005fd0        -       0x00000800   Zero   RW         9968    .bss                dac_wav.o
    0x200067d0        -       0x00000c06   Zero   RW        10049    .bss                debug.o
    0x200073d6   COMPRESSED   0x00000002   PAD
    0x200073d8        -       0x00000018   Zero   RW        10631    .bss                libeflash.lib(lib_eflash.o)
    0x200073f0        -       0x000000c8   Zero   RW        11076    .bss                LT776_FreeRTOS.lib(tasks.o)
    0x200074b8        -       0x00005000   Zero   RW         8874    STACK               startup_armcm4.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

         0          0      32776          0          0        616   acorn.o
         0          0      32776          0          0        621   acorn1.o
       592         36          0         37          0     227960   bsp.o
       696          8          0          0          0       1968   cache_drv.o
        88          0          0          0          0       1591   cache_hal.o
         0          0          0         78         36       5210   can_drv.o
         0          0          0          0          0      44516   can_hal.o
       140          6          0          8          0       3453   clcd_hal.o
       978         32          0         16          0      16854   cpm_drv.o
       890        174        216          1          0       4910   cpm_hal.o
       244         36          0         14       2048       3041   dac_wav.o
         0          0          0          6       2106       3914   data.o
       792         76          0         38       3078       7062   debug.o
        80         10          0          0          0        602   delay.o
         0          0          0         12         16      12355   dma_drv.o
         4          0          0          0          0        531   eflash_drv.o
        12          0          0          0          0        538   eflash_hal.o
       170          6          0          0          0       1841   eport_drv.o
         0          0      11020          0          0       1075   font_data.o
       504         56          0          1        128     115667   ft5216.o
        80         10          0          0          0       4431   hal.o
       740         32          0          0          0       6766   i2c.o
       132          0          0          0          0       2310   i2c_drv.o
        10          0          0          0          0       3441   i2c_hal.o
       492        100          0          0          0      92257   interrupt.o
        64          0          0          0          0       2220   ioctrl_drv.o
        24          0          0          0          0       1187   ioctrl_hal.o
       280         64          0          1         48       2231   lcd.o
       112          0          0          0          0       2312   lt776_grac.o
      2346        628         21         56      21720      38840   main.o
       110          0          0          0          0       1988   misc_c.o
        70         12          0          0          0       2370   pit.o
         0          0          0          0          0       1984   pit32_drv.o
        28          4          0          4          0       1999   pit32_hal.o
       176         28          0          0         72       3866   pwm.o
      2018        192          0          0          0      37914   pwm_drv.o
       704         42          0          4          0       7065   pwm_hal.o
       634         48         24         10          0       5656   rtc.o
        68         10          0          0          0       6954   rtc_drv.o
       164         14          0          0          0       1625   sdram_drv.o
        86          0          0          0          0       1097   sdram_hal.o
       582         16          0          0          0       6217   ssi_drv.o
       148         26        840          0      20480        880   startup_armcm4.o
       114         10          0          0          0       2285   sys.o
        48          8          0          0          0        537   system_armcm4.o
        92          8          0          0         36        799   winbond.o

    ----------------------------------------------------------------------
     14548       1692      77708        296      49772     693556   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        36          0          3         10          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       434          6          0          0          0      32740   event_groups.o
       124          0          0          0          0       8537   list.o
       472         56          0          4          0       9100   port.o
      1540         16          0          0          0      14589   queue.o
      3358        378          0         64        200      44253   tasks.o
       224          4          0          0          0     103142   clcd_drv.o
       164         12          0          0          0       6610   libswithosc500mhz.o
       236         36          0          0         24       5703   lib_eflash.o
        86          0          0          0          0          0   __dczerorl2.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
        30          0          0          0          0         68   llshl.o
        32          0          0          0          0         68   llushr.o
        36          0          0          0          0         68   memcpya.o
        36          0          0          0          0        108   memseta.o
      1154         54          0          0          0        352   printf8.o
        98          0          0          0          0         92   uldiv.o

    ----------------------------------------------------------------------
      8124        578          0         68        224     225498   Library Totals
        14          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      5928        456          0         68        200     109219   LT776_FreeRTOS.lib
       224          4          0          0          0     103142   libCLCD.lib
       164         12          0          0          0       6610   libSwithOSC500MHz.lib
       236         36          0          0         24       5703   libeflash.lib
      1558         70          0          0          0        824   mc_w.l

    ----------------------------------------------------------------------
      8124        578          0         68        224     225498   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     22672       2270      77708        364      49996     879074   Grand Totals
     22672       2270      77708         64      49996     879074   ELF Image Totals (compressed)
     22672       2270      77708         64          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)               100380 (  98.03kB)
    Total RW  Size (RW Data + ZI Data)             50360 (  49.18kB)
    Total ROM Size (Code + RO Data + RW Data)     100444 (  98.09kB)

==============================================================================

